# 前言

本说明为中兴服务器的SNMP MIB说明，通过本说明，可以了解SNMP接口的使用方法以及SNMP TRAP信息。

    本文档主要适用于以下工程师：
        技术支持工程师
        维护工程师



# 1 SNMP特性综述

## 1.1 基本原理

简单网络管理协议SNMP（Simple  Network  Management  Protocol）用于网络设备的管理。SNMP作为广泛应用于TCP/IP网络的网络管理标准协议，提供了统一的接口，从而实现了不同种类和厂商的网络设备之间的统一管理。

SNMP协议分为三个版本：SNMPv1、SNMPv2c和SNMPv3。

●	SNMPv1是SNMP协议的最初版本，提供最小限度的网络管理功能。SNMPv1基于团体名认证，安全性较差，且返回报文的错误码也较少。

●	SNMPv2c也采用团体名认证。在SNMPv1版本的基础上引入了GetBulk和Inform操作，支持更多的标准错误码信息，支持更多的数据类型（Counter64、 Counter32）。

●	SNMPv3主要在安全性方面进行了增强，提供了基于USM（用户安全模块：User  Security Module）的认证加密和基于VACM（基于视图的访问控制模型：View-based Access Control Model）的访问控制。SNMPv3版本支持的操作和SNMPv2c版本支持的操作一样。

本软件支持SNMP V1、 V2C 、 V3 版本，本 MIB 主要实现 SNMP 的特性，针对主板、硬盘、标卡、内存、电源、风扇、功率、上下电、TRAP上报等进行管理。



## 1.2 参数说明

**NMS**

NMS是网络中的管理者，是一个采用SNMP协议对网络设备进行管理/监视的系统，运行在NMS服务器上。

●	NMS可以向设备上的SNMP  Agent发出请求，查询或修改一个或多个具体的参数值。

●	NMS可以接收设备上的SNMP  Agent主动发送的SNMP  Traps，以获知被管理设备当前的状态。



**SNMP Agent**

SNMP Agent是被管理设备中的一个代理进程，用于维护被管理设备的信息数据并响应来自NMS的请求，把管理数据汇报给发送请求的NMS。

●	SNMP Agent接收到NMS的请求信息后，通过MIB表完成相应指令后，并把操作结果响应给NMS。

●	当设备发生故障或者其它事件时，设备会通过SNMP Agent主动发送SNMP Traps给NMS，向NMS报告设备当前的状态变化。

中兴服务器BMC软件提供了SNMP Agent服务。



**MIB**

MIB是一个数据库，指明了被管理设备所维护的变量。MIB在数据库中定义了被管理设备的一系列属性：对象的名称、对象的状态、对象的访问权限和对象的数据类型等。

MIB也可以看作是NMS和SNMP Agent之间的一个接口，通过这个接口，NMS对被管理设备所维护的变量进行查询/设置操作。

MIB是以树状结构进行存储的，如[图***\*1-1\****](#_bookmark2)所示。树的节点表示被管理对象，它可以用从根开始的一条路径唯一地识别，这条路径就称为OID，如system的OID为 1.3.6.1.2.1.1，interfaces的OID为1.3.6.1.2.1.2。

子树可以用该子树根节点的OID来标识。如以private为根节点的子树的OID为private的OID{1.3.6.1.4.--}。

图 ***\*1-1\**** OID 树结构

![](snmp_doc_pic/wps1.jpg)



## 1.3 操作说明

**SNMP查询**

SNMP查询是指NMS主动向SNMP Agent发送查询请求，如[图***\*1-2\****](#_bookmark4)所示。SNMP Agent接收到查询请求后，通过MIB表完成相应指令，并将结果反馈给NMS。

SNMP查询操作有三种：Get、GetNext和GetBulk。SNMPv1版本不支持GetBulk操作。

●	Get操作：NMS使用该操作从SNMP Agent中获取一个或多个参数值。

●	GetNext操作：NMS使用该操作从SNMP Agent中获取一个或多个参数的下一个参数值。

●	GetBulk操作：基于GetNext实现，相当于连续执行多次GetNext操作。在NMS上可以设置被管理设备在一次GetBulk报文交互时，执行GetNext操作的次数。



图 ***\*1-2\**** SNMP 查询操作

![](snmp_doc_pic/wps2.jpg)



**SNMP设置**

SNMP设置是指NMS主动向SNMP Agent发送对设备进行Set操作的请求，如[图***\*1-3\****](#_bookmark13)所 示。SNMP Agent接收到Set请求后，通过MIB表完成相应指令，并将结果反馈给NMS。

SNMP设置操作只有一种Set，NMS使用该操作可设置SNMP Agent中的一个或多个参数值。



图 ***\*1-3\**** SNMP Set 操作

![](snmp_doc_pic/wps3.jpg)



**SNMP TRAPS**

SNMP Traps是指SNMP Agent主动将设备产生的告警或事件上报给NMS，以便网络管理员及时了解设备当前运行的状态。

SNMP Agent上报SNMP Traps有两种方式：Trap和Inform。SNMPv1版本不支持 Inform。Trap和Inform的区别在于，SNMP Agent通过Inform向NMS发送告警或事件后，NMS需要回复InformResponse进行确认，如[图***\*1-4\****](#_bookmark17)所示。



图 ***\*1-4\**** SNMP Traps 操作

![](snmp_doc_pic/wps4.jpg)





# 2 表描述
表分为：表量表(Tabular)和标量表(Scalar)；其中标量表所有节点都是叶子节点，没有索引，而表量表，是存在索引的。


表量表定义描述如下，其中fanIndex为索引。

![](snmp_doc_pic/tabular.JPG)



标量表定义描述如下，无索引。

![](snmp_doc_pic/scalar.JPG)



**zteBMC(1.3.6.1.4.1.3902.2601.15.1)MIB表间关系如下：**

| 节点OID                       | 节点名称               | 子节点名称                                                   |
| ----------------------------- | ---------------------- | ------------------------------------------------------------ |
| 1.3.6.1.4.1.3902.2601.15.1.1  | systemInfo             | systemInfo标量表     |
| 1.3.6.1.4.1.3902.2601.15.1.2  | domainNameSystem       | domainNameSystem（DNS）标量表                                |
| 1.3.6.1.4.1.3902.2601.15.1.5  | ntp                    | ntp标量表                                                    |
| 1.3.6.1.4.1.3902.2601.15.1.6  | syslog                 | syslog标量表<br /> syslogInfoDescriptionTable                |
| 1.3.6.1.4.1.3902.2601.15.1.7  | trap                   | trap标量表<br /> trapInfoDescriptionTable                    |
| 1.3.6.1.4.1.3902.2601.15.1.8  | smtp                   | smtp标量表<br /> smtpReceiverDescriptionTable                |
| 1.3.6.1.4.1.3902.2601.15.1.10 | powerSupplyProperty    | powerSupplyProperty标量表<br />powerSupplyPresenceTable<br />powerSupplyDescriptionTable<br />powerSupplyGroupTable|
| 1.3.6.1.4.1.3902.2601.15.1.11 | powerStatistic         | powerStatistic标量表                                         |
| 1.3.6.1.4.1.3902.2601.15.1.12 | powerManagement        | powerManagement标量表                                        |
| 1.3.6.1.4.1.3902.2601.15.1.13 | fanProperty            | fanProperty标量表<br />fanDescriptionTable                   |
| 1.3.6.1.4.1.3902.2601.15.1.16 | firmwareProperty       | firmwareDescriptionTable                                     |
| 1.3.6.1.4.1.3902.2601.15.1.17 | networkProperty        | networkProperty标量表<br />networkDescriptionTable           |
| 1.3.6.1.4.1.3902.2601.15.1.18 | sensorProperty         | sensorDescriptionTable                                       |
| 1.3.6.1.4.1.3902.2601.15.1.21 | cpuProperty            | cpuProperty标量表<br />cpuDescriptionTable<br />cpuPresenceTable |
| 1.3.6.1.4.1.3902.2601.15.1.22 | memoryProperty         | memoryProperty标量表<br />memoryDescriptionTable<br />memoryPresenceTable |
| 1.3.6.1.4.1.3902.2601.15.1.23 | fruInfo                | fruDescriptionTable                                          |
| 1.3.6.1.4.1.3902.2601.15.1.24 | pCIeDeviceProperty     | pCIeDeviceProperty标量表<br />pCIeDeviceDescriptionTable     |
| 1.3.6.1.4.1.3902.2601.15.1.26 | netCardProperty        | netCardDescriptionTable<br />netPortDescriptionTable<br />netCardMemoryInfoDescriptionTable |
| 1.3.6.1.4.1.3902.2601.15.1.27 | fcCardProperty         | fcCardDescriptionTable<br />fcPortDescriptionTable           |
| 1.3.6.1.4.1.3902.2601.15.1.28 | gpuProperty            | gpuDescriptionTable<br />gpuPerfParamTable                   |
| 1.3.6.1.4.1.3902.2601.15.1.29 | raidControllerProperty | raidControllerDescriptionTable                               |
| 1.3.6.1.4.1.3902.2601.15.1.30 | hardDiskProperty       | hardDiskProperty标量表<br /> hardDiskDescriptionTable<br /> hardDiskPresenceTable |
| 1.3.6.1.4.1.3902.2601.15.1.31 | nvmeDeviceProperty     | nvmeDeviceDescriptionTable                                   |
| 1.3.6.1.4.1.3902.2601.15.1.32 | logicalDriveProperty   | logicalDriveDescriptionTable                                 |
| 1.3.6.1.4.1.3902.2601.15.1.500 | zteTrap               | zteTrapVar<br />zteTrapEvent                                 |





# 3 接口文档修改记录

| 修改日期   | 修改记录 | BMC版本号 |
| ---------- | -------- | --------- |
| 2022/10/22 | 首次发布 |           |
| 2024/03/28 |raidControllerDeviceInterface 节点修改， hardDiskCapableSpeed 节点修改|V04.24.02.00|
| 2024/04/10 |TRAP OID变量绑定列表错别字及错别信息修改|V04.24.02.00|
| 2024/04/12 |hardDiskCapableSpeed 节点修改，hardDiskNegotiatedSpeed 节点修改|V04.24.02.00|
| 2024/04/22 |修正文档错误信息|V04.24.03.00|
| 2024/05/09 |新增trap类型GPU和加速卡|V04.24.03.00|
| 2024/05/10 |修改cpuFamily节点名称为cpuModel|V04.24.03.00|
| 2024/05/10 |fruInfo表间关系字段修改、raidControllerDeviceInterface描述信息修改|V04.24.03.00|
| 2024/05/13 | syslogProtocolType增加TLS类型 | V04.24.03.00 |
| 2024/05/17 |新增百度硬盘寿命预警|V04.24.03.00|
| 2024/05/23 |新增内存预故障trap|V04.24.03.00|
| 2024/06/04 |新增入风口温度|V04.24.03.00|
| 2024/06/13 |新增板载网卡温度告警|ZXSAC-NEO20-BMCV04.24.02.00|
| 2024/06/18 |增加syslogAuthMode节点|V04.24.03.00|
| 2024/07/01 |增加systemCurrentBootMode节点，修改systemBootMode节点为systemNextBootMode节点|V04.24.03.00|
| 2024/07/02 |修改systemInfo使用示例|V04.24.03.00|
| 2024/07/04 |systemCurrentBootMode、systemNextBootMode节点增加单值unknown|V04.24.03.00|
| 2024/07/03 |删除风扇预测故障声明告警更改为电源风扇预测故障声明告警|V04.24.03.00|
| 2024/07/16 |新增iSACVlanID及iSACVlanPriority节点|V04.24.03.00|
| 2024/07/18 |新增EDPC事件trap|V04.24.03.00|
| 2024/07/30 |新增GPU基板光模块告警|V04.24.04.00|
| 2024/08/01 |修改sensorType枚举定义|V04.24.04.00|
| 2024/08/08 |修改硬盘转速枚举定义|V04.24.04.00|
| 2024/08/09 |修改identify定义|V04.24.04.00|
| 2024/08/12 |新增环境湿度告警|V04.24.04.00|
| 2024/08/21 |新增GPU基板状态告警|V04.24.04.00|
| 2024/08/22 |修改systemPowerOnPolicy描述信息及取值范围|V04.24.04.00|
| 2024/08/26 |sensorUnit增加percent枚举定义|V04.24.04.00|
| 2024/09/09 |systemBootsequence增加RemotelyHdd描述信息|V04.24.04.00|
| 2024/09/11 |修改systemNextBootMode取值范围|V04.24.04.00|
| 2024/09/18 |新增leakageEvent sensortype,新增漏液告警|V04.24.04.00|
| 2024/09/19 |修改powerSupplyWorkMode、powerSupplyMaxAmbientTemperature描述信息|V04.24.04.00|
| 2024/09/27 |新增gpu内存不可纠正告警|V04.24.04.00|
| 2024/10/12 |新增扩展板温度告警|V04.24.04.00|
| 2024/10/15 |修改systemTimeZoneStr节点描述信息|V04.24.04.00|
| 2024/10/17 |新增gpuPerfParamTable表节点|V04.24.04.00|
| 2024/10/17 |为gpuPower节点增加单位描述|V04.24.04.00|
| 2024/10/26 | 修改powerSupplyProperty节点取值范围、OID信息及trap节点信息及systemInfo节点信息|V04.25.01.10|
| 2024/10/28 | 修改powerSupplyProperty节点OID实例|V04.25.01.10|
| 2024/10/28 |修改ntp节点描述信息|V04.25.01.10|
| 2024/10/28 | 修改syslog表描述信息|V04.25.01.20|
| 2024/10/29 | 修改fanProperty节点以及networkProperty节点|V04.25.01.20|
| 2024/11/04 | 修改pCIeDeviceProperty节点和netCardProperty节点|V04.25.01.20|
| 2024/11/05 | 修改zteTrap节点以及cpuProperty节点|V04.25.01.20|
| 2024/11/05 | 修改netCardDescriptionEntry节点|V04.25.01.20|
| 2024/11/05 | 质量任务：SNMP文档及MIB烧结文件问题梳理整改1 章节1-章节4.4, 文档描述20余处问题(正确性、一致性、中英文、格式等)|V04.25.01.20|
| 2024/11/06 | 质量任务：SNMP文档及MIB烧结文件问题梳理整改1 章节4.5-章节4.13, 文档描述20余处问题(正确性、一致性、中英文、格式等)|V04.25.01.20|
| 2024/11/07 | 修改netCardDescriptionEntry以及fcCardProperty节点|V04.25.01.20|
| 2024/11/07 | 修改fcCardModel节点以及netCardNICModel节点|V04.25.01.20|
| 2024/11/12 | 修改logicalDriveMemberList节点描述信息|V04.25.01.20|
| 2024/11/12 | 质量任务：SNMP文档及MIB烧结文件问题梳理整改 章节4.13-章节完, 文档问题|V04.25.01.20|
| 2024/11/27 | 质量任务：SNMP文档及MIB烧结文件问题梳理整改(TE BA DEV达成一致) |V04.25.01.20|
| 2024/11/28 | 新增GPU接线错误告警|V04.25.01.20|
| 2024/11/27 | 质量任务：SNMP文档及MIB烧结文件问题梳理整改(TE BA DEV达成一致，修正网络协议节点名) |V04.25.01.20|
| 2024/12/07 | 修改pCIeDeviceCurrentPower节点描述信息 |V04.25.01.20|
| 2024/12/07 | 修改hostName节点描述信息 |V04.25.01.20|
| 2024/12/20 | 新增CDU轻微故障和严重故障告警 |V04.25.01.20|
| 2024/12/27 | 修改systemBootsequence和systemBootOnce节点的描述信息 |V04.25.01.20|
| 2024/12/27 | fanAutoMode 去掉 customizedMode | V04.25.01.20 |
| 2024/12/30 | 修改systemBootOnce节点的描述信息 | V04.25.01.20 |
| 2025/01/02 | sensorUnit增加litersPerMinute枚举定义 |V04.25.01.20|
| 2025/01/02 | 新增netCardDeviceId, netPortNICDeviceId, fcCardDeviceId, fcPortCardDeviceId, gpuDeviceId节点 |V04.25.01.20|
| 2025/01/02 | 为bmcTimeSource节点扩充同步源信息 |V04.25.01.20|
| 2025/01/07 | 新增PDB严重和紧急门限告警 |V04.25.01.20|
| 2025/01/13 | 更新netCardProperty，fcCardProperty，gpuProperty使用示例 | V04.25.01.20 |
| 2025/02/21 | 更新gpuRatedPower节点描述信息 | V04.25.01.20 |
| 2025/03/06 | hardDiskAvailabilityStatus节点增加predictive-failure枚举定义 | V04.25.01.20 |
| 2025/03/10  |新增sel almost full通知|V04.25.01.20|
| 2025/03/10  |新增PCIE降带宽告警，软件热复位冷复位通知|V04.25.01.20|
| 2025/03/16 |新增0x036f0706 0x036f0707 0x03ef0707 0x206f0c06 0x20ef0c06 0x206f0c0b|V04.25.01.20|
| 2025/03/31 |新增0x07010200 0x07010202 0x07010207 0x07010209||
| 2025/03/31 |修改systemCpuUsageThre描述信息|V04.25.02.00|
| 2025/04/10 |修改systemMemUsageThre和systemDiskPartitionUsageThre描述信息|V04.25.02.00|
| 2025/05/08 |新增PDB温度高于高轻微告警阈值、电源按键误触、液冷系统故障告警|V04.25.02.10|
| 2025/05/08 |修改boardAssetTag描述信息，|V04.25.02.00|
| 2025/05/13 |新增LLDP节点描述信息|V04.25.02.20|
| 2025/05/19 |新增0x03010309|V04.25.02.00|
| 2025/05/23 |新增0x076f0801|V04.25.02.00|
| 2025/05/24 |新增0x98071802 0x98071803|V04.25.02.00|

# 4 MIB表详细规格

## 4.1  systemInfo详细规格

### 4.1.1 功能说明

#### 4.1.1.1 父节点介绍

systemInfo信息节点，包括bmc系统时间、Uid点灯配置。

systemInfo表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).systemInfo(1)

#### 4.1.1.2 子节点介绍

**标量表**

| 节点名称                     | 节点 OID 实例                   | 描述                                                         | 类型          | 权限       |
| ---------------------------- | ------------------------------- | ------------------------------------------------------------ | ------------- | ---------- |
| systemHealth                 | 1.3.6.1.4.1.3902.2601.15.1.1.1  | systemHealth information about system present state of health.<br/>This value will be one of the following:<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) | INTEGER | read-only |
| systemTime                   | 1.3.6.1.4.1.3902.2601.15.1.1.2  | systemTime information about BMC system time.<br/>the value such as (yyyy-mm-dd hh:mm:ss). | DisplayString | read-only  |
| systemTimeZone               | 1.3.6.1.4.1.3902.2601.15.1.1.3  | systemTimeZone information about BMC time zone(Integer).<br/>The value is in [-720, 840].  | Integer32     | read-only  |
| systemTimeZoneStr            | 1.3.6.1.4.1.3902.2601.15.1.1.4  | systemTimeZone information about BMC time zone(String).<br/>The value such as (Asia/Shanghai(GMT+08:00 CST)). | DisplayString | read-only  |
| systemBootsequence           | 1.3.6.1.4.1.3902.2601.15.1.1.5  | Description: Decide the system's first boot device.<br/>When systemBootOnce is permanent, setting BIOS Setup boot options is not allowed.<br/>1: noOverride(0) <br/>2: pxe(1)<br/>3: hdd(2)<br/>4: cdDvd(5)<br/> 5: biosSetup(6)<br/> 6: RemotelyHdd(11)<br/> 7: removableDevice(15) | INTEGER       | read-write |
| systemNextBootMode           | 1.3.6.1.4.1.3902.2601.15.1.1.6  | Description: Decide the next system's boot mode.<br/>1: legacy(0) <br/>2: UEFI(1) <br/>3- noOverride(2) <br/>4- unknown(255) | INTEGER       | read-write |
| systemBootOnce               | 1.3.6.1.4.1.3902.2601.15.1.1.7  | Description: System boot once or permanent.<br/> When systemBootsequence is BIOS Setup, setting permanent boot options is not allowed.<br/>1: oneTime(0) <br/>2: permanent(1)<br/> When setting one-time boot options, set systemBootOnce before systemBootsequence and systemNextBootMode. | INTEGER       | read-write  |
| systemGuid                   | 1.3.6.1.4.1.3902.2601.15.1.1.8  | The GUID is hex string such as ********-****-****-****-************.| DisplayString | read-only  |
| deviceName                   | 1.3.6.1.4.1.3902.2601.15.1.1.9  | The device name value between 1 and 63 characters.  | DisplayString | read-only  |
| deviceSerialNo               | 1.3.6.1.4.1.3902.2601.15.1.1.10 | The device serial number value between 1 and 63 characters.| DisplayString | read-only  |
| hostName                     | 1.3.6.1.4.1.3902.2601.15.1.1.11 | The host name value between 1 and 63 characters.<br/>The length range is from 1 to 63. It can only contain numbers, letters, dots (.), underscores (_), and hyphens (-). There cannot be consecutive hyphens (-). The first character must be a letter or a number, and the last character cannot be a hyphen (-) or a dot (.). | DisplayString | read-only  |
| boardAssetTag                | 1.3.6.1.4.1.3902.2601.15.1.1.12 | Asset tag is a string of 2 to 63 alpha-numeric characters. It is case-sensitive. Special characters '-'(hyphen), ':'(colon), '_'(underscore), ' '(space), '@'(a-tail) are allowed. Special characters '-'(hyphen), ':'(colon), '_'(underscore) and ' '(space) cannot be at the beginning or end. | DisplayString | read-write  |
| chassisIntrusionState        | 1.3.6.1.4.1.3902.2601.15.1.1.13 | Chassis intrusion state.<br/>1: normal(1)<br/>2: chassisIntrusion(2)<br/>3: unknown(-1)    | INTEGER  | read-only  |
| systemPowerState             | 1.3.6.1.4.1.3902.2601.15.1.1.14 | System Power Status Get.<br/>0 - Power Status Is Off<br/>1 - Power Status Is On<br/>System Power Status Set.<br/>1: powerOff(0)<br/> 2: powerOn(1)<br/> 3: powerCycle(2)<br/> 4: powerReset(3)<br/> 5: normalPowerOff(5)<br/>The set actions are a process which will take effect in a while.<br/>When system in powerOff state, Power Off/Reset/PowerCycle commands are not supported." | INTEGER       | read-write |
| systemPowerOnPolicy          | 1.3.6.1.4.1.3902.2601.15.1.1.15 | 1: stayOff(1) <br/>2: restorePreviousState(2) <br/>3: turnon(3) <br/>4: na(255)<br/> The valid input value only contains 1, 2 and 3. | INTEGER       | read-write |
| systemPresentPower           | 1.3.6.1.4.1.3902.2601.15.1.1.16 | Display the present system power. | INTEGER       | read-only |
| identify                     | 1.3.6.1.4.1.3902.2601.15.1.1.17 | identify use to control on or off of led.<br/> identify mode:<br/> 0 - Off<br/> 1 - Temporary On<br/> 2 - Force Identify On<br/> 3 - UnSupported <br />set format: <mode>,[ontime]<br/> get format: <mode><br/> 	When <mode> = 0 or <mode> = 2,<br/>the format is only <mode>.<br/> [ontime] is option and value is in [1,255],<br/> When set Temporary On without [ontime],<br/> The default Temporary On time are 255 seconds. | DisplayString | read-write |
| systemCpuUsage               | 1.3.6.1.4.1.3902.2601.15.1.1.18 | Percent of CPU usage. <br/> The value defined as: <br/> -1: invalid current CPU usage. <br/> [0,100]: represents the current CPU usage." | INTEGER       | read-only  |
| systemMemUsage               | 1.3.6.1.4.1.3902.2601.15.1.1.19 | Percent of memory usage. <br/>The value defined as: <br/> -1: invalid current memory usage. <br/> [0,100]: represents the current memory usage. | INTEGER       | read-only  |
| systemIoUsage                | 1.3.6.1.4.1.3902.2601.15.1.1.20 | Percent of IO usage. <br/>The value defined as: <br/> -1: invalid current IO usage. <br/> [0,100]: represents the current IO usage. <br/> 255:unknown <br/>NOTE: <br/>The Intel management Engine (ME) provides the ios usage. Other cpu platforms do not support this usage. | INTEGER       | read-only  |
| systemCpuUsageThre           | 1.3.6.1.4.1.3902.2601.15.1.1.21 | Percent of CPU usage threshold.<br/>This value is in [6,100].<br/>If the value is more than 100, the alarm is disabled. | INTEGER       | read-write |
| systemMemUsageThre           | 1.3.6.1.4.1.3902.2601.15.1.1.22 | Percent of memory usage threshold.<br/>This value is in [6,100].<br/>If the value is more than 100, the alarm is disabled. | INTEGER       | read-write |
| systemDiskPartitionUsageThre | 1.3.6.1.4.1.3902.2601.15.1.1.23 | Percent of hard disk partition usage threshold.<br/>This value is in [6,100].<br/>If the value is more than 100, the alarm is disabled. | INTEGER       | read-write |
| bmcReboot                    | 1.3.6.1.4.1.3902.2601.15.1.1.24 | Reboot the BMC management system.<br/>1: reboot(1)<br/>When set, the value is only 1, write only. | INTEGER       | write-only |
| systemCurrentBootMode        | 1.3.6.1.4.1.3902.2601.15.1.1.25 | the current system's boot mode.<br/>1: legacy(0)<br/>2: UEFI(1)<br/>3: unknown(255)| INTEGER       | read-only |



### 4.1.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.1.3 设置操作约束

​        支持set操作

### 4.1.4 使用示例
	***** SNMP QUERY STARTED *****
	1: systemHealth.0 (integer) ok(0)
	2: systemTime.0 (octet string) 2000-01-03 10:48:43 [32.30.30.30.2D.30.31.2D.30.33.20.31.30.3A.34.38.3A.34.33 (hex)]
	3: systemTimeZone.0 (integer) 480
	4: systemTimeZoneStr.0 (octet string) UTC+08:00 [55.54.43.2B.30.38.3A.30.30 (hex)]
	5: systemBootsequence.0 (integer) noOverride(0)
	6: systemNextBootMode.0 (integer) UEFI(1)
	7: systemBootOnce.0 (integer) permanent(1)
	8: systemGuid.0 (octet string) 30e72400-0000-1000-0000-000000000000 [33.30.65.37.32.34.30.30.2D.30.30.30.30.2D.31.30.30.30.2D.30.30.30.30.2D.30.30.30.30.30.30.30.30.30.30.30.30 (hex)]
	9: deviceName.0 (octet string) (zero-length)
	10: deviceSerialNo.0 (octet string) (zero-length)
	11: hostName.0 (octet string) iSAC0E68FAABD2C0 [69.53.41.43.30.45.36.38.46.41.41.42.44.32.43.30 (hex)]
	12: boardAssetTag.0 (octet string) (zero-length)
	13: chassisIntrusionState.0 (integer) 0
	14: systemPowerState.0 (integer) powerOn(1)
	15: systemPowerOnPolicy.0 (integer) restorePreviousState(2)
	16: systemPresentPower.0 (integer) 0
	17: identify.0 (octet string) <00> [00 (hex)]
	18: systemCpuUsage.0 (integer) -1
	19: systemMemUsage.0 (integer) -1
	20: systemIoUsage.0 (integer) -1
	21: systemCpuUsageThre.0 (integer) 75
	22: systemMemUsageThre.0 (integer) 75
	23: systemDiskPartitionUsageThre.0 (integer) 75
	25: systemCurrentBootMode.0 (integer) UEFI(1)
	***** SNMP QUERY FINISHED *****



## 4.2 domainNameSystem详细规格

### 4.2.1 功能说明

#### 4.2.1.1 父节点介绍

DNS信息的节点包括：DNS使能开关、DNS服务器设置、注册选项、域名、首选服务器、备选服务器1、备选服务器2。

domainNameSystem 表节点的OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).domainNameSystem(2)

#### 4.2.1.2 子节点介绍

**标量表**

| 节点名称           | 节点 OID 实例                  | 描述                                                                | 类型          | 权限      |
| ------------------ | ------------------------------ | ------------------------------------------------------------------- | ------------- | --------- |
| dnsEnable          | 1.3.6.1.4.1.3902.2601.15.1.2.1 | Information about DNS enabled. <br/>1: disable(1) <br/>2: enable(2) | INTEGER       | read-only |
| dnsServerSetup     | 1.3.6.1.4.1.3902.2601.15.1.2.2 | Information about DNS server setup. <br/>1: manual(1) <br/>2:autoBaseIPv4(2) <br/>3:autoBaseIPv6(3) | INTEGER       | read-only |
| dnsDynamicRegistration | 1.3.6.1.4.1.3902.2601.15.1.2.3 | Information about DNS dynamic registration method. <br/>1:hostname(1) <br/>2:FQDN(2)    | INTEGER       | read-only |
| dnsDomainName          | 1.3.6.1.4.1.3902.2601.15.1.2.4 | Domain name.                                           | DisplayString | read-only |
| preferredDNSServer     | 1.3.6.1.4.1.3902.2601.15.1.2.5 | Preferred DNS server address.                          | DisplayString | read-only |
| alternateDNSServer1    | 1.3.6.1.4.1.3902.2601.15.1.2.6 | Alternate DNS server address. It is value can be empty.| DisplayString | read-only |
| alternateDNSServer2    | 1.3.6.1.4.1.3902.2601.15.1.2.7 | Alternate DNS server address. It is value can be empty.| DisplayString | read-only |

### 4.2.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作 

### 4.2.3 设置操作约束

​        不支持set操作

### 4.2.4 使用示例
	***** SNMP QUERY STARTED *****
	1: dnsEnable.0 (integer) disable(1)
	2: dnsServerSetup.0 (integer) autoBaseIPv4(2)
	3: dnsDynamicRegistration.0 (integer) FQDN(2)
	4: dnsDomainName.0 (octet string) (zero-length)
	5: preferredDNSServer.0 (octet string) :: [3A.3A (hex)]
	6: alternateDNSServer1.0 (octet string) 0.0.0.0 [30.2E.30.2E.30.2E.30 (hex)]
	7: alternateDNSServer2.0 (octet string) :: [3A.3A (hex)]
	***** SNMP QUERY FINISHED *****



## 4.3 ntp详细规格

### 4.3.1 功能说明

#### 4.3.1.1 父节点介绍

ntp信息节点，包括5个标量：时间同步源、三组ntpserver、ntp同步时间间隔。

ntp表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).ntp(5)

#### 4.3.1.2 子节点介绍

**标量表**

| 节点名称           | 节点 OID 实例                  | 描述                                                                         | 类型          | 权限       |
| ------------------ | ------------------------------ | ---------------------------------------------------------------------------- | ------------- | ---------- |
| bmcTimeSource      | 1.3.6.1.4.1.3902.2601.15.1.5.1 | Information about ntp sync status. <br/>1: fromNtp(1) <br/>2:fromBios(2) <br/>3:fromDHCPv4(3) <br/>4:fromDHCPv6(4)    | INTEGER       | read-write |
| primaryNtpServer   | 1.3.6.1.4.1.3902.2601.15.1.5.2 | 1.Ntp primary server <br/>2.IPv4 or IPv6 address, or domain name of the preferred NTP server.<br/>3.The default value is a null string. size(0..128) | DisplayString | read-write |
| secondaryNtpServer | 1.3.6.1.4.1.3902.2601.15.1.5.3 | 1.Ntp secondary server<br/>2.IPv4 or IPv6 address, or domain name of the preferred NTP server.<br/>3.The default value is a null string. size(0..128)| DisplayString | read-write |
| tertiaryNtpServer  | 1.3.6.1.4.1.3902.2601.15.1.5.4 | 1.Ntp tertiary server<br/>2.IPv4 or IPv6 address, or domain name of the preferred NTP server.<br/>3.The default value is a null string. size(0..128) | DisplayString | read-write |
| ntpInterval        | 1.3.6.1.4.1.3902.2601.15.1.5.5 | 1.interval seconds of Ntp<br/>2.Min value is 60s. <br/>60..65535             | INTEGER       | read-write |

### 4.3.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.3.3 设置操作约束

​        支持set操作

### 4.3.4 使用示例
	***** SNMP QUERY STARTED *****
	1: bmcTimeSource.0 (integer) fromBios(2)
	2: primaryNtpServer.0 (octet string) (zero-length)
	3: secondaryNtpServer.0 (octet string) (zero-length)
	4: tertiaryNtpServer.0 (octet string) (zero-length)
	5: ntpInterval.0 (integer) 60
	***** SNMP QUERY FINISHED *****



## 4.4 syslog详细规格

### 4.4.1 功能说明

#### 4.4.1.1 父节点介绍

syslog报文信息的配置及查询，包括： 使能标志、传输协议、服务器标识；syslog接收端的各种配置信息，包括使能、接收端的地址、端口，传输的日志类型以及测试日志等。

syslog表节点的OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).syslog(6) (注： 由于trap节点占用7，所以syslog改成6)

#### 4.4.1.2 子节点介绍

**标量表**

| 节点名称             | 节点 OID 实例                  | 描述                                                         | 类型          | 权限       |
| -------------------- | ------------------------------ | ------------------------------------------------------------ | ------------- | ---------- |
| syslogEnable         | 1.3.6.1.4.1.3902.2601.15.1.6.1 | The enable state of syslog. <br/>1: disable(1)<br/>2: enable(2) <br/>Default value is enable(2). | INTEGER       | read-write |
| syslogIdentity       | 1.3.6.1.4.1.3902.2601.15.1.6.2 | Choose the server Identity when sending syslog. <br/>1: boardSN(1)<br/>2: productAssetTag(2)<br/>3: hostName(3)  | INTEGER       | read-write |
| syslogProtocolType   | 1.3.6.1.4.1.3902.2601.15.1.6.3 | The syslog protocol type. <br/>1: udp(1) <br/>2: tcp(2) <br/>3: tls(3)<br/> udp:When receiving messages using the UDP protocol. <br/> tcp:When receiving messages using the TCP protocol.<br/> tls:When receiving messages using the TLS protocol. | INTEGER | read-write |
| syslogAuthMode       | 1.3.6.1.4.1.3902.2601.15.1.6.4 | TLS authentication mode. <br/>1: oneway(1)<br/>2: twoway(2)<br/>3: na(255) <br/>When set, 255 is not supported.| INTEGER | read-write |

**表量表**

节点syslogInfoDescriptionEntry是描述syslog接收端配置的具体信息表（syslogInfoDescriptionTable）组成成分的。
其OID 为：
iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1). syslog(6). syslogInfoDescriptionTable(50). syslogInfoDescriptionEntry(1)

提示：x表示syslog接收端序号

| 节点名称            | 节点 OID 实例                         | 描述                                                         | 类型          | 权限       |
| ------------------- | ------------------------------------- | ------------------------------------------------------------ | ------------- | ---------- |
| syslogReceiverIndex  | 1.3.6.1.4.1.3902.2601.15.1.6.50.1.1.x | Information about syslog receiver index.                    | INTEGER       | read-only  |
| syslogReceiverEnable | 1.3.6.1.4.1.3902.2601.15.1.6.50.1.2.x | Syslog receiver state. <br/>1: disable(1) <br/>2: enable(2).| INTEGER       | read-write |
| syslogReceiverAddress| 1.3.6.1.4.1.3902.2601.15.1.6.50.1.3.x | Syslog receiver IP addrsss. Default value is empty.         | DisplayString | read-write |
| syslogReceiverPort   | 1.3.6.1.4.1.3902.2601.15.1.6.50.1.4.x |Syslog receiver port[1~65535]. Default value is 514.         | INTEGER       | read-write |
| syslogSendLogType    | 1.3.6.1.4.1.3902.2601.15.1.6.50.1.5.x | The log type of syslog send. <br/> Support set/get any combination of the 3 log type(OperationLogs,SecurityLogs,EventLogs), use command to separate them. <br/> all is also supported,but never use it with the 3 log types together. <br/> e.g. <br/> To set OperationLogs + SecurityLogs log type message, just set: <br/> OperationLogs,SecurityLogs <br/> To set EventLogs message, just set: <br/> EventLogs <br/> To set all level message, just set: <br/> all   | DisplayString       | read-write |
| syslogReceiverTest   | 1.3.6.1.4.1.3902.2601.15.1.6.50.1.6.x |Test the syslog. <br/>1: test(1) <br/>When set, the value is only 1.              | INTEGER       | read-write |

### 4.4.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.4.3 设置操作约束

​        支持set操作

### 4.4.4 使用示例

    ***** SNMP QUERY STARTED *****
    1: syslogEnable.0 (integer) disable(1)
    2: syslogIdentity.0 (integer) boardSN(1)
    3: syslogProtocolType.0 (integer) tls(3)
    4: syslogAuthMode.0 (integer) twoway(2)
    5: syslogReceiverIndex.0 (integer) 0
    6: syslogReceiverIndex.1 (integer) 1
    7: syslogReceiverIndex.2 (integer) 2
    8: syslogReceiverIndex.3 (integer) 3
    9: syslogReceiverEnable.0 (integer) disable(1)
    10: syslogReceiverEnable.1 (integer) disable(1)
    11: syslogReceiverEnable.2 (integer) disable(1)
    12: syslogReceiverEnable.3 (integer) disable(1)
    13: syslogReceiverAddress.0 (octet string) (zero-length)
    14: syslogReceiverAddress.1 (octet string) (zero-length)
    15: syslogReceiverAddress.2 (octet string) (zero-length)
    16: syslogReceiverAddress.3 (octet string) (zero-length)
    17: syslogReceiverPort.0 (integer) 514
    18: syslogReceiverPort.1 (integer) 514
    19: syslogReceiverPort.2 (integer) 514
    20: syslogReceiverPort.3 (integer) 514
    21: syslogSendLogType.0 (octet string) (zero-length)
    22: syslogSendLogType.1 (octet string) (zero-length)
    23: syslogSendLogType.2 (octet string) (zero-length)
    24: syslogSendLogType.3 (octet string) (zero-length)
    25: syslogReceiverTest.0 (integer) 0
    26: syslogReceiverTest.1 (integer) 0
    27: syslogReceiverTest.2 (integer) 0
    28: syslogReceiverTest.3 (integer) 0
    ***** SNMP QUERY FINISHED *****


## 4.5 trap详细规格

### 4.5.1 功能说明

#### 4.5.1.1 父节点介绍

trap信息节点，包括6个标量，以及1个表格。

trap表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).trap(7)

#### 4.5.1.2 子节点介绍

**标量表**

| 节点名称             | 节点 OID 实例                  | 描述                                     | 类型          | 权限      |
| -------------------- | ------------------------------ | ---------------------------------------- | ------------- | --------- |
| trapEnable           | 1.3.6.1.4.1.3902.2601.15.1.7.1 | The state of Trap. <br/> This value will be one of the following: <br/>1: disable(0) <br/>2: enable(1)  | INTEGER       | read-write |
| trapVersion          | 1.3.6.1.4.1.3902.2601.15.1.7.2 | Trap version. <br/> This value will be one of the following: <br/>1: v1(1) <br/>2: v2c(2) <br/>3: v3(3) | INTEGER       | read-write |
| trapCommunity        | 1.3.6.1.4.1.3902.2601.15.1.7.3 | SNMP trap community is a string of 1 to 18 alpha-numeric and special characters. <br/> Special characters: visible character except ' '(space), '''(single quotes), '\'(Backslash). <br/> '#'(#) cannot be at the beginning. | DisplayString | read-write |
| trapSecurityUserName | 1.3.6.1.4.1.3902.2601.15.1.7.4 | The security user name for SNMP TRAP V3, the user should be one of the BMC local user(with SNMP channel permission). | DisplayString | read-write |
| trapServerIdentity   | 1.3.6.1.4.1.3902.2601.15.1.7.5 | Choose the server Identity when sending trap. <br/>1: boardSN(1) <br/>2: productAssetTag(2) <br/>3: hostName(3)| INTEGER       | read-write |
| trapLevel            | 1.3.6.1.4.1.3902.2601.15.1.7.6 | The level of trap send. <br/> inform:send all level message. <br/> minor:send minor and above level message. <br/> major:send major and above level message. <br/> critical:send critical level message. <br/> 1: inform(1) <br/> 2: minor(2) <br/> 3: major(3) <br/> 4: critical(4) | INTEGER  | read-write |

**表量表**

节点trapInfoDescriptionEntry是描述表节点描述trap服务器配置的具体信息表（trapInfoDescriptionTable）组成成分的。

其OID 为：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1). trap(7). trapInfoDescriptionTable(50).trapInfoDescriptionEntry(1)

提示：x表示trap服务器序号

| 节点名称            | 节点 OID 实例                         | 描述                                                         | 类型          | 权限      |
| ------------------- | ------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| trapReceiverIndex   | 1.3.6.1.4.1.3902.2601.15.1.7.50.1.1.x |                                                              | INTEGER       | read-only |
| trapReceiverEnable  | 1.3.6.1.4.1.3902.2601.15.1.7.50.1.2.x | Trap Receiver state. <br/> 1: disable(0) <br/> 2: enable(1). | INTEGER       | read-write |
| trapReceiverPort    | 1.3.6.1.4.1.3902.2601.15.1.7.50.1.3.x | SNMP trap port, default is 162.（1~65535）                   | INTEGER       | read-write |
| trapReceiverAddress | 1.3.6.1.4.1.3902.2601.15.1.7.50.1.4.x | Trap Receiver IPv4 addrsss, IPv6 address or domain name. <br/> Default value is empty. | DisplayString | read-write |
| trapTest            | 1.3.6.1.4.1.3902.2601.15.1.7.50.1.5.x | Test the SNMP trap whether could send. <br/> When set, the value is only 1. | INTEGER       | read-write |

### 4.5.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.5.3 设置操作约束

​        支持set操作

### 4.5.4 使用示例
	1: trapEnable.0 (integer) enable(1)
	2: trapVersion.0 (integer) v2c(2)
	3: trapCommunity.0 (octet string) public [70.75.62.6C.69.63 (hex)]
	4: trapSecurityUserName.0 (octet string) (zero-length)
	5: trapServerIdentity.0 (integer) boardSN(1)
	6: trapLevel.0 (integer) inform(1)
	7: trapReceiverIndex.1 (integer) 1
	8: trapReceiverIndex.2 (integer) 2
	9: trapReceiverIndex.3 (integer) 3
	10: trapReceiverIndex.4 (integer) 4
	11: trapReceiverEnable.1 (integer) disable(0)
	12: trapReceiverEnable.2 (integer) disable(0)
	13: trapReceiverEnable.3 (integer) disable(0)
	14: trapReceiverEnable.4 (integer) disable(0)
	15: trapReceiverPort.1 (integer) 162
	16: trapReceiverPort.2 (integer) 162
	17: trapReceiverPort.3 (integer) 162
	18: trapReceiverPort.4 (integer) 162
	19: trapReceiverAddress.1 (octet string) (zero-length)
	20: trapReceiverAddress.2 (octet string) (zero-length)
	21: trapReceiverAddress.3 (octet string) (zero-length)
	22: trapReceiverAddress.4 (octet string) (zero-length)
	23: trapTest.1 (integer) 0
	24: trapTest.2 (integer) 0
	25: trapTest.3 (integer) 0
	26: trapTest.4 (integer) 0
	***** SNMP QUERY FINISHED *****



## 4.6 smtp详细规格

### 4.6.1 功能说明

#### 4.6.1.1 父节点介绍

smtp信息节点，包括10个标量，以及1个表格。

smtp表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).smtp(8)

#### 4.6.1.2 子节点介绍

**标量表**

| 节点名称             | 节点 OID 实例                  | 描述                                                         | 类型          | 权限       |
| -------------------- | ------------------------------ | ------------------------------------------------------------ | ------------- | ---------- |
| smtpEnable           | 1.3.6.1.4.1.3902.2601.15.1.8.1 | The state of SMTP. <br/>1: disable (1)<br/>2: enable (2) <br/>Default value is disable(1).  | INTEGER       | read-only  |
| smtpServerIP         | 1.3.6.1.4.1.3902.2601.15.1.8.3 | The SMTP server IPv4 address, IPv6 address or domain name.   | DisplayString | read-only  |
| smtpServerPort       | 1.3.6.1.4.1.3902.2601.15.1.8.4 | The SMTP server Port.                                        | INTEGER | read-only |
| smtpTLSEnable        | 1.3.6.1.4.1.3902.2601.15.1.8.5 | The TLS state for SMTP. <br/>1: disable (1)<br/>2: enable (2). <br/>Default value is disable(1).  | INTEGER | read-only |
| smtpLoginType        | 1.3.6.1.4.1.3902.2601.15.1.8.6 | SMTP login type. <br/>1: anonymous(1)<br/>2: account(2) <br/>Default value is anonymous(1). | INTEGER       | read-only |
| smtpLoginAccount     | 1.3.6.1.4.1.3902.2601.15.1.8.7 | Login account between 1 to 64 characters.  <br/> A login account supports all characters except space,double quotationthe,equal and the following characters:#'&. | DisplayString       | read-only |
| smtpLoginPassword    | 1.3.6.1.4.1.3902.2601.15.1.8.8 | Set user login SMTP password. Login password between 1 to 50 characters. | DisplayString       | read-only |
| smtpSendAddr         | 1.3.6.1.4.1.3902.2601.15.1.8.9 | SendAddr between 0 to 255 characters. A sendAddr supports all characters except space,double quotation,equal and the following characters:#'&. | DisplayString       | read-only |
| smtpMailTitle        | 1.3.6.1.4.1.3902.2601.15.1.8.10 |SMTP Mail Title. | DisplayString | read-only|
| smtpHostIdentify     | 1.3.6.1.4.1.3902.2601.15.1.8.11 | The HostIdentify of SMTP email title. <br/> Support set/get any combination of the 3 levels(BoardSN, AssetTag, HostName) e.g.<br/>  "BoardSN, AssetTag,HostName" | DisplayString | read-only |


**表量表**

节点smtpReceiverDescriptionEntry是描述表节点描述smtp服务器配置的具体信息表（smtpReceiverDescriptionTable）组成成分的。

其OID 为：

iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).smtp(8).smtpReceiverDescriptionTable(50).smtpReceiverDescriptionEntry(1)

提示：x表示表示smtp服务器序号

| 节点名称            | 节点 OID 实例                         | 描述                                                         | 类型          | 权限       |
| ------------------- | ------------------------------------- | ------------------------------------------------------------ | ------------- | ---------- |
| smtpReceiverIndex   | 1.3.6.1.4.1.3902.2601.15.1.8.50.1.1.x | SMTP receiver index.                                         | INTEGER       | read-only  |
| smtpReceiverState   | 1.3.6.1.4.1.3902.2601.15.1.8.50.1.2.x | SMTP receiver enable state. <br/>1: disable (1)<br/>2: enable (2) <br/>Default value is disable(1).    | INTEGER       | read-only |
| smtpReceiverAddr    | 1.3.6.1.4.1.3902.2601.15.1.8.50.1.3.x | Email address between 0 and 255 characters.  <br/> A email address supports all characters except space,double quotation,equal and the following characters:#'&.   | DisplayString       | read-only |
| smtpReceiverDescription | 1.3.6.1.4.1.3902.2601.15.1.8.50.1.4.x | Email description between 0 and 255 characters.  <br/> A email description supports all characters except double quotation,equal and the following characters:#'&. | DisplayString   | read-only |

### 4.6.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.6.3 设置操作约束

​        不支持set操作

### 4.6.4 使用示例
	***** SNMP QUERY STARTED *****
	1: smtpEnable.0 (integer) disable(1)
	2: smtpServerIP.0 (octet string) (zero-length)
	3: smtpServerPort.0 (integer) 25
	4: smtpTLSEnable.0 (integer) disable(1)
	5: smtpLoginType.0 (integer) anonymous(1)
	6: smtpLoginAccount.0 (octet string) (zero-length)
	7: smtpLoginPassword.0 (octet string) (zero-length)
	8: smtpSendAddr.0 (octet string) (zero-length)
	9: smtpMailTitle.0 (octet string) Server Alert [53.65.72.76.65.72.20.41.6C.65.72.74 (hex)]
	10: smtpHostIdentify.0 (octet string) (zero-length)
	11: smtpReceiverIndex.1 (integer) 1
	12: smtpReceiverIndex.2 (integer) 2
	13: smtpReceiverIndex.3 (integer) 3
	14: smtpReceiverIndex.4 (integer) 4
	15: smtpReceiverState.1 (integer) disable(1)
	16: smtpReceiverState.2 (integer) disable(1)
	17: smtpReceiverState.3 (integer) disable(1)
	18: smtpReceiverState.4 (integer) disable(1)
	19: smtpReceiverAddr.1 (octet string) (zero-length)
	20: smtpReceiverAddr.2 (octet string) (zero-length)
	21: smtpReceiverAddr.3 (octet string) (zero-length)
	22: smtpReceiverAddr.4 (octet string) (zero-length)
	23: smtpReceiverDescription.1 (octet string) (zero-length)
	24: smtpReceiverDescription.2 (octet string) (zero-length)
	25: smtpReceiverDescription.3 (octet string) (zero-length)
	26: smtpReceiverDescription.4 (octet string) (zero-length)
	***** SNMP QUERY FINISHED *****



## 4.7 powerSupplyProperty详细规格

### 4.7.1 功能说明

#### 4.7.1.1 父节点介绍

    powerSupply信息节点，包括支持的最大数量、在位数量、3个表量。
    表量1：powerSupplyPresence信息的显示，包括位置信息、在位信息；
    表量2：powerSupplyDescription信息的显示，包括编号Index、位置信息、设备名称、健康状态、输出状态、制造商、序列号、生产日期、固件版本、部件号、最大工作环境温度、最低工作环境温度、当前温度、输入模式、最大输出功率、当前输出功率、当前输入功率、当前输出电压、当前输入电压、工作模式；
    表量3：powerSupplyGroup信息的显示，包括：组编号Index、整体状态、设置的电源模式、实际的电源模式、主用电源。

powerSupplyProperty表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).powerSupplyProperty(10)

#### 4.7.1.2 子节点介绍

**标量表**

| 节点名称                    | 节点 OID 实例                   | 描述                                                         | 类型    | 权限      |
| --------------------------- | ------------------------------- | ------------------------------------------------------------ | ------- | --------- |
| powerSupplyMaxSupportNum    | 1.3.6.1.4.1.3902.2601.15.1.10.1 | Information about Maximum number of power supply supported.  | INTEGER | read-only |
| powerSupplyPresentNum       | 1.3.6.1.4.1.3902.2601.15.1.10.2 | Information about number of present power supply.            | INTEGER | read-only |

**表量表**

节点powerSupplyPresenceEntry是描述表节点（powerSupplyPresenceTable）组成成分的。

其OID 为：

iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1). powerSupplyProperty(10). powerSupplyPresenceTable(50).powerSupplyPresenceEntry(1)

    提示：x表示电源序号

| 节点名称                  | 节点 OID 实例                          | 描述                                                         | 类型    | 权限      |
| ------------------------- | -------------------------------------- | ------------------------------------------------------------ | ------- | --------- |
| powerSupplyLocationSlot   | 1.3.6.1.4.1.3902.2601.15.1.10.50.1.1.x | Information about power supply location slot.                | INTEGER | read-only |
| powerSupplyPresenceStatus | 1.3.6.1.4.1.3902.2601.15.1.10.50.1.2.x | Information about power supply presence.<br/>1: absence(1) <br/>2: presence(2) | INTEGER | read-only |



节点powerSupplyDescriptionEntry是描述表节点powerSupply详细信息表（powerSupplyDescriptionTable）组成成分的。其OID 为：

iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1). powerSupplyProperty(10).powerSupplyDescriptionTable(51).powerSupplyDescriptionEntry(1)

    提示：x表示电源序号

| 节点名称        | 节点 OID 实例                           | 描述                                     | 类型          | 权限      |
| --------------- | --------------------------------------- | ---------------------------------------- | ------------- | --------- |
| powerSupplyIndex                 | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.1.x  | Information about power supply index.                        | INTEGER       | read-only |
| powerSupplyLocation              | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.2.x  | Information about power supply location.                     | INTEGER       | read-only |
| powerSupplyName                  | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.3.x  | Information about power supply name.                         | DisplayString | read-only |
| powerSupplyHealthStatus          | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.4.x  | Information about power supply health status. <br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER | read-only |
| powerSupplyOutputStatus          | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.5.x  | Information about power supply output status. <br/>1: close(0) <br/>2: open(1) <br/>3: unknown(65535)| INTEGER | read-only |
| powerSupplyManufacture           | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.6.x  | Information about power supply manufacture name.             | DisplayString | read-only |
| powerSupplySN                    | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.7.x  | Information about power supply manufacture serial number.    | DisplayString | read-only |
| powerSupplyManufactureDate       | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.8.x | Information about power supply manufacture date.             | DisplayString | read-only |
| powerSupplyManufactureModel      | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.9.x | Information about power supply manufacture model.            | DisplayString | read-only |
| powerSupplyVersion               | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.10.x | Information about power supply manufacture version.          | DisplayString | read-only |
| powerSupplyPartNum               | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.11.x | Information about power supply part number.                  | DisplayString | read-only |
| powerSupplyMaxAmbientTemperature | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.12.x | Maximum ambient temperature for power supply operation(unit: Celsius). <br/>65535 means unknown.     |     INTEGER       | read-only |
| powerSupplyMinAmbientTemperature | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.13.x | Minimum ambient temperature for power supply operation(unit: Celsius).<br/>65535 means unknown.     |   INTEGER       | read-only |
| powerSupplyCurrentTemperature    | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.14.x | Information about power supply current temperature(unit: Celsius).<br/>65535 means unknown.         |   INTEGER       | read-only |
| powerSupplyInputMode             | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.15.x | Information about power supply input mode.                   | DisplayString | read-only |
| powerSupplyMaxOutputPower        | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.16.x | Information about power supply max output power(unit: W).<br/>65535 means unknown.          | INTEGER       | read-only |
| powerSupplyOutputPower           | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.17.x | Information about power supply current output power(unit: W). <br/>65535 means unknown.     | INTEGER       | read-only |
| powerSupplyInputPower            | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.18.x | Information about power supply current input power(unit: W). <br/>65535 means unknown.      | INTEGER       | read-only |
| powerSupplyVoltageOut            | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.19.x | Information about power supply current output voltage(unit: V).    | DisplayString | read-only |
| powerSupplyVoltageIn             | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.20.x | Information about power supply current input voltage(unit: V).     | DisplayString | read-only |
| powerSupplyWorkMode              | 1.3.6.1.4.1.3902.2601.15.1.10.51.1.21.x | Information about power supply work mode.<br/>1: active(1)<br/>2: backup(2)<br/>3: unknown(255) | INTEGER  | read-only |

节点powerSupplyGroupEntry是描述表节点powerSupplyGroupTable组成成分的。其OID为：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).powerSupplyProperty(10).powerSupplyGroupTable(52).powerSupplyGroupEntry(1)

    提示：x表示组序号

| 节点名称                        | 节点OID实例                            | 描述                                                                                                                                                                                          | 类型    | 权限      |
| ------------------------------- | -------------------------------------- | --------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------- | ------- | --------- |
| powerSupplyGroupIndex           | 1.3.6.1.4.1.3902.2601.15.1.10.52.1.1.x | Information about power supply group index. <br/>1:mainboard(1) <br/>2:gpu(2)                                                                                                                 | INTEGER | read-only |
| powerSupplyEntireStatus         | 1.3.6.1.4.1.3902.2601.15.1.10.52.1.2.x | Information about all power supply health status<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255)                                                      | INTEGER | read-only |
| settedPowerSupplyEntireMode     | 1.3.6.1.4.1.3902.2601.15.1.10.52.1.3.x | Setted power supply entire mode. <br/>1:loadBalance(1) <br/>2:activeBackup(2) <br/>3:unsupport(65535)                                                                                         | INTEGER | read-only |
| actualPowerSupplyEntireMode     | 1.3.6.1.4.1.3902.2601.15.1.10.52.1.4.x | Actual power supply entire mode. <br/>1:loadBalance(1) <br/>2:activeBackup(2) <br/>3:unsupport(65535)                                                                                         | INTEGER | read-only |
| settedActivePowerSupply         | 1.3.6.1.4.1.3902.2601.15.1.10.52.1.5.x | Setted active power supply. per bit represents a PS, bit0 is PS1, and so on, the bit value of 1 indicates the PS is active.can not set all PS are active or backup.The result 0 is unsupport. | INTEGER | read-only |


### 4.7.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.7.3 设置操作约束

​        不支持


### 4.7.4 使用示例


***** SNMP QUERY STARTED *****
1: powerSupplyMaxSupportNum.0 (integer) 8
2: powerSupplyPresentNum.0 (integer) 8
3: powerSupplyLocationSlot.1 (integer) 1
4: powerSupplyLocationSlot.2 (integer) 2
5: powerSupplyLocationSlot.3 (integer) 3
6: powerSupplyLocationSlot.4 (integer) 4
7: powerSupplyLocationSlot.5 (integer) 5
8: powerSupplyLocationSlot.6 (integer) 6
9: powerSupplyLocationSlot.7 (integer) 7
10: powerSupplyLocationSlot.8 (integer) 8
11: powerSupplyPresenceStatus.1 (integer) presence(2)
12: powerSupplyPresenceStatus.2 (integer) presence(2)
13: powerSupplyPresenceStatus.3 (integer) presence(2)
14: powerSupplyPresenceStatus.4 (integer) presence(2)
15: powerSupplyPresenceStatus.5 (integer) presence(2)
16: powerSupplyPresenceStatus.6 (integer) presence(2)
17: powerSupplyPresenceStatus.7 (integer) presence(2)
18: powerSupplyPresenceStatus.8 (integer) presence(2)
19: powerSupplyIndex.1 (integer) 1
20: powerSupplyIndex.2 (integer) 2
21: powerSupplyIndex.3 (integer) 3
22: powerSupplyIndex.4 (integer) 4
23: powerSupplyIndex.5 (integer) 5
24: powerSupplyIndex.6 (integer) 6
25: powerSupplyIndex.7 (integer) 7
26: powerSupplyIndex.8 (integer) 8
27: powerSupplyLocation.1 (integer) 1
28: powerSupplyLocation.2 (integer) 2
29: powerSupplyLocation.3 (integer) 3
30: powerSupplyLocation.4 (integer) 4
31: powerSupplyLocation.5 (integer) 5
32: powerSupplyLocation.6 (integer) 6
33: powerSupplyLocation.7 (integer) 7
34: powerSupplyLocation.8 (integer) 8
35: powerSupplyName.1 (octet string) PSU1 [50.53.55.31 (hex)]
36: powerSupplyName.2 (octet string) PSU2 [50.53.55.32 (hex)]
37: powerSupplyName.3 (octet string) PSU3 [50.53.55.33 (hex)]
38: powerSupplyName.4 (octet string) PSU4 [50.53.55.34 (hex)]
39: powerSupplyName.5 (octet string) PSU5 [50.53.55.35 (hex)]
40: powerSupplyName.6 (octet string) PSU6 [50.53.55.36 (hex)]
41: powerSupplyName.7 (octet string) PSU7 [50.53.55.37 (hex)]
42: powerSupplyName.8 (octet string) PSU8 [50.53.55.38 (hex)]
43: powerSupplyHealthStatus.1 (integer) ok(0)
44: powerSupplyHealthStatus.2 (integer) ok(0)
45: powerSupplyHealthStatus.3 (integer) ok(0)
46: powerSupplyHealthStatus.4 (integer) ok(0)
47: powerSupplyHealthStatus.5 (integer) ok(0)
48: powerSupplyHealthStatus.6 (integer) ok(0)
49: powerSupplyHealthStatus.7 (integer) ok(0)
50: powerSupplyHealthStatus.8 (integer) ok(0)
51: powerSupplyOutputStatus.1 (integer) open(1)
52: powerSupplyOutputStatus.2 (integer) open(1)
53: powerSupplyOutputStatus.3 (integer) open(1)
54: powerSupplyOutputStatus.4 (integer) open(1)
55: powerSupplyOutputStatus.5 (integer) open(1)
56: powerSupplyOutputStatus.6 (integer) open(1)
57: powerSupplyOutputStatus.7 (integer) open(1)
58: powerSupplyOutputStatus.8 (integer) open(1)
59: powerSupplyManufacture.1 (octet string) Great Wall [47.72.65.61.74.20.57.61.6C.6C (hex)]
60: powerSupplyManufacture.2 (octet string) Great Wall [47.72.65.61.74.20.57.61.6C.6C (hex)]
61: powerSupplyManufacture.3 (octet string) Great Wall [47.72.65.61.74.20.57.61.6C.6C (hex)]
62: powerSupplyManufacture.4 (octet string) Great Wall [47.72.65.61.74.20.57.61.6C.6C (hex)]
63: powerSupplyManufacture.5 (octet string) Great Wall [47.72.65.61.74.20.57.61.6C.6C (hex)]
64: powerSupplyManufacture.6 (octet string) Great Wall [47.72.65.61.74.20.57.61.6C.6C (hex)]
65: powerSupplyManufacture.7 (octet string) Great Wall [47.72.65.61.74.20.57.61.6C.6C (hex)]
66: powerSupplyManufacture.8 (octet string) Great Wall [47.72.65.61.74.20.57.61.6C.6C (hex)]
67: powerSupplySN.1 (octet string) 22N090000556 [32.32.4E.30.39.30.30.30.30.35.35.36 (hex)]
68: powerSupplySN.2 (octet string) 22N110000933 [32.32.4E.31.31.30.30.30.30.39.33.33 (hex)]
69: powerSupplySN.3 (octet string) 22N110000934 [32.32.4E.31.31.30.30.30.30.39.33.34 (hex)]
70: powerSupplySN.4 (octet string) 22N090000570 [32.32.4E.30.39.30.30.30.30.35.37.30 (hex)]
71: powerSupplySN.5 (octet string) 22N090000562 [32.32.4E.30.39.30.30.30.30.35.36.32 (hex)]
72: powerSupplySN.6 (octet string) 22N090000552 [32.32.4E.30.39.30.30.30.30.35.35.32 (hex)]
73: powerSupplySN.7 (octet string) 22N080000628 [32.32.4E.30.38.30.30.30.30.36.32.38 (hex)]
74: powerSupplySN.8 (octet string) 22N070001019 [32.32.4E.30.37.30.30.30.31.30.31.39 (hex)]
75: powerSupplyManufactureDate.1 (octet string) 230922 [32.33.30.39.32.32 (hex)]
76: powerSupplyManufactureDate.2 (octet string) 231105 [32.33.31.31.30.35 (hex)]
77: powerSupplyManufactureDate.3 (octet string) 231105 [32.33.31.31.30.35 (hex)]
78: powerSupplyManufactureDate.4 (octet string) 230922 [32.33.30.39.32.32 (hex)]
79: powerSupplyManufactureDate.5 (octet string) 230922 [32.33.30.39.32.32 (hex)]
80: powerSupplyManufactureDate.6 (octet string) 230922 [32.33.30.39.32.32 (hex)]
81: powerSupplyManufactureDate.7 (octet string) 230818 [32.33.30.38.31.38 (hex)]
82: powerSupplyManufactureDate.8 (octet string) 230822 [32.33.30.38.32.32 (hex)]
83: powerSupplyManufactureModel.1 (octet string) CRPS3200TS5 [43.52.50.53.33.32.30.30.54.53.35 (hex)]
84: powerSupplyManufactureModel.2 (octet string) CRPS3200TS5 [43.52.50.53.33.32.30.30.54.53.35 (hex)]
85: powerSupplyManufactureModel.3 (octet string) CRPS3200TS5 [43.52.50.53.33.32.30.30.54.53.35 (hex)]
86: powerSupplyManufactureModel.4 (octet string) CRPS3200TS5 [43.52.50.53.33.32.30.30.54.53.35 (hex)]
87: powerSupplyManufactureModel.5 (octet string) CRPS3200TS5 [43.52.50.53.33.32.30.30.54.53.35 (hex)]
88: powerSupplyManufactureModel.6 (octet string) CRPS3200TS5 [43.52.50.53.33.32.30.30.54.53.35 (hex)]
89: powerSupplyManufactureModel.7 (octet string) CRPS2700D2 [43.52.50.53.32.37.30.30.44.32 (hex)]
90: powerSupplyManufactureModel.8 (octet string) CRPS2700D2 [43.52.50.53.32.37.30.30.44.32 (hex)]
91: powerSupplyVersion.1 (octet string) DC:1.1 PFC:1.1 [44.43.3A.31.2E.31.20.50.46.43.3A.31.2E.31 (hex)]
92: powerSupplyVersion.2 (octet string) DC:1.1 PFC:1.1 [44.43.3A.31.2E.31.20.50.46.43.3A.31.2E.31 (hex)]
93: powerSupplyVersion.3 (octet string) DC:1.1 PFC:1.1 [44.43.3A.31.2E.31.20.50.46.43.3A.31.2E.31 (hex)]
94: powerSupplyVersion.4 (octet string) DC:1.1 PFC:1.1 [44.43.3A.31.2E.31.20.50.46.43.3A.31.2E.31 (hex)]
95: powerSupplyVersion.5 (octet string) DC:1.1 PFC:1.1 [44.43.3A.31.2E.31.20.50.46.43.3A.31.2E.31 (hex)]
96: powerSupplyVersion.6 (octet string) DC:1.1 PFC:1.1 [44.43.3A.31.2E.31.20.50.46.43.3A.31.2E.31 (hex)]
97: powerSupplyVersion.7 (octet string) DC:0.5 PFC:0.4 [44.43.3A.30.2E.35.20.50.46.43.3A.30.2E.34 (hex)]
98: powerSupplyVersion.8 (octet string) DC:0.5 PFC:0.4 [44.43.3A.30.2E.35.20.50.46.43.3A.30.2E.34 (hex)]
99: powerSupplyPartNum.1 (octet string) N/A [4E.2F.41 (hex)]
100: powerSupplyPartNum.2 (octet string) N/A [4E.2F.41 (hex)]
101: powerSupplyPartNum.3 (octet string) N/A [4E.2F.41 (hex)]
102: powerSupplyPartNum.4 (octet string) N/A [4E.2F.41 (hex)]
103: powerSupplyPartNum.5 (octet string) N/A [4E.2F.41 (hex)]
104: powerSupplyPartNum.6 (octet string) N/A [4E.2F.41 (hex)]
105: powerSupplyPartNum.7 (octet string) N/A [4E.2F.41 (hex)]
106: powerSupplyPartNum.8 (octet string) N/A [4E.2F.41 (hex)]
107: powerSupplyMaxAmbientTemperature.1 (integer) 55
108: powerSupplyMaxAmbientTemperature.2 (integer) 55
109: powerSupplyMaxAmbientTemperature.3 (integer) 55
110: powerSupplyMaxAmbientTemperature.4 (integer) 55
111: powerSupplyMaxAmbientTemperature.5 (integer) 55
112: powerSupplyMaxAmbientTemperature.6 (integer) 55
113: powerSupplyMaxAmbientTemperature.7 (integer) 55
114: powerSupplyMaxAmbientTemperature.8 (integer) 55
115: powerSupplyMinAmbientTemperature.1 (integer) 0
116: powerSupplyMinAmbientTemperature.2 (integer) 0
117: powerSupplyMinAmbientTemperature.3 (integer) 0
118: powerSupplyMinAmbientTemperature.4 (integer) 0
119: powerSupplyMinAmbientTemperature.5 (integer) 0
120: powerSupplyMinAmbientTemperature.6 (integer) 0
121: powerSupplyMinAmbientTemperature.7 (integer) 0
122: powerSupplyMinAmbientTemperature.8 (integer) 0
123: powerSupplyCurrentTemperature.1 (integer) 26
124: powerSupplyCurrentTemperature.2 (integer) 28
125: powerSupplyCurrentTemperature.3 (integer) 29
126: powerSupplyCurrentTemperature.4 (integer) 28
127: powerSupplyCurrentTemperature.5 (integer) 27
128: powerSupplyCurrentTemperature.6 (integer) 26
129: powerSupplyCurrentTemperature.7 (integer) 27
130: powerSupplyCurrentTemperature.8 (integer) 25
131: powerSupplyInputMode.1 (octet string) AC [41.43 (hex)]
132: powerSupplyInputMode.2 (octet string) AC [41.43 (hex)]
133: powerSupplyInputMode.3 (octet string) AC [41.43 (hex)]
134: powerSupplyInputMode.4 (octet string) AC [41.43 (hex)]
135: powerSupplyInputMode.5 (octet string) AC [41.43 (hex)]
136: powerSupplyInputMode.6 (octet string) AC [41.43 (hex)]
137: powerSupplyInputMode.7 (octet string) AC [41.43 (hex)]
138: powerSupplyInputMode.8 (octet string) AC [41.43 (hex)]
139: powerSupplyMaxOutputPower.1 (integer) 3200
140: powerSupplyMaxOutputPower.2 (integer) 3200
141: powerSupplyMaxOutputPower.3 (integer) 3200
142: powerSupplyMaxOutputPower.4 (integer) 3200
143: powerSupplyMaxOutputPower.5 (integer) 3200
144: powerSupplyMaxOutputPower.6 (integer) 3200
145: powerSupplyMaxOutputPower.7 (integer) 2700
146: powerSupplyMaxOutputPower.8 (integer) 2700
147: powerSupplyOutputPower.1 (integer) 0
148: powerSupplyOutputPower.2 (integer) 462
149: powerSupplyOutputPower.3 (integer) 465
150: powerSupplyOutputPower.4 (integer) 441
151: powerSupplyOutputPower.5 (integer) 0
152: powerSupplyOutputPower.6 (integer) 0
153: powerSupplyOutputPower.7 (integer) 455
154: powerSupplyOutputPower.8 (integer) 0
155: powerSupplyInputPower.1 (integer) 4
156: powerSupplyInputPower.2 (integer) 491
157: powerSupplyInputPower.3 (integer) 486
158: powerSupplyInputPower.4 (integer) 471
159: powerSupplyInputPower.5 (integer) 4
160: powerSupplyInputPower.6 (integer) 4
161: powerSupplyInputPower.7 (integer) 488
162: powerSupplyInputPower.8 (integer) 4
163: powerSupplyVoltageOut.1 (octet string) 53.05 [35.33.2E.30.35 (hex)]
164: powerSupplyVoltageOut.2 (octet string) 54.47 [35.34.2E.34.37 (hex)]
165: powerSupplyVoltageOut.3 (octet string) 54.53 [35.34.2E.35.33 (hex)]
166: powerSupplyVoltageOut.4 (octet string) 54.52 [35.34.2E.35.32 (hex)]
167: powerSupplyVoltageOut.5 (octet string) 53.04 [35.33.2E.30.34 (hex)]
168: powerSupplyVoltageOut.6 (octet string) 53.06 [35.33.2E.30.36 (hex)]
169: powerSupplyVoltageOut.7 (octet string) 12.19 [31.32.2E.31.39 (hex)]
170: powerSupplyVoltageOut.8 (octet string) 11.71 [31.31.2E.37.31 (hex)]
171: powerSupplyVoltageIn.1 (octet string) 230 [32.33.30 (hex)]
172: powerSupplyVoltageIn.2 (octet string) 230 [32.33.30 (hex)]
173: powerSupplyVoltageIn.3 (octet string) 234 [32.33.34 (hex)]
174: powerSupplyVoltageIn.4 (octet string) 231 [32.33.31 (hex)]
175: powerSupplyVoltageIn.5 (octet string) 230 [32.33.30 (hex)]
176: powerSupplyVoltageIn.6 (octet string) 230 [32.33.30 (hex)]
177: powerSupplyVoltageIn.7 (octet string) 230 [32.33.30 (hex)]
178: powerSupplyVoltageIn.8 (octet string) 231 [32.33.31 (hex)]
179: powerSupplyWorkMode.1 (integer) backup(2)
180: powerSupplyWorkMode.2 (integer) active(1)
181: powerSupplyWorkMode.3 (integer) active(1)
182: powerSupplyWorkMode.4 (integer) active(1)
183: powerSupplyWorkMode.5 (integer) backup(2)
184: powerSupplyWorkMode.6 (integer) backup(2)
185: powerSupplyWorkMode.7 (integer) active(1)
186: powerSupplyWorkMode.8 (integer) backup(2)
187: powerSupplyGroupIndex.1 (integer) 1
188: powerSupplyGroupIndex.2 (integer) 2
189: powerSupplyEntireStatus.1 (integer) ok(0)
190: powerSupplyEntireStatus.2 (integer) ok(0)
191: settedPowerSupplyEntireMode.1 (integer) activeBackup(2)
192: settedPowerSupplyEntireMode.2 (integer) activeBackup(2)
193: actualPowerSupplyEntireMode.1 (integer) activeBackup(2)
194: actualPowerSupplyEntireMode.2 (integer) activeBackup(2)
195: settedActivePowerSupply.1 (integer) 1
196: settedActivePowerSupply.2 (integer) 14
***** SNMP QUERY FINISHED *****


## 4.8 powerStatistic详细规格

### 4.8.1 功能说明

#### 4.8.1.1 父节点介绍

功率统计相关信息查询，包括峰值功率、峰值功率发生时间、平均功率等。

powerStatistic表节点的OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).powerStatistic(11)

#### 4.8.1.2 子节点介绍

**标量表**

| 节点名称          | 节点 OID 实例                   | 描述                                                | 类型          | 权限      |
| ----------------- | ------------------------------- | ----------------------------------------------------| ------------- | --------- |
| peakPower         | 1.3.6.1.4.1.3902.2601.15.1.11.1 | System peak power(unit: W).                         | DisplayString | read-only |
| peakPowerOccurTime| 1.3.6.1.4.1.3902.2601.15.1.11.2 | System peak power occur time, based on UTC.         | DisplayString | read-only |
| averagePower      | 1.3.6.1.4.1.3902.2601.15.1.11.3 | System average power(unit: W).                      | DisplayString | read-only |

### 4.8.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.8.3 设置操作约束

​        不支持

### 4.8.4 使用示例
	***** SNMP QUERY STARTED *****
	1: peakPower.0 (octet string) 0W [30.57 (hex)]
	2: peakPowerOccurTime.0 (octet string) 1970-01-01 00:00:00 [31.39.37.30.2D.30.31.2D.30.31.20.30.30.3A.30.30.3A.30.30 (hex)]
	3: averagePower.0 (octet string) 0W [30.57 (hex)]
	***** SNMP QUERY FINISHED *****



## 4.9 powerManagement详细规格

### 4.9.1 功能说明

#### 4.9.1.1 父节点介绍

powerManagement信息节点，包括功率控制功能的配置及查询，包括使能标志和封顶值，及封顶失败的主机动作（暂未实现）。

powerManagement表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).powerManagment(12)

#### 4.9.1.2 子节点介绍

**标量表**

| 节点名称          | 节点 OID 实例                   | 描述                                                         | 类型    | 权限       |
| ----------------- | ------------------------------- | ------------------------------------------------------------ | ------- | ---------- |
| powerThreshEnable | 1.3.6.1.4.1.3902.2601.15.1.12.1 | Power threshold status. <br/>1: disable(1) <br/>2: enable(2) <br/>Default value is disable(1). | INTEGER | read-write |
| powerThreshValue  | 1.3.6.1.4.1.3902.2601.15.1.12.2 | Power threshold value, the vaule is in [5, 32767].           | INTEGER | read-write |
| powerLimitEnable  | 1.3.6.1.4.1.3902.2601.15.1.12.4 | Power limit status. <br/>1: disable(1) <br/>2: enable(2) <br/>Default value is disable(1). | INTEGER | read-write |
| powerLimitValue   | 1.3.6.1.4.1.3902.2601.15.1.12.5 | Power limit value, the vaule is in [1, 32767].               | INTEGER | read-write |

### 4.9.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作 				

### 4.9.3 设置操作约束

​        支持set操作

### 4.9.4 使用示例
	***** SNMP QUERY STARTED *****
	1: powerThreshEnable.0 (integer) disable(1)
	2: powerThreshValue.0 (integer) 500
	3: powerLimitEnable.0 (integer) disable(1)
	4: powerLimitValue.0 (integer) 500
	***** SNMP QUERY FINISHED *****



## 4.10 fanProperty详细规格

### 4.10.1 功能说明

#### 4.10.1.1 父节点介绍

    风扇信息节点，包括：散热策略、自动策略下的散热模式、手动策略下的转速百分比的查询和配置，1个表量：风扇的详细信息表（包括风扇名称、风扇在位信息、风扇健康状态、风扇转速比、风扇最大转速、风扇最小转速、风扇型号）。

fanProperty表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).fanProperty(13)

#### 4.10.1.2 子节点介绍

**标量表**

| 节点名称           | 节点 OID 实例                   | 描述                                                         | 类型    | 权限       |
| ------------------ | ------------------------------- | ------------------------------------------------------------ | ------- | ---------- |
| fanEntireStatus    | 1.3.6.1.4.1.3902.2601.15.1.13.1 | Information about all fantray health status.<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255)  | INTEGER | read-only  |
| fanControlPolicy   | 1.3.6.1.4.1.3902.2601.15.1.13.2 | Thermal Policy. <br/>1: auto(0) <br/> 2: manual(1)           | INTEGER | read-write |
| fanAutoMode        | 1.3.6.1.4.1.3902.2601.15.1.13.3 | Cooling Mode when thermal policy is auto. It can't set when thermal policy is manual. <br/>1: normalMode(0) <br/> 2: highPerformanceMode(1) <br/>3: lowNoiseMode(2) <br/> 4: unknown(255)| INTEGER | read-write |
| fanSpeedLevel      | 1.3.6.1.4.1.3902.2601.15.1.13.4 | Speed Percentage when thermal policy is manual. It can't set when thermal policy is auto. <br/>255 means unknown.| INTEGER | read-write |



**表量表**

节点fanDescriptionEntry是描述表节点风扇的详细信息表（ fanDescriptionTable）组成成分的。

其OID 为：

iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).fanProperty(13).fanDescriptionTable(50).fanDescriptionEntry(1)

    提示：x表示风扇序号

| 节点名称        | 节点 OID 实例                           | 描述                                     | 类型          | 权限      |
| --------------- | --------------------------------------- | ---------------------------------------- | ------------- | --------- |
| fanIndex        | 1.3.6.1.4.1.3902.2601.15.1.13.50.1.1.x  | Information about fantray index.         | INTEGER       | read-only |
| fanName         | 1.3.6.1.4.1.3902.2601.15.1.13.50.1.2.x  | Information about fantray silk print.    | DisplayString | read-only |
| fanPresence     | 1.3.6.1.4.1.3902.2601.15.1.13.50.1.3.x  | Information about fantray presence. <br/>1: absence(1) <br/> 2: presence(2)     | INTEGER       | read-only |
| fanHealthStatus | 1.3.6.1.4.1.3902.2601.15.1.13.50.1.4.x  | Information about fantray health status. <br/>1:ok(0) <br/> 2:minor(2) <br/> 3:major(3) <br/> 4:critical(4) <br/> 5:unknown(255)| INTEGER       | read-only |
| fanSpeedRatio   | 1.3.6.1.4.1.3902.2601.15.1.13.50.1.5.x  | Information about fantray pwm Ratio. <br/>255 means unknown. | INTEGER       | read-only |
| fanCurrentSpeed | 1.3.6.1.4.1.3902.2601.15.1.13.50.1.6.x  | Information about fantray speed.         | DisplayString | read-only |
| fanMaxSpeed     | 1.3.6.1.4.1.3902.2601.15.1.13.50.1.7.x  | Information about fantray maximum speed. | DisplayString | read-only |
| fanMinSpeed     | 1.3.6.1.4.1.3902.2601.15.1.13.50.1.8.x  | Information about fantray minimum speed. | DisplayString | read-only |
| fanSerialNumber | 1.3.6.1.4.1.3902.2601.15.1.13.50.1.9.x  | Information about fantray serial number. | DisplayString | read-only |
| fanModel        | 1.3.6.1.4.1.3902.2601.15.1.13.50.1.10.x | Information about fantray Model.         | DisplayString | read-only |

### 4.10.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.10.3 设置操作约束

​        支持set操作

### 4.10.4 使用示例
	***** SNMP QUERY STARTED *****
	1: fanEntireStatus.0 (integer) unknown(255)
	2: fanControlPolicy.0 (integer) auto(0)
	3: fanAutoMode.0 (integer) normalMode(0)
	4: fanSpeedLevel.0 (integer) unknown(255)
	5: fanIndex.1 (integer) 1
	6: fanIndex.2 (integer) 2
	7: fanIndex.3 (integer) 3
	8: fanIndex.4 (integer) 4
	9: fanIndex.5 (integer) 5
	10: fanIndex.6 (integer) 6
	11: fanIndex.7 (integer) 7
	12: fanIndex.8 (integer) 8
	13: fanIndex.9 (integer) 9
	14: fanIndex.10 (integer) 10
	15: fanIndex.11 (integer) 11
	16: fanIndex.12 (integer) 12
	17: fanName.1 (octet string) N/A [4E.2F.41 (hex)]
	18: fanName.2 (octet string) N/A [4E.2F.41 (hex)]
	19: fanName.3 (octet string) N/A [4E.2F.41 (hex)]
	20: fanName.4 (octet string) N/A [4E.2F.41 (hex)]
	21: fanName.5 (octet string) N/A [4E.2F.41 (hex)]
	22: fanName.6 (octet string) N/A [4E.2F.41 (hex)]
	23: fanName.7 (octet string) N/A [4E.2F.41 (hex)]
	24: fanName.8 (octet string) N/A [4E.2F.41 (hex)]
	25: fanName.9 (octet string) N/A [4E.2F.41 (hex)]
	26: fanName.10 (octet string) N/A [4E.2F.41 (hex)]
	27: fanName.11 (octet string) N/A [4E.2F.41 (hex)]
	28: fanName.12 (octet string) N/A [4E.2F.41 (hex)]
	29: fanPresence.1 (integer) presence(2)
	30: fanPresence.2 (integer) presence(2)
	31: fanPresence.3 (integer) presence(2)
	32: fanPresence.4 (integer) presence(2)
	33: fanPresence.5 (integer) absence(1)
	34: fanPresence.6 (integer) presence(2)
	35: fanPresence.7 (integer) presence(2)
	36: fanPresence.8 (integer) presence(2)
	37: fanPresence.9 (integer) presence(2)
	38: fanPresence.10 (integer) presence(2)
	39: fanPresence.11 (integer) presence(2)
	40: fanPresence.12 (integer) presence(2)
	41: fanHealthStatus.1 (integer) unknown(255)
	42: fanHealthStatus.2 (integer) unknown(255)
	43: fanHealthStatus.3 (integer) unknown(255)
	44: fanHealthStatus.4 (integer) unknown(255)
	45: fanHealthStatus.5 (integer) unknown(255)
	46: fanHealthStatus.6 (integer) unknown(255)
	47: fanHealthStatus.7 (integer) unknown(255)
	48: fanHealthStatus.8 (integer) unknown(255)
	49: fanHealthStatus.9 (integer) unknown(255)
	50: fanHealthStatus.10 (integer) unknown(255)
	51: fanHealthStatus.11 (integer) unknown(255)
	52: fanHealthStatus.12 (integer) unknown(255)
	53: fanSpeedRatio.1 (integer) 0
	54: fanSpeedRatio.2 (integer) 0
	55: fanSpeedRatio.3 (integer) 0
	56: fanSpeedRatio.4 (integer) 0
	57: fanSpeedRatio.5 (integer) unknown(255)
	58: fanSpeedRatio.6 (integer) 0
	59: fanSpeedRatio.7 (integer) 0
	60: fanSpeedRatio.8 (integer) 0
	61: fanSpeedRatio.9 (integer) 0
	62: fanSpeedRatio.10 (integer) 0
	63: fanSpeedRatio.11 (integer) 0
	64: fanSpeedRatio.12 (integer) 0
	65: fanCurrentSpeed.1 (octet string) N/A [4E.2F.41 (hex)]
	66: fanCurrentSpeed.2 (octet string) N/A [4E.2F.41 (hex)]
	67: fanCurrentSpeed.3 (octet string) N/A [4E.2F.41 (hex)]
	68: fanCurrentSpeed.4 (octet string) N/A [4E.2F.41 (hex)]
	69: fanCurrentSpeed.5 (octet string) N/A [4E.2F.41 (hex)]
	70: fanCurrentSpeed.6 (octet string) N/A [4E.2F.41 (hex)]
	71: fanCurrentSpeed.7 (octet string) N/A [4E.2F.41 (hex)]
	72: fanCurrentSpeed.8 (octet string) N/A [4E.2F.41 (hex)]
	73: fanCurrentSpeed.9 (octet string) N/A [4E.2F.41 (hex)]
	74: fanCurrentSpeed.10 (octet string) N/A [4E.2F.41 (hex)]
	75: fanCurrentSpeed.11 (octet string) N/A [4E.2F.41 (hex)]
	76: fanCurrentSpeed.12 (octet string) N/A [4E.2F.41 (hex)]
	77: fanMaxSpeed.1 (octet string) N/A [4E.2F.41 (hex)]
	78: fanMaxSpeed.2 (octet string) N/A [4E.2F.41 (hex)]
	79: fanMaxSpeed.3 (octet string) N/A [4E.2F.41 (hex)]
	80: fanMaxSpeed.4 (octet string) N/A [4E.2F.41 (hex)]
	81: fanMaxSpeed.5 (octet string) N/A [4E.2F.41 (hex)]
	82: fanMaxSpeed.6 (octet string) N/A [4E.2F.41 (hex)]
	83: fanMaxSpeed.7 (octet string) N/A [4E.2F.41 (hex)]
	84: fanMaxSpeed.8 (octet string) N/A [4E.2F.41 (hex)]
	85: fanMaxSpeed.9 (octet string) N/A [4E.2F.41 (hex)]
	86: fanMaxSpeed.10 (octet string) N/A [4E.2F.41 (hex)]
	87: fanMaxSpeed.11 (octet string) N/A [4E.2F.41 (hex)]
	88: fanMaxSpeed.12 (octet string) N/A [4E.2F.41 (hex)]
	89: fanMinSpeed.1 (octet string) N/A [4E.2F.41 (hex)]
	90: fanMinSpeed.2 (octet string) N/A [4E.2F.41 (hex)]
	91: fanMinSpeed.3 (octet string) N/A [4E.2F.41 (hex)]
	92: fanMinSpeed.4 (octet string) N/A [4E.2F.41 (hex)]
	93: fanMinSpeed.5 (octet string) N/A [4E.2F.41 (hex)]
	94: fanMinSpeed.6 (octet string) N/A [4E.2F.41 (hex)]
	95: fanMinSpeed.7 (octet string) N/A [4E.2F.41 (hex)]
	96: fanMinSpeed.8 (octet string) N/A [4E.2F.41 (hex)]
	97: fanMinSpeed.9 (octet string) N/A [4E.2F.41 (hex)]
	98: fanMinSpeed.10 (octet string) N/A [4E.2F.41 (hex)]
	99: fanMinSpeed.11 (octet string) N/A [4E.2F.41 (hex)]
	100: fanMinSpeed.12 (octet string) N/A [4E.2F.41 (hex)]
	101: fanSerialNumber.1 (octet string) N/A [4E.2F.41 (hex)]
	102: fanSerialNumber.2 (octet string) N/A [4E.2F.41 (hex)]
	103: fanSerialNumber.3 (octet string) N/A [4E.2F.41 (hex)]
	104: fanSerialNumber.4 (octet string) N/A [4E.2F.41 (hex)]
	105: fanSerialNumber.5 (octet string) N/A [4E.2F.41 (hex)]
	106: fanSerialNumber.6 (octet string) N/A [4E.2F.41 (hex)]
	107: fanSerialNumber.7 (octet string) N/A [4E.2F.41 (hex)]
	108: fanSerialNumber.8 (octet string) N/A [4E.2F.41 (hex)]
	109: fanSerialNumber.9 (octet string) N/A [4E.2F.41 (hex)]
	110: fanSerialNumber.10 (octet string) N/A [4E.2F.41 (hex)]
	111: fanSerialNumber.11 (octet string) N/A [4E.2F.41 (hex)]
	112: fanSerialNumber.12 (octet string) N/A [4E.2F.41 (hex)]
	113: fanModel.1 (octet string) N/A [4E.2F.41 (hex)]
	114: fanModel.2 (octet string) N/A [4E.2F.41 (hex)]
	115: fanModel.3 (octet string) N/A [4E.2F.41 (hex)]
	116: fanModel.4 (octet string) N/A [4E.2F.41 (hex)]
	117: fanModel.5 (octet string) N/A [4E.2F.41 (hex)]
	118: fanModel.6 (octet string) N/A [4E.2F.41 (hex)]
	119: fanModel.7 (octet string) N/A [4E.2F.41 (hex)]
	120: fanModel.8 (octet string) N/A [4E.2F.41 (hex)]
	121: fanModel.9 (octet string) N/A [4E.2F.41 (hex)]
	122: fanModel.10 (octet string) N/A [4E.2F.41 (hex)]
	123: fanModel.11 (octet string) N/A [4E.2F.41 (hex)]
	124: fanModel.12 (octet string) N/A [4E.2F.41 (hex)]
	***** SNMP QUERY FINISHED *****



## 4.11 firmwareProperty详细规格

### 4.11.1 功能说明

#### 4.11.1.1 父节点介绍

母版和子卡固件版本信息

firmwareProperty表节点的OID为：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).firmwareProperty(16)

**表量表**

节点firmwareDescriptionEntry是描述表节点固件的详细信息表（firmwareDescriptionTable）组成成分的。

其OID 为：

iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).firmwareProperty(16).firmwareDescriptionTable(50).firmwareDescriptionEntry(1)

    提示：x表示固件设备序号

| 节点名称        | 节点 OID 实例                           | 描述                                | 类型          | 权限      |
| --------------- | --------------------------------------- | ----------------------------------- | ------------- | --------- |
| firmwareName    | 1.3.6.1.4.1.3902.2601.15.1.16.50.1.1.x  | The name of firmware. size(0..128)  | DisplayString | read-only |
| firmwareType    | 1.3.6.1.4.1.3902.2601.15.1.16.50.1.2.x  | Version Type. <br/>1: epld(7) <br/>2: bmc(14) <br/>3: fru(15) <br/>4: boot(20) <br/>5: bios(26) <br/> 6: unknown(255)  | INTEGER       | read-only |
| firmwareVersion | 1.3.6.1.4.1.3902.2601.15.1.16.50.1.3.x  | Firmware Version. size(0..128)      | DisplayString | read-only |
| fruNumber       | 1.3.6.1.4.1.3902.2601.15.1.16.50.1.4.x  | Fru id.                             | INTEGER       | read-only |
| firmwareBoard   | 1.3.6.1.4.1.3902.2601.15.1.16.50.1.5.x  | Descripts the firmware's location. size(0..128)| DisplayString | read-only |
| firmwareExtraInfo | 1.3.6.1.4.1.3902.2601.15.1.16.50.1.6.x | Resevered. size(0..128)            | DisplayString | read-only |

### 4.11.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.11.3 设置操作约束

​        不支持set操作

### 4.11.4 使用示例
	***** SNMP QUERY STARTED *****
	1: firmwareName.0.4.66.79.79.84 (octet string) BOOT [42.4F.4F.54 (hex)]
	2: firmwareName.0.9.83.108.97.118.101.32.66.77.67 (octet string) Slave BMC [53.6C.61.76.65.20.42.4D.43 (hex)]
	3: firmwareName.0.10.77.97.115.116.101.114.32.66.77.67 (octet string) Master BMC [4D.61.73.74.65.72.20.42.4D.43 (hex)]
	4: firmwareName.0.10.83.108.97.118.101.32.66.73.79.83 (octet string) Slave BIOS [53.6C.61.76.65.20.42.49.4F.53 (hex)]
	5: firmwareName.0.11.77.97.115.116.101.114.32.66.73.79.83 (octet string) Master BIOS [4D.61.73.74.65.72.20.42.49.4F.53 (hex)]
	6: firmwareName.0.13.77.97.105.110.98.111.97.114.100.32.70.82.85 (octet string) Mainboard FRU [4D.61.69.6E.62.6F.61.72.64.20.46.52.55 (hex)]
	7: firmwareName.0.14.77.97.105.110.98.111.97.114.100.32.69.80.76.68 (octet string) Mainboard EPLD [4D.61.69.6E.62.6F.61.72.64.20.45.50.4C.44 (hex)]
	8: firmwareName.2.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) SubCard FRU [53.75.62.43.61.72.64.20.46.52.55 (hex)]
	9: firmwareName.2.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) SubCard EPLD [53.75.62.43.61.72.64.20.45.50.4C.44 (hex)]
	10: firmwareName.3.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) SubCard FRU [53.75.62.43.61.72.64.20.46.52.55 (hex)]
	11: firmwareName.3.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) SubCard EPLD [53.75.62.43.61.72.64.20.45.50.4C.44 (hex)]
	12: firmwareName.6.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) SubCard FRU [53.75.62.43.61.72.64.20.46.52.55 (hex)]
	13: firmwareName.6.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) SubCard EPLD [53.75.62.43.61.72.64.20.45.50.4C.44 (hex)]
	14: firmwareType.0.4.66.79.79.84 (integer) boot(20)
	15: firmwareType.0.9.83.108.97.118.101.32.66.77.67 (integer) bmc(14)
	16: firmwareType.0.10.77.97.115.116.101.114.32.66.77.67 (integer) bmc(14)
	17: firmwareType.0.10.83.108.97.118.101.32.66.73.79.83 (integer) bios(26)
	18: firmwareType.0.11.77.97.115.116.101.114.32.66.73.79.83 (integer) bios(26)
	19: firmwareType.0.13.77.97.105.110.98.111.97.114.100.32.70.82.85 (integer) fru(15)
	20: firmwareType.0.14.77.97.105.110.98.111.97.114.100.32.69.80.76.68 (integer) epld(7)
	21: firmwareType.2.11.83.117.98.67.97.114.100.32.70.82.85 (integer) fru(15)
	22: firmwareType.2.12.83.117.98.67.97.114.100.32.69.80.76.68 (integer) epld(7)
	23: firmwareType.3.11.83.117.98.67.97.114.100.32.70.82.85 (integer) fru(15)
	24: firmwareType.3.12.83.117.98.67.97.114.100.32.69.80.76.68 (integer) epld(7)
	25: firmwareType.6.11.83.117.98.67.97.114.100.32.70.82.85 (integer) fru(15)
	26: firmwareType.6.12.83.117.98.67.97.114.100.32.69.80.76.68 (integer) epld(7)
	27: firmwareVersion.0.4.66.79.79.84 (octet string) 04.22.02.01 [30.34.2E.32.32.2E.30.32.2E.30.31 (hex)]
	28: firmwareVersion.0.9.83.108.97.118.101.32.66.77.67 (octet string) N/A [4E.2F.41 (hex)]
	29: firmwareVersion.0.10.77.97.115.116.101.114.32.66.77.67 (octet string) 04.22.02.01 [30.34.2E.32.32.2E.30.32.2E.30.31 (hex)]
	30: firmwareVersion.0.10.83.108.97.118.101.32.66.73.79.83 (octet string) N/A [4E.2F.41 (hex)]
	31: firmwareVersion.0.11.77.97.115.116.101.114.32.66.73.79.83 (octet string) N/A [4E.2F.41 (hex)]
	32: firmwareVersion.0.13.77.97.105.110.98.111.97.114.100.32.70.82.85 (octet string) 01.03.0004 [30.31.2E.30.33.2E.30.30.30.34 (hex)]
	33: firmwareVersion.0.14.77.97.105.110.98.111.97.114.100.32.69.80.76.68 (octet string) 00.00.00.101 [30.30.2E.30.30.2E.30.30.2E.31.30.31 (hex)]
	34: firmwareVersion.2.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) 01.03.0001 [30.31.2E.30.33.2E.30.30.30.31 (hex)]
	35: firmwareVersion.2.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) N/A [4E.2F.41 (hex)]
	36: firmwareVersion.3.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) N/A [4E.2F.41 (hex)]
	37: firmwareVersion.3.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) N/A [4E.2F.41 (hex)]
	38: firmwareVersion.6.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) 01.03.0001 [30.31.2E.30.33.2E.30.30.30.31 (hex)]
	39: firmwareVersion.6.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) N/A [4E.2F.41 (hex)]
	40: fruNumber.0.4.66.79.79.84 (integer) 0
	41: fruNumber.0.9.83.108.97.118.101.32.66.77.67 (integer) 0
	42: fruNumber.0.10.77.97.115.116.101.114.32.66.77.67 (integer) 0
	43: fruNumber.0.10.83.108.97.118.101.32.66.73.79.83 (integer) 0
	44: fruNumber.0.11.77.97.115.116.101.114.32.66.73.79.83 (integer) 0
	45: fruNumber.0.13.77.97.105.110.98.111.97.114.100.32.70.82.85 (integer) 0
	46: fruNumber.0.14.77.97.105.110.98.111.97.114.100.32.69.80.76.68 (integer) 0
	47: fruNumber.2.11.83.117.98.67.97.114.100.32.70.82.85 (integer) 2
	48: fruNumber.2.12.83.117.98.67.97.114.100.32.69.80.76.68 (integer) 2
	49: fruNumber.3.11.83.117.98.67.97.114.100.32.70.82.85 (integer) 3
	50: fruNumber.3.12.83.117.98.67.97.114.100.32.69.80.76.68 (integer) 3
	51: fruNumber.6.11.83.117.98.67.97.114.100.32.70.82.85 (integer) 6
	52: fruNumber.6.12.83.117.98.67.97.114.100.32.69.80.76.68 (integer) 6
	53: firmwareBoard.0.4.66.79.79.84 (octet string) R5XG5_MB [52.35.58.47.35.5F.4D.42 (hex)]
	54: firmwareBoard.0.9.83.108.97.118.101.32.66.77.67 (octet string) R5XG5_MB [52.35.58.47.35.5F.4D.42 (hex)]
	55: firmwareBoard.0.10.77.97.115.116.101.114.32.66.77.67 (octet string) R5XG5_MB [52.35.58.47.35.5F.4D.42 (hex)]
	56: firmwareBoard.0.10.83.108.97.118.101.32.66.73.79.83 (octet string) R5XG5_MB [52.35.58.47.35.5F.4D.42 (hex)]
	57: firmwareBoard.0.11.77.97.115.116.101.114.32.66.73.79.83 (octet string) R5XG5_MB [52.35.58.47.35.5F.4D.42 (hex)]
	58: firmwareBoard.0.13.77.97.105.110.98.111.97.114.100.32.70.82.85 (octet string) R5XG5_MB [52.35.58.47.35.5F.4D.42 (hex)]
	59: firmwareBoard.0.14.77.97.105.110.98.111.97.114.100.32.69.80.76.68 (octet string) R5XG5_MB [52.35.58.47.35.5F.4D.42 (hex)]
	60: firmwareBoard.2.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) SWP65G50A [53.57.50.36.35.47.35.30.41 (hex)]
	61: firmwareBoard.2.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) SWP65G50A [53.57.50.36.35.47.35.30.41 (hex)]
	62: firmwareBoard.3.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) SUB CARD [53.55.42.20.43.41.52.44 (hex)]
	63: firmwareBoard.3.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) SUB CARD [53.55.42.20.43.41.52.44 (hex)]
	64: firmwareBoard.6.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) SBF25M [53.42.46.32.35.4D (hex)]
	65: firmwareBoard.6.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) SBF25M [53.42.46.32.35.4D (hex)]
	66: firmwareExtraInfo.0.4.66.79.79.84 (octet string) N/A [4E.2F.41 (hex)]
	67: firmwareExtraInfo.0.9.83.108.97.118.101.32.66.77.67 (octet string) N/A [4E.2F.41 (hex)]
	68: firmwareExtraInfo.0.10.77.97.115.116.101.114.32.66.77.67 (octet string) N/A [4E.2F.41 (hex)]
	69: firmwareExtraInfo.0.10.83.108.97.118.101.32.66.73.79.83 (octet string) N/A [4E.2F.41 (hex)]
	70: firmwareExtraInfo.0.11.77.97.115.116.101.114.32.66.73.79.83 (octet string) N/A [4E.2F.41 (hex)]
	71: firmwareExtraInfo.0.13.77.97.105.110.98.111.97.114.100.32.70.82.85 (octet string) N/A [4E.2F.41 (hex)]
	72: firmwareExtraInfo.0.14.77.97.105.110.98.111.97.114.100.32.69.80.76.68 (octet string) N/A [4E.2F.41 (hex)]
	73: firmwareExtraInfo.2.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) N/A [4E.2F.41 (hex)]
	74: firmwareExtraInfo.2.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) N/A [4E.2F.41 (hex)]
	75: firmwareExtraInfo.3.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) N/A [4E.2F.41 (hex)]
	76: firmwareExtraInfo.3.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) N/A [4E.2F.41 (hex)]
	77: firmwareExtraInfo.6.11.83.117.98.67.97.114.100.32.70.82.85 (octet string) N/A [4E.2F.41 (hex)]
	78: firmwareExtraInfo.6.12.83.117.98.67.97.114.100.32.69.80.76.68 (octet string) N/A [4E.2F.41 (hex)]
	***** SNMP QUERY FINISHED *****



## 4.12 networkProperty详细规格

### 4.12.1 功能说明

#### 4.12.1.1 父节点介绍

网口模式：

网口信息：包括每个网口的信息。如果是自动模式或固定模式，则只有一个网口信息。如果是独立模式，则有两个网口信息。

networkProperty 表节点的OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).networkProperty(17)

#### 4.12.1.2 子节点介绍

**标量表**

| 节点名称           | 节点 OID 实例                    | 描述                                             | 类型    | 权限       |
| ------------------ | -------------------------------- | ------------------------------------------------ | ------- | ---------- |
| networkMode        | 1.3.6.1.4.1.3902.2601.15.1.17.1  | Information about  network mode. <br/>1: auto(0) <br/>2: fixed(1) <br/>3: independent(2)  | INTEGER | read-only  |
| NCSIVlanID         | 1.3.6.1.4.1.3902.2601.15.1.17.11 | NCSI VLAN ID.                                    | INTEGER       | read-only  |
| NCSIVlanPriority   | 1.3.6.1.4.1.3902.2601.15.1.17.12 | NCSI VLAN Priority.                              | INTEGER       | read-only  |
| iSACVlanID         | 1.3.6.1.4.1.3902.2601.15.1.17.13 | iSAC VLAN ID.                                    | INTEGER       | read-only  |
| iSACVlanPriority   | 1.3.6.1.4.1.3902.2601.15.1.17.14 | iSAC VLAN Priority.                              | INTEGER       | read-only  |
| iSAClldpEnable     | 1.3.6.1.4.1.3902.2601.15.1.17.15 | iSAC lldp enabled status. <br/>1: true(1) <br/>2: false(0) | INTEGER       | read-only  |
| iSAClldpWorkMode   | 1.3.6.1.4.1.3902.2601.15.1.17.16 | iSAC lldp working mode.                          | DisplayString | read-only  |
**表量表**

节点networkDescriptionEntry是描述表节点网络的详细信息表（networkDescriptionTable）组成成分的。

其OID 为：

iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).networkProperty(17).networkDescriptionTable(50).networkDescriptionEntry(1)

    提示：x表示网络设备序号

| 节点名称        | 节点 OID 实例                           | 描述                                     | 类型          | 权限      |
| --------------- | --------------------------------------- | ---------------------------------------- | ------------- | --------- |
| ethIndex        | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.1.x  | Information about ethernet port number.  | INTEGER       | read-only |
| ethMACAddress   | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.2.x  | Information about MAC Address.           | DisplayString | read-only |
| ethNetworkProtocol    | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.3.x  | Information about network protocol. <br/>1:ipv4(1) <br/>2:ipv6(2) <br/>3:ipv4andipv6(3)     | INTEGER       | read-only |
| ethIPv4Source         | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.4.x  | Information about IPv4 Source. <br/>1:static(1) <br/>2:dhcp(2) | INTEGER       | read-only |
| ethIPv4Address        | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.5.x  | Information about IPv4 address.     | DisplayString | read-only |
| ethIPv4Netmask        | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.6.x  | Information about IPv4 netmask.     | DisplayString | read-only |
| ethIPv4DefaultGateway | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.7.x  | Information about IPv4 default gateway. | DisplayString | read-only |
| ethIPv6Source         | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.8.x  | Information about IPv6 source. <br/>1:static(1) <br/>2:dhcp(2)| INTEGER | read-only |
| ethIPv6Address        | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.9.x  | Information about IPv6 address.     | DisplayString | read-only |
| ethIPv6Prefix         | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.10.x | Information about IPv6 prefix.      | INTEGER | read-only |
| ethIPv6DefaultGateway | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.11.x  | Information about IPv6 default gateway.     | DisplayString       | read-only |
| ethIPv6LinkLocalAddress | 1.3.6.1.4.1.3902.2601.15.1.17.50.1.12.x  | Information about IPv6 link-local address.     | DisplayString       | read-only |

### 4.12.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.12.3 设置操作约束

​        不支持set操作

### 4.12.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: networkMode.0 (integer) independent(2)
    2: NCSIVlanID.0 (integer) 0
    3: NCSIVlanPriority.0 (integer) 0
    4: iSACVlanID.0 (integer) 0
    5: iSACVlanPriority.0 (integer) 0
    6: ethIndex.1 (integer) 1
    7: ethIndex.2 (integer) 2
    8: ethMACAddress.1 (octet string) 0E:68:FA:AB:D2:C0 [30.45.3A.36.38.3A.46.41.3A.41.42.3A.44.32.3A.43.30 (hex)]
    9: ethMACAddress.2 (octet string) 0E:68:FA:AB:D2:C1 [30.45.3A.36.38.3A.46.41.3A.41.42.3A.44.32.3A.43.31 (hex)]
    10: ethNetworkProtocol.1 (integer) ipv4andipv6(3)
    11: ethNetworkProtocol.2 (integer) ipv4andipv6(3)
    12: ethIPv4Source.1 (integer) static(1)
    13: ethIPv4Source.2 (integer) static(1)
    14: ethIPv4Address.1 (octet string) 192.168.5.7 [31.39.32.2E.31.36.38.2E.35.2E.37 (hex)]
    15: ethIPv4Address.2 (octet string) 192.168.114.7 [31.39.32.2E.31.36.38.2E.31.31.34.2E.37 (hex)]
    16: ethIPv4Netmask.1 (octet string) 255.255.255.0 [32.35.35.2E.32.35.35.2E.32.35.35.2E.30 (hex)]
    17: ethIPv4Netmask.2 (octet string) 255.255.255.0 [32.35.35.2E.32.35.35.2E.32.35.35.2E.30 (hex)]
    18: ethIPv4DefaultGateway.1 (octet string) 0.0.0.0 [30.2E.30.2E.30.2E.30 (hex)]
    19: ethIPv4DefaultGateway.2 (octet string) 0.0.0.0 [30.2E.30.2E.30.2E.30 (hex)]
    20: ethIPv6Source.1 (integer) static(1)
    21: ethIPv6Source.2 (integer) static(1)
    22: ethIPv6Address.1 (octet string) 2023::4 [32.30.32.33.3A.3A.34 (hex)]
    23: ethIPv6Address.2 (octet string) 2003::5 [32.30.30.33.3A.3A.35 (hex)]
    24: ethIPv6Prefix.1 (integer) 64
    25: ethIPv6Prefix.2 (integer) 64
    26: ethIPv6DefaultGateway.1 (octet string) 2023:: [32.30.32.33.3A.3A (hex)]
    27: ethIPv6DefaultGateway.2 (octet string) 2003:: [32.30.30.33.3A.3A (hex)]
    28: ethIPv6LinkLocalAddress.1 (octet string) fe80::c68:faff:feab:d2c0 [66.65.38.30.3A.3A.63.36.38.3A.66.61.66.66.3A.66.65.61.62.3A.64.32.63.30 (hex)]
    29: ethIPv6LinkLocalAddress.2 (octet string) fe80::c68:faff:feab:d2c1 [66.65.38.30.3A.3A.63.36.38.3A.66.61.66.66.3A.66.65.61.62.3A.64.32.63.31 (hex)]
    30: iSAClldpEnable.0 (integer) true(1)
    31: iSAClldpWorkMode.0 RX [52.58 (hex)]
    ***** SNMP QUERY FINISHED *****



## 4.13 sensorProperty详细规格

### 4.13.1 功能说明

#### 4.13.1.1 父节点介绍

    传感器信息包括：传感器名称、读取状态、高紧急门限、高严重门限、高轻微门限、低紧急门限、低严重门限、低轻微门限、传感器状态、传感器类型、传感器正滞后、传感器负滞后、传感器正滞后字符串、传感器负滞后字符串、传感器单位、传感器事件读取类型等。

sensorProperty表节点的OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).sensorProperty(18)

#### 4.13.1.2 子节点介绍

**表量表**

节点 sensorDescriptionEntry是描述表节点sensor的详细信息表（sensorDescriptionTable）组成成分的。

其OID 为：

iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).sensorProperty(18).sensorDescriptionTable(50).sensorDescriptionEntry(1)

    提示：x 表示传感器序号

| 节点名称                    | 节点 OID 实例                           | 描述                                                         | 类型          | 权限      |
| --------------------------- | --------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| sensorNumber                | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.1.x  | Information about sensor number.                             | INTEGER       | read-only |
| sensorName                  | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.2.x  | Information about sensor name.                               | DisplayString | read-only |
| sensorReading               | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.3.x  | Sensor current reading.                                      | DisplayString | read-only |
| sensorUpperNonRecoverable   | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.4.x  | Information about sensor upper nonrecoverable threshold.     | DisplayString | read-only |
| sensorUpperCritical         | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.5.x  | Information about sensor upper crtical threshold.            | DisplayString | read-only |
| sensorUpperMinor            | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.6.x  | Information about sensor upper minor threshold.              | DisplayString | read-only |
| sensorLowerNonRecoverable   | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.7.x  | Information about sensor lower nonrecoverable threshold.     | DisplayString | read-only |
| sensorLowerCritical         | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.8.x  | Information about sensor lower crtical threshold.            | DisplayString | read-only |
| sensorLowerMinor            | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.9.x  | Information about sensor lower minor threshold.              | DisplayString | read-only |
| sensorStatus                | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.10.x  | Information about sensor status.                            | DisplayString | read-only |
| sensorType                  | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.11.x  | Information about sensor type.<br/>1: temperature(1)<br/>2: voltage(2)<br/>3: current(3)<br/>4: fan(4)<br/>5: physicalSecurity(5)<br/>6: platSecurityViolationAttempt(6)<br/>7: processor(7)<br/>8: powerSupply(8)<br/>9: powerUnit(9)<br/>10: coolingDevice(10)<br/>11: otherUnitsBasedSensor(11)<br/>12: memory(12)<br/>13: driveSlot(13)<br/>14: postMemoryResize(14)<br/>15: systemFirmwareProgress(15)<br/>16: eventLoggingDisabled(16)<br/>17: watchdog1(17)<br/>18: systemEvent(18)<br/>19: criticalInterrupt(19)<br/>20: buttonOrSwitch(20)<br/>21: moduleOrBoard(21)<br/>22: microcontrollerOrCoprocessor(22)<br/>23: add-inCard(23)<br/>24: chassis(24)<br/>25: chipSet(25)<br/>26: otherFru(26)<br/>27: cableOrInterconnect(27)<br/>28: terminator(28)<br/>29: systemBootOrRestartInitiated(29)<br/>30: bootError(30)<br/>31: baseOsBootOrInstallationStatus(31)<br/>32: osStopOrShutdown(32)<br/>33: slotOrConnector(33)<br/>34: systemAcpiPowerState(34)<br/>35: watchdog2(35)<br/>36: platformAlert(36)<br/>37: entityPresence(37)<br/>38: monitorAsicOrIc(38)<br/>39: lan(39)<br/>40: managementSubsystemHealth(40)<br/>41: battery(41)<br/>42: sessionAudit(42)<br/>43: versionChange(43)<br/>44: fruState(44)<br/>45: leakageEvent(181)<br/> 46: smiTimeout(192)<br/>47: selfTest(193)<br/>48: hostEvent(194)<br/>49: biosStartup(195)<br/>50: sensorSelfEvent(196)<br/>51: pemVoltageFalling(197)<br/>52: boardPoweronFailure(198)<br/>53: hotSwapState(240)<br/>54: ipmbLinkStatus(241)                               | INTEGER       | read-only |
| sensorPositiveHysteresis    | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.12.x  | Positive-going Threshold Hysteresis Value. Set to 00h if sensor does not support positive-going threshold hysteresis.                                  | INTEGER       | read-only |                   |
| sensorNegativeHysteresis    | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.13.x  | Negative-going Threshold Hysteresis Value. Set to 00h if sensor does not support negative-going threshold hysteresis.                                  | INTEGER       | read-only |                   |
| sensorPositiveHysteresisString | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.14.x  | Positive-going Threshold Hysteresis Value. Set to 'na' if sensor does not support positive-going threshold hysteresis.                                 | DisplayString       | read-only |                   |
| sensorNegativeHysteresisString | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.15.x  | Negative-going Threshold Hysteresis Value. Set to 'na' if sensor does not support negative-going threshold hysteresis.                                 | DisplayString       | read-only |                   |
| sensorUnit                     | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.16.x  | Information about sensor unit.<br/>1: unspecified(0)<br/>2: degreesC(1)<br/>3: degreesF(2)<br/>4: degreesK(3)<br/>5: volts(4)<br/>6: amps(5)<br/>7: watts(6)<br/>8: joules(7)<br/>9: coulombs(8)<br/>10: va(9)<br/>11: nits(10)<br/>12: lumen(11)<br/>13: lux(12)<br/>14: candela(13)<br/>15: kPa(14)<br/>16: psi(15)<br/>17: newton(16)<br/>18: cfm(17)<br/>19: rpm(18)<br/>20: hz(19)<br/>21: microsecond(20)<br/>22: millisecond(21)<br/>23: second(22)<br/>24: minute(23)<br/>25: hour(24)<br/>26: day(25)<br/>27: week(26)<br/>28: mil(27)<br/>29: inches(28)<br/>30: feet(29)<br/>31: cuIn(30)<br/>32: cuFeet(31)<br/>33: mm(32)<br/>34: cm(33)<br/>35: m(34)<br/>36: cuCm(35)<br/>37: cuM(36)<br/>38: liters(37)<br/>39: fluidOunce(38)<br/>40: radians(39)<br/>41: steradians(40)<br/>42: revolutions(41)<br/>43: cycles(42)<br/>44: gravities(43)<br/>45: ounce(44)<br/>46: pound(45)<br/>47: ftlb(46)<br/>48: ozIn(47)<br/>49: gauss(48)<br/>50: gilberts(49)<br/>51: henry(50)<br/>52: millihenry(51)<br/>53: farad(52)<br/>54: microfarad(53)<br/>55: ohms(54)<br/>56: siemens(55)<br/>57: mole(56)<br/>58: becquerel(57)<br/>59: ppm(58)<br/>60: reserved(59)<br/>61: decibels(60)<br/>62: dbA(61)<br/>63: dbC(62)<br/>64: gray(63)<br/>65: sievert(64)<br/>66: colortempdegK(65)<br/>67: bit(66)<br/>68: kilobit(67)<br/>69: megabit(68)<br/>70: gigabit(69)<br/>71: byte(70)<br/>72: kilobyte(71)<br/>73: megabyte(72)<br/>74: gigabyte(73)<br/>75: word(74)<br/>76: dword(75)<br/>77: qword(76)<br/>78: line(77)<br/>79: hit(78)<br/>80: miss(79)<br/>81: retry(80)<br/>82: reset(81)<br/>83: overrunOverflow(82)<br/>84: underrun(83)<br/>85: collision(84)<br/>86: packets(85)<br/>87: messages(86)<br/>88: characters(87)<br/>89: error(88)<br/>90: correctableError(89)<br/>91: uncorrectableError(90)<br/>92: litersPerMinute(253)<br/>93: percent(254)                                  | INTEGER       | read-only |
| sensorEventReadingType         | 1.3.6.1.4.1.3902.2601.15.1.18.50.1.17.x  | Information about event reading type.<br/>1: unspecified(0)<br/>2: threshold(1)<br/>3: genericDiscrite1(2)<br/>4: genericDiscrite2(3)<br/>5: genericDiscrite3(4)<br/>6: genericDiscrite4(5)<br/>7: genericDiscrite5(6)<br/>8: genericDiscrite6(7)<br/>9: genericDiscrite7(8)<br/>10: genericDiscrite8(9)<br/>11: genericDiscrite9(10)<br/>12: genericDiscrite10(11)<br/>13: genericDiscrite11(12)<br/>14: sensorSpecific(111)<br/>15: oem1(112)<br/>16: oem2(113)<br/>17: oem3(114)<br/>18: oem4(115)<br/>19: oem5(116)<br/>20: oem6(117)<br/>21: oem7(118)<br/>22: oem8(119)<br/>23: oem9(120)<br/>24: oem10(121)<br/>25: oem11(122)<br/>26: oem12(123)<br/>27: oem13(124)<br/>28: oem14(125)<br/>29: oem15(126)<br/>30: oem16(127)                                | INTEGER       | read-only |

### 4.13.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.13.3 设置操作约束

​        不支持

### 4.13.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: sensorNumber.1 (integer) 1
    2: sensorName.1 (octet string) CPU_PROCHOT_01 [43.50.55.5F.50.52.4F.43.48.4F.54.5F.30.31 (hex)]
    3: sensorReading.1 (octet string) Reading/state unavailable [52.65.61.64.69.6E.67.2F.73.74.61.74.65.20.75.6E.61.76.61.69.6C.61.62.6C.65 (hex)]
    4: sensorUpperNonRecoverable.1 (octet string) -- [2D.2D (hex)]
    5: sensorUpperCritical.1 (octet string) -- [2D.2D (hex)]
    6: sensorUpperMinor.1 (octet string) -- [2D.2D (hex)]
    7: sensorLowerNonRecoverable.1 (octet string) -- [2D.2D (hex)]
    8: sensorLowerCritical.1 (octet string) -- [2D.2D (hex)]
    9: sensorLowerMinor.1 (octet string) -- [2D.2D (hex)]
    10: sensorStatus.1 (octet string) OK [4F.4B (hex)]
    11: sensorType.1 (integer) processor(7)
    12: sensorPositiveHysteresis.1 (integer) 3
    13: sensorNegativeHysteresis.1 (integer) 3
    14: sensorPositiveHysteresisString.1 (octet string) NA [4E.41 (hex)]
    15: sensorNegativeHysteresisString.1 (octet string) NA [4E.41 (hex)]
    16: sensorUnit.1 (integer) unspecified(0)
    17: sensorEventReadingType.1 (integer) threshold(1)
    ***** SNMP QUERY FINISHED *****



## 4.14 cpuProperty详细规格

### 4.14.1 功能说明

#### 4.14.1.1 父节点介绍

    cpu信息节点，包括：cpu整体健康状态、支持的最大数量、在位数量和在位信息，2个表量：cpu的详细信息表（包括编号Index、位置信息、设备名称、使能状态、健康状态、厂商、处理器类型、型号、序列号、TDP、外频、主频、最大频率、处理器ID、内核数、使能内核数、线程数、使能线程数、CPU L1 cache、CPU L2 cache、CPU L3 cache、部件号、架构、指令集、增强指令集）、cpu在位状态表（包括槽位号、在位状态）。

cpuProperty表节点的OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).cpuProperty(21) 

#### 4.14.1.2 子节点介绍

**标量表**

| 节点名称           | 节点 OID 实例                   | 描述                                                         | 类型    | 权限      |
| ------------------ | ------------------------------- | ------------------------------------------------------------ | ------- | --------- |
| cpuEntireStatus    | 1.3.6.1.4.1.3902.2601.15.1.21.1 | CPU entire health status. <br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER | read-only |
| cpuMaxSupportNum   | 1.3.6.1.4.1.3902.2601.15.1.21.2 | Information about max cpu number on board.<br /> 255 means unknown. | INTEGER | read-only |
| cpuTotalPresentNum | 1.3.6.1.4.1.3902.2601.15.1.21.3 | Information about present cpu number on board.               | INTEGER | read-only |



**表量表**

节点 cpuDescriptionEntry是描述表节点CPU的详细信息表（cpuDescriptionTable）组成成分的。

其OID 为：

iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).cpuProperty(21).cpuDescriptionTable(50).cpuDescriptionEntry(1)

    提示：x 表示cpu序号

| 节点名称                    | 节点 OID 实例                           | 描述                                                         | 类型          | 权限      |
| --------------------------- | --------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| cpuIndex                    | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.1.x  | Information about cpu index.                                 | INTEGER       | read-only |
| cpuLocation                 | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.2.x  | Information about cpu location.                              | INTEGER       | read-only |
| cpuDeviceName               | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.3.x  | Information about cpu name.                                  | DisplayString | read-only |
| cpuAvailabilityStatus       | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.4.x  | Information about cpu enable status. <br />1: unknown(1) <br />2: disabled(2) <br />3: backup(3) <br />4: active(4)| INTEGER       | read-only |
| cpuHealthStatus             | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.5.x  | CPU health status<br /><br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER       | read-only |
| cpuManufacturer             | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.6.x  | Information about cpu manufacturer.                          | DisplayString | read-only |
| cpuModel                    | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.7.x  | Information about cpu model type.                            | DisplayString | read-only |
| cpuType                     | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.8.x  | Information about cpu type.                                  | DisplayString | read-only |
| cpuSerialNumber             | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.9.x  | Information about cpu serial number.                         | DisplayString | read-only |
| cpuTdp                      | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.10.x | Information about cpu TDP number(unit: W).                   | INTEGER       | read-only |
| cpuExternalClock            | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.11.x | Information about cpu external Clock.                        | INTEGER       | read-only |
| cpuClockRate                | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.12.x | Information about cpu clock rate(unit: MHz).                 | INTEGER       | read-only |
| cpuMaxClockRate             | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.13.x | Information about cpu max clock rate(unit: MHz).             | INTEGER       | read-only |
| cpuProcessorID              | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.14.x | Information about cpu processor id.                          | DisplayString | read-only |
| cpuCoreCount                | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.15.x | Information about cpu total core number.                     | INTEGER       | read-only |
| cpuEnabledCoreCount         | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.16.x | Information about cpu enabled core number.                   | INTEGER       | read-only |
| cpuThreadCount              | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.17.x | Information about cpu thread number.                         | INTEGER       | read-only |
| cpuEnabledThreadCount       | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.18.x | Information about cpu enabled thread number.                 | INTEGER       | read-only |
| cpuL1CacheInKB              | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.19.x | Information about cpu L1 Cache(unit: KB).                    | INTEGER       | read-only |
| cpuL2CacheInKB              | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.20.x | Information about cpu L2 Cache(unit: KB).                    | INTEGER       | read-only |
| cpuL3CacheInKB              | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.21.x | Information about cpu L3 Cache(unit: KB).<br />0 means unknown.| INTEGER       | read-only |
| cpuPartNumber               | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.22.x | Information about cpu part number.                           | DisplayString | read-only |
| cpuArchitecture             | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.23.x | Information about cpu architecture.                          | DisplayString | read-only |
| cpuInstructionSet           | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.24.x | Information about cpu instructionset.                        | DisplayString | read-only |
| cpuInstructionSetExtensions | 1.3.6.1.4.1.3902.2601.15.1.21.50.1.25.x | Information about cpu instructionset extensions.             | DisplayString | read-only |


节点 cpuPresenceEntry是描述表节点CPU在位状态表（cpuPresenceTable）组成成分的。其OID 为： iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).cpuProperty(21).cpuPresenceTable(51).cpuPresenceEntry(1) 

    提示：x 表示cpu序号

| 节点名称          | 节点 OID 实例                          | 描述                 | 类型    | 权限      |
| ----------------- | -------------------------------------- | -------------------- | ------- | --------- |
| cpuLocationSlot   | 1.3.6.1.4.1.3902.2601.15.1.21.51.1.1.x | CPU location slot.   | INTEGER | read-only |
| cpuPresenceStatus | 1.3.6.1.4.1.3902.2601.15.1.21.51.1.2.x | CPU presence status.<br />1: disabled(1)<br />2: presence(2)<br />3: unknown(255) | INTEGER | read-only |



### 4.14.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.14.3 设置操作约束

​        不支持

### 4.14.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: cpuEntireStatus.0 (integer) ok(0)
    2: cpuMaxSupportNum.0 (integer) 2
    3: cpuTotalPresentNum.0 (integer) 0
    4: cpuLocationSlot.1 (integer) 1
    5: cpuLocationSlot.2 (integer) 2
    6: cpuPresenceStatus.1 (integer) disabled(1)
    7: cpuPresenceStatus.2 (integer) disabled(1)
    ***** SNMP QUERY FINISHED *****



## 4.15 memoryProperty详细规格

### 4.15.1 功能说明

#### 4.15.1.1 父节点介绍

    memory信息节点，包括3个标量：memory整体健康状态、服务器支持的最大数量、当前在位数量，2个表量：memory的详细信息表（包括编号Index、丝印编号、位置信息、设备名称、归属内存控制器Controller号、归属Channel号、归属DIMM号、Bank位置、使能状态、健康状态、容量、厂商、序列号、部件号、资产标签、DDR类型、插槽类型FormFactor、DIMM类型、Rank数、EccType、主频、配置频率、数据带宽、总带宽、最小电压、最大电压、配置电压）、memory在位状态表（包括槽位号、在位状态）。

memoryProperty表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).memoryProperty(22) 

#### 4.15.1.2 子节点介绍

**标量表**

| 节点名称              | 节点 OID 实例                   | 描述                                                         | 类型    | 权限      |
| --------------------- | ------------------------------- | ------------------------------------------------------------ | ------- | --------- |
| memoryEntireStatus    | 1.3.6.1.4.1.3902.2601.15.1.22.1 | Memory entire health status. <br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER | read-only |
| memoryMaxSupportNum   | 1.3.6.1.4.1.3902.2601.15.1.22.2 | Information about max memory number on board.<br />255 means unknown.  | INTEGER | read-only |
| memoryTotalPresentNum | 1.3.6.1.4.1.3902.2601.15.1.22.3 | Information about present memory number on board.            | INTEGER | read-only |



**表量表**

节点memoryDescriptionEntry是描述表节点memory详细信息表（memoryDescriptionTable）组成成分的。

其OID 为： iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).memoryProperty(22).memoryDescriptionTable(50).memoryDescriptionEntry(1) 

    提示：x 表示memory序号

| 节点名称                  | 节点 OID 实例                           | 描述                                                         | 类型          | 权限      |
| ------------------------- | --------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| memoryIndex               | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.1.x  | Information about memory index number.                       | INTEGER       | read-only |
| memoryDimmNumber          | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.2.x  | Information about memory silk number.                        | INTEGER       | read-only |
| memoryLocation            | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.3.x  | Information about memory silk type.                          | DisplayString | read-only |
| memoryCpuDeviceName       | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.4.x  | Information about memory cpu belong.                         | DisplayString | read-only |
| memoryController          | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.5.x  | Information about memory controller.                         | INTEGER       | read-only |
| memoryChannel             | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.6.x  | Information about memory channel.                            | INTEGER       | read-only |
| memoryDimm                | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.7.x  | Information about memory dimm.                               | INTEGER       | read-only |
| memoryBank                | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.8.x  | Information about memory bank.                               | DisplayString | read-only |
| memoryAvailabilityStatus  | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.9.x  | Information about memory enable status.<br />1: unknown(1) <br />2: disabled(2) <br />3: backup(3) <br />4: active(4) | INTEGER       | read-only |
| memoryHealthStatus        | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.10.x | Memory health status.<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER       | read-only |
| memorySizeInGB            | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.11.x | Information about memory capacity.                           | INTEGER       | read-only |
| memoryManufacturer        | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.12.x | Information about memory manufacture.                        | DisplayString | read-only |
| memorySerialNumber        | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.13.x | Information about memory serial number.                      | DisplayString | read-only |
| memoryPartNumber          | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.14.x | Information about memory part number.                        | DisplayString | read-only |
| memoryAssetTag            | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.15.x | Information about memory asset tag.                          | DisplayString | read-only |
| memoryType                | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.16.x | Information about DIMM type.                                 | DisplayString | read-only |
| memoryFormFactor          | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.17.x | Information about memory form factor.                        | DisplayString | read-only |
| memoryBModuleType         | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.18.x | Information about memory bmodule type.                       | DisplayString | read-only |
| memoryRank                | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.19.x | Information about memory memory rank.                        | INTEGER       | read-only |
| memoryEccType             | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.20.x | Information about memory ecc type.                           | DisplayString | read-only |
| memoryFrequency           | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.21.x | Information about memory frequency(unit: MHz).               | INTEGER       | read-only |
| memoryConfiguredFrequency | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.22.x | Information about memory configured frequency(unit: MHz).    | INTEGER       | read-only |
| memoryDataWidthBits       | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.23.x | Information about memory data width.                         | INTEGER       | read-only |
| memoryTotalWidthBits      | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.24.x | Information about memory total width.                        | INTEGER       | read-only |
| memoryMinimumVoltage      | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.25.x | Information about DDR minimum voltage(unit: V).              | DisplayString | read-only |
| memoryMaximumVoltage      | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.26.x | Information about DDR maximum voltage(unit: V).              | DisplayString | read-only |
| memoryConfiguredVoltage   | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.27.x | Information about DDR current voltage(unit: V).              | DisplayString | read-only |
| memoryTemperature         | 1.3.6.1.4.1.3902.2601.15.1.22.50.1.28.x | Information about current temperature(unit: Celsius).<br /> 255 means unknown.     | INTEGER       | read-only |

节点 memoryPresenceEntry是描述表节点memory在位状态表（ memoryPresenceTable）组成成分的。

其OID 为： iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).memoryProperty(22).memoryPresenceTable(51).memoryPresenceEntry(1) 

    提示：x 表示memory序号

| 节点名称             | 节点 OID 实例                          | 描述                    | 类型    | 权限      |
| -------------------- | -------------------------------------- | ----------------------- | ------- | --------- |
| memoryLocationSlot   | 1.3.6.1.4.1.3902.2601.15.1.22.51.1.1.x | Memory location.        | INTEGER | read-only |
| memoryPresenceStatus | 1.3.6.1.4.1.3902.2601.15.1.22.51.1.2.x | Memory presence status.<br />1: absence(1)<br />2: presence(2)<br />3: unknown(255) | INTEGER | read-only |

### 4.15.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.15.3 设置操作约束

​        不支持

### 4.15.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: memoryEntireStatus.0 (integer) ok(0)
    2: memoryMaxSupportNum.0 (integer) 32
    3: memoryTotalPresentNum.0 (integer) 0
    4: memoryLocationSlot.1 (integer) 1
    5: memoryLocationSlot.2 (integer) 2
    6: memoryLocationSlot.3 (integer) 3
    7: memoryLocationSlot.4 (integer) 4
    8: memoryLocationSlot.5 (integer) 5
    9: memoryLocationSlot.6 (integer) 6
    10: memoryLocationSlot.7 (integer) 7
    11: memoryLocationSlot.8 (integer) 8
    12: memoryLocationSlot.9 (integer) 9
    13: memoryLocationSlot.10 (integer) 10
    14: memoryLocationSlot.11 (integer) 11
    15: memoryLocationSlot.12 (integer) 12
    16: memoryLocationSlot.13 (integer) 13
    17: memoryLocationSlot.14 (integer) 14
    18: memoryLocationSlot.15 (integer) 15
    19: memoryLocationSlot.16 (integer) 16
    20: memoryLocationSlot.17 (integer) 17
    21: memoryLocationSlot.18 (integer) 18
    22: memoryLocationSlot.19 (integer) 19
    23: memoryLocationSlot.20 (integer) 20
    24: memoryLocationSlot.21 (integer) 21
    25: memoryLocationSlot.22 (integer) 22
    26: memoryLocationSlot.23 (integer) 23
    27: memoryLocationSlot.24 (integer) 24
    28: memoryLocationSlot.25 (integer) 25
    29: memoryLocationSlot.26 (integer) 26
    30: memoryLocationSlot.27 (integer) 27
    31: memoryLocationSlot.28 (integer) 28
    32: memoryLocationSlot.29 (integer) 29
    33: memoryLocationSlot.30 (integer) 30
    34: memoryLocationSlot.31 (integer) 31
    35: memoryLocationSlot.32 (integer) 32
    36: memoryPresenceStatus.1 (integer) absence(1)
    37: memoryPresenceStatus.2 (integer) absence(1)
    38: memoryPresenceStatus.3 (integer) absence(1)
    39: memoryPresenceStatus.4 (integer) absence(1)
    40: memoryPresenceStatus.5 (integer) absence(1)
    41: memoryPresenceStatus.6 (integer) absence(1)
    42: memoryPresenceStatus.7 (integer) absence(1)
    43: memoryPresenceStatus.8 (integer) absence(1)
    44: memoryPresenceStatus.9 (integer) absence(1)
    45: memoryPresenceStatus.10 (integer) absence(1)
    46: memoryPresenceStatus.11 (integer) absence(1)
    47: memoryPresenceStatus.12 (integer) absence(1)
    48: memoryPresenceStatus.13 (integer) absence(1)
    49: memoryPresenceStatus.14 (integer) absence(1)
    50: memoryPresenceStatus.15 (integer) absence(1)
    51: memoryPresenceStatus.16 (integer) absence(1)
    52: memoryPresenceStatus.17 (integer) absence(1)
    53: memoryPresenceStatus.18 (integer) absence(1)
    54: memoryPresenceStatus.19 (integer) absence(1)
    55: memoryPresenceStatus.20 (integer) absence(1)
    56: memoryPresenceStatus.21 (integer) absence(1)
    57: memoryPresenceStatus.22 (integer) absence(1)
    58: memoryPresenceStatus.23 (integer) absence(1)
    59: memoryPresenceStatus.24 (integer) absence(1)
    60: memoryPresenceStatus.25 (integer) absence(1)
    61: memoryPresenceStatus.26 (integer) absence(1)
    62: memoryPresenceStatus.27 (integer) absence(1)
    63: memoryPresenceStatus.28 (integer) absence(1)
    64: memoryPresenceStatus.29 (integer) absence(1)
    65: memoryPresenceStatus.30 (integer) absence(1)
    66: memoryPresenceStatus.31 (integer) absence(1)
    67: memoryPresenceStatus.32 (integer) absence(1)
    ***** SNMP QUERY FINISHED *****



## 4.16  fru详细规格

### 4.16.1 功能说明

#### 4.16.1.1 父节点介绍

fru的信息节点，包括1个表量表，含：fru编号，chassis类型，chassis部件号，chassis序列号，单板生产厂商，单板产品名，单板序列号，单板部件号，单板生产日期，产品生产厂商，产品产品名，产品部件号，产品版本号，产品序列号，产品资产标签。

fru表节点的OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).fruInfo(23)

#### 4.16.1.2 子节点介绍

**表量表**

节点fruDescriptionEntry是描述表节点fru的详细信息表（fruCardDescriptionTable）组成成分的。

其OID 为：1.3.6.1.4.1.3902.2601.15.1.23.50 iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).fru(23).fruDescriptionEntry(50). 

    提示：x表示网卡编号

| 节点名称               | 节点 OID 实例                         | 描述                                                         | 类型          | 权限      |
| ---------------------- | ------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| fruId                  | 1.3.6.1.4.1.3902.2601.15.1.23.50.1.1.x  | Information about FRU id.                                  | INTEGER       | read-only |
| fruChassisType         | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.2.x  | FRU chassis type.                                          | DisplayString | read-only |
| fruChassisPartNumber   | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.3.x  | FRU chassis part number                                    | DisplayString | read-only |
| fruChassisSerialNumber | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.4.x  | FRU chassis serial number                                  | DisplayString | read-only |
| fruBoardMfgDate        | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.5.x  | FRU borad manufacturing date.                              | DisplayString | read-only |
| fruBoardManufacturer   | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.6.x  | FRU board manufacturer.                                    | DisplayString | read-only |
| fruBoardProductName    | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.7.x  | FRU board product name.                                    | DisplayString | read-only |
| fruBoardSerialNumber   | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.8.x  | FRU board serial number.                                   | DisplayString | read-only |
| fruBoardPartNumber     | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.9.x  | FRU board part number.                                     | DisplayString | read-only |
| fruProductManufacturer | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.10.x | FRU product maufacturer.                                   | DisplayString | read-only |
| fruProductName         | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.11.x | FRU product name.                                          | DisplayString | read-only |
| fruProductPartNumber   | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.12.x | FRU product part number.                                   | DisplayString | read-only |
| fruProductVersion      | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.13.x | FRU product version .                                      | DisplayString | read-only |
| fruProductSerialNumber | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.14.x | FRU product serial number.                                 | DisplayString | read-only |
| fruProductAssetTag     | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.15.x | FRU product asset tag.                                     | DisplayString | read-only |

### 4.16.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.16.3 设置操作约束

​        不支持

### 4.16.4 使用示例
	***** SNMP QUERY STARTED *****
	1: fruId.0 (integer) 0
	2: fruId.2 (integer) 2
	3: fruId.6 (integer) 6
	4: fruId.17 (integer) 17
	5: fruChassisType.0 (octet string) N/A [4E.2F.41 (hex)]
	6: fruChassisType.2 (octet string) N/A [4E.2F.41 (hex)]
	7: fruChassisType.6 (octet string) N/A [4E.2F.41 (hex)]
	8: fruChassisType.17 (octet string) N/A [4E.2F.41 (hex)]
	9: fruChassisPartNumber.0 (octet string) N/A [4E.2F.41 (hex)]
	10: fruChassisPartNumber.2 (octet string) N/A [4E.2F.41 (hex)]
	11: fruChassisPartNumber.6 (octet string) N/A [4E.2F.41 (hex)]
	12: fruChassisPartNumber.17 (octet string) N/A [4E.2F.41 (hex)]
	13: fruChassisSerialNumber.0 (octet string) N/A [4E.2F.41 (hex)]
	14: fruChassisSerialNumber.2 (octet string) N/A [4E.2F.41 (hex)]
	15: fruChassisSerialNumber.6 (octet string) N/A [4E.2F.41 (hex)]
	16: fruChassisSerialNumber.17 (octet string) N/A [4E.2F.41 (hex)]
	17: fruBoardMfgDate.0 (octet string) 2022-04-03 00:52:00 [32.30.32.32.2D.30.34.2D.30.33.20.30.30.3A.35.32.3A.30.30 (hex)]
	18: fruBoardMfgDate.2 (octet string) 2022-09-01 00:02:00 [32.30.32.32.2D.30.39.2D.30.31.20.30.30.3A.30.32.3A.30.30 (hex)]
	19: fruBoardMfgDate.6 (octet string) 2022-07-15 19:03:00 [32.30.32.32.2D.30.37.2D.31.35.20.31.39.3A.30.33.3A.30.30 (hex)]
	20: fruBoardMfgDate.17 (octet string) N/A [4E.2F.41 (hex)]
	21: fruBoardManufacturer.0 (octet string) ZTE [5A.54.45 (hex)]
	22: fruBoardManufacturer.2 (octet string) ZTE [5A.54.45 (hex)]
	23: fruBoardManufacturer.6 (octet string) ZTE [5A.54.45 (hex)]
	24: fruBoardManufacturer.17 (octet string) N/A [4E.2F.41 (hex)]
	25: fruBoardProductName.0 (octet string) R5XG5_MB [52.35.58.47.35.5F.4D.42 (hex)]
	26: fruBoardProductName.2 (octet string) SWP65G50A [53.57.50.36.35.47.35.30.41 (hex)]
	27: fruBoardProductName.6 (octet string) SBF25M [53.42.46.32.35.4D (hex)]
	28: fruBoardProductName.17 (octet string) N/A [4E.2F.41 (hex)]
	29: fruBoardSerialNumber.0 (octet string) N/A [4E.2F.41 (hex)]
	30: fruBoardSerialNumber.2 (octet string) N/A [4E.2F.41 (hex)]
	31: fruBoardSerialNumber.6 (octet string) N/A [4E.2F.41 (hex)]
	32: fruBoardSerialNumber.17 (octet string) N/A [4E.2F.41 (hex)]
	33: fruBoardPartNumber.0 (octet string) 21080000 [32.31.30.38.30.30.30.30 (hex)]
	34: fruBoardPartNumber.2 (octet string) 21120000 [32.31.31.32.30.30.30.30 (hex)]
	35: fruBoardPartNumber.6 (octet string) 19010200 [31.39.30.31.30.32.30.30 (hex)]
	36: fruBoardPartNumber.17 (octet string) N/A [4E.2F.41 (hex)]
	37: fruProductManufacturer.0 (octet string) ZTE [5A.54.45 (hex)]
	38: fruProductManufacturer.2 (octet string) ZTE [5A.54.45 (hex)]
	39: fruProductManufacturer.6 (octet string) ZTE [5A.54.45 (hex)]
	40: fruProductManufacturer.17 (octet string) Great Wall [47.72.65.61.74.20.57.61.6C.6C (hex)]
	41: fruProductName.0 (octet string) N/A [4E.2F.41 (hex)]
	42: fruProductName.2 (octet string) N/A [4E.2F.41 (hex)]
	43: fruProductName.6 (octet string) SBF25MA [53.42.46.32.35.4D.41 (hex)]
	44: fruProductName.17 (octet string) CRPS1200D [43.52.50.53.31.32.30.30.44 (hex)]
	45: fruProductPartNumber.0 (octet string) N/A [4E.2F.41 (hex)]
	46: fruProductPartNumber.2 (octet string) N/A [4E.2F.41 (hex)]
	47: fruProductPartNumber.6 (octet string) N/A [4E.2F.41 (hex)]
	48: fruProductPartNumber.17 (octet string) N/A [4E.2F.41 (hex)]
	49: fruProductVersion.0 (octet string) N/A [4E.2F.41 (hex)]
	50: fruProductVersion.2 (octet string) N/A [4E.2F.41 (hex)]
	51: fruProductVersion.6 (octet string) N/A [4E.2F.41 (hex)]
	52: fruProductVersion.17 (octet string) DC:1.01 PFC:1.00 [44.43.3A.31.2E.30.31.20.50.46.43.3A.31.2E.30.30 (hex)]
	53: fruProductSerialNumber.0 (octet string) N/A [4E.2F.41 (hex)]
	54: fruProductSerialNumber.2 (octet string) N/A [4E.2F.41 (hex)]
	55: fruProductSerialNumber.6 (octet string) N/A [4E.2F.41 (hex)]
	56: fruProductSerialNumber.17 (octet string) 22M010020464 [32.32.4D.30.31.30.30.32.30.34.36.34 (hex)]
	57: fruProductAssetTag.0 (octet string) N/A [4E.2F.41 (hex)]
	58: fruProductAssetTag.2 (octet string) N/A [4E.2F.41 (hex)]
	59: fruProductAssetTag.6 (octet string) N/A [4E.2F.41 (hex)]
	60: fruProductAssetTag.17 (octet string) N/A [4E.2F.41 (hex)]
	***** SNMP QUERY FINISHED *****



## 4.17   pCIeDeviceProperty详细规格

### 4.17.1 功能说明

#### 4.17.1.1 父节点介绍

    pCIeDevice信息节点，包括2个标量：pCIeDevice整体健康状态、服务器支持的最大数量（未实现）；1个表量：pCIeDevice的详细信息表（包括编号Index、槽位号、位置类型、Vendor ID、Device ID、Sub Vendor ID、Sub System ID、Bus Number、Device Number、Function Number、归属CPU号、使能状态、健康状态、芯片型号、厂商、设备描述、设备类型、ClassCode、固件版本、序列号、最大带宽、实际带宽、设备内存、额定功耗、实时功耗）。

pCIeDeviceProperty表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).pCIeDeviceProperty(24)

#### 4.17.1.2 子节点介绍

**标量表**

| 节点名称               | 节点 OID 实例                   | 描述                                                         | 类型    | 权限      |
| ---------------------- | ------------------------------- | ------------------------------------------------------------ | ------- | --------- |
| pCIeDeviceEntireStatus | 1.3.6.1.4.1.3902.2601.15.1.24.1 | Pcie device entire health status. <br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER | read-only |



**表量表**

节点pCIeDeviceDescriptionEntry是描述表节点物理盘的详细信息表（pCIeDeviceDescriptionTable）组成成分的。

其OID 为： iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).pCIeDeviceProperty(24).pCIeDeviceDescriptionTable(50).pCIeDeviceDescriptionEntry(1) 

    提示：x 表示pCIeDevice序号

| 节点名称                     | 节点 OID 实例                           | 描述                                                         | 类型          | 权限      |
| ---------------------------- | --------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| pCIeDeviceIndex              | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.1.x  | Information about pcie device index number.                  | INTEGER       | read-only |
| pCIeDeviceSlotNumber         | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.2.x  | Information about pcie device slot number.                   | INTEGER       | read-only |
| pCIeDeviceLocationType       | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.3.x  | Pcie device location type.<br />1: embedded(0) <br />2: pcie(1) <br />3: ocp(2) | INTEGER       | read-only |
| pCIeDeviceVendorID           | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.4.x  | Information about pcie device vendor Id.                     | DisplayString | read-only |
| pCIeDeviceDeviceID           | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.5.x  | Information about pcie device device Id.                     | DisplayString | read-only |
| pCIeDeviceSubVendorID        | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.6.x  | Information about pcie device sub-vendor Id.                 | DisplayString | read-only |
| pCIeDeviceSubSystemID        | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.7.x  | Information about pcie device sub-system Id.                 | DisplayString | read-only |
| pCIeDeviceBusNum             | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.8.x  | Information about pcie device bus number.                    | DisplayString | read-only |
| pCIeDeviceDeviceNum          | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.9.x  | Information about pcie device device number.                 | DisplayString | read-only |
| pCIeDeviceFunctionNum        | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.10.x | Information about pcie device function number.               | DisplayString | read-only |
| pCIeDeviceResourceOwnership  | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.11.x | Information about pcie device belonging cpu number.          | DisplayString | read-only |
| pCIeDeviceAvailabilityStatus | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.12.x | Information about pcie enable status.<br />1: unknown(1)<br />2: disabled(2)<br />3: backup(3)<br />4: active(4)  | INTEGER       | read-only |
| pCIeDeviceHealthStatus       | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.13.x | Pcie device health status.<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255)| INTEGER       | read-only |
| pCIeDeviceModel              | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.14.x | Information about pcie device model.                         | DisplayString | read-only |
| pCIeDeviceManufacturer       | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.15.x | Information about pcie device manufacturer.                  | DisplayString | read-only |
| pCIeDeviceDescription        | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.16.x | Information about pcie device description.                   | DisplayString | read-only |
| pCIeDeviceType               | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.17.x | Information about pcie device type.                          | DisplayString | read-only |
| pCIeDeviceClassCode          | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.18.x | PCIE class code<br/>1: storage(1) <br/>2: network <br/>3：display(3) <br/>4: multimedia(4) <br/>5: memoryController(5) <br/>6: bridge <br/>7: simpleCommunication(7) <br/>8: basicSystemPeripheral(8) <br/>9: input(9) <br/>10: castle(10)<br/>11: processor(11) <br/>12: serialBusController(12)<br/>13: wirelessController(13) <br/>14: integratedIOController(14) <br/>15: satelliteCommunicationController(15) <br/>16: encryptionAndDecryptionControlleR(16) <br/>17: dataAcquisitionAndSignalProcessingController(17) <br/>18: processingAccelerators(18)<br/>19: unsupported(255) <br/>value between 19 and 254 are reserved. | INTEGER       | read-only |
| pCIeDeviceFirmwareVersion    | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.19.x | Information about pcie device firmware version.              | DisplayString | read-only |
| pCIeDeviceSerialNumber       | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.20.x | Information about pcie device serial number.                 | DisplayString | read-only |
| pCIeDeviceLinkWidthAbility   | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.21.x | Information about pcie device link width ability.<br/>0 means unknown. | INTEGER       | read-only |
| pCIeDeviceLinkWidth          | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.22.x | Information about pcie device link width.<br/>0 means unknown. | INTEGER       | read-only |
| pCIeDeviceMemorySize         | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.23.x | Information about pcie device total memory size(unit: MB).<br/>0 means unknown. | INTEGER       | read-only |
| pCIeDeviceRatedPower         | 1.3.6.1.4.1.3902.2601.15.1.24.50.1.24.x | Information about pcie device rated power(unit: W).<br/>0 means unknown. | INTEGER       | read-only |
| pCIeDeviceCurrentPower       | 1.3.6.1.4.1.3902.2601.15.1.30.24.1.25.x | Information about pcie device current power(unit: mW).<br/>0 means unknown. | INTEGER       | read-only |
| pCIeDeviceLocator            | 1.3.6.1.4.1.3902.2601.15.1.30.24.1.26.x | Information about Location. | DisplayString       | read-only |

### 4.17.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.17.3 设置操作约束

​        不支持

### 4.17.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: pCIeDeviceEntireStatus.0 (integer) ok(0)
    2: pCIeDeviceIndex.1 (integer) 1
    3: pCIeDeviceSlotNumber.1 (integer) 64
    4: pCIeDeviceLocationType.1 (integer) ocp(2)
    5: pCIeDeviceVendorID.1 (octet string) 0x8086 [30.78.38.30.38.36 (hex)]
    6: pCIeDeviceDeviceID.1 (octet string) 0x159b [30.78.31.35.39.62 (hex)]
    7: pCIeDeviceSubVendorID.1 (octet string) 0x8086 [30.78.38.30.38.36 (hex)]
    8: pCIeDeviceSubSystemID.1 (octet string) 0x0005 [30.78.30.30.30.35 (hex)]
    9: pCIeDeviceBusNum.1 (octet string) N/A [4E.2F.41 (hex)]
    10: pCIeDeviceDeviceNum.1 (octet string) N/A [4E.2F.41 (hex)]
    11: pCIeDeviceFunctionNum.1 (octet string) N/A [4E.2F.41 (hex)]
    12: pCIeDeviceResourceOwnership.1 (octet string) N/A [4E.2F.41 (hex)]
    13: pCIeDeviceAvailabilityStatus.1 (integer) active(4)
    14: pCIeDeviceHealthStatus.1 (integer) ok(0)
    15: pCIeDeviceModel.1 (octet string) E810 [45.38.31.30 (hex)]
    16: pCIeDeviceManufacturer.1 (octet string) Intel [49.6E.74.65.6C (hex)]
    17: pCIeDeviceDescription.1 (octet string) E810-XXVDA2 [45.38.31.30.2D.58.58.56.44.41.32 (hex)]
    18: pCIeDeviceType.1 (octet string) NIC [4E.49.43 (hex)]
    19: pCIeDeviceClassCode.1 (integer) network(2)
    20: pCIeDeviceFirmwareVersion.1 (octet string) 2.3 [32.2E.33 (hex)]
    21: pCIeDeviceSerialNumber.1 (octet string) N/A [4E.2F.41 (hex)]
    22: pCIeDeviceLinkWidthAbility.1 (integer) unknown(0)
    23: pCIeDeviceLinkWidth.1 (integer) unknown(0)
    24: pCIeDeviceMemorySize.1 (integer) unknown(0)
    25: pCIeDeviceRatedPower.1 (integer) unknown(0)
    26: pCIeDeviceCurrentPower.1 (integer) unknown(0)
    ***** SNMP QUERY FINISHED *****



## 4.18  netCardProperty详细规格

### 4.18.1 功能说明

#### 4.18.1.1 父节点介绍

网卡的信息节点，包括3个表量：网卡的详细信息表（包括网卡编号、网卡物理位置信息、网卡槽位号、网卡设备名称、网卡健康状态、网卡名称、网卡厂商名称、网卡芯片名称、网卡芯片厂商名称、网卡最大端口数量、网卡端口类型、网卡model、网卡温度、网卡历史最大温度、网卡firmware版本、网卡序列号、网卡驱动名称、网卡BDF信息、网卡部件号等信息）；网卡的网口详细信息表（包括网口编号、网口丝印编号、网口类型、网口链接状态、网口标称速率、网口当前速率、网口mac地址、网口协商模式、网口双工模式、网口LLDP模式、网口BDF、网口所属网卡设备名称）；网卡的内存信息表（包括网卡编号、网卡内存编号、网卡内存类型、网卡内存模式、网卡内存容量、网卡内存状态）。

netCardProperty表节点的OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).netCardProperty (26)

#### 4.18.1.2 子节点介绍

**表量表**

节点netCardDescriptionEntry是描述表节点网卡的详细信息表（netCardDescriptionTable）组成成分的。

其OID 为：1.3.6.1.4.1.3902.2601.15.1.26.50.1  iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).netCardProperty(26).netCardDescriptionTable(50).netCardDescriptionEntry(1) 

    提示：x表示网卡编号

| 节点名称                     | 节点 OID 实例                           | 描述                                       | 类型          | 权限      |
| ---------------------------- | --------------------------------------- | ------------------------------------------ | ------------- | --------- |
| netCardIndex                 | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.1.x  | Net card index.                            | INTEGER       | read-only |
| netCardLocationType          | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.2.x  | Net card location type define as: <br/>1: embedded(0) <br/>2: pcie(1) <br/>3: ocp(2) <br/>4: unknown(255) | INTEGER       | read-only |
| netCardLocationSlot          | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.3.x  | Net card location slot.                    | INTEGER       | read-only |
| netCardDevicename            | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.4.x  | Net card slot info string: location type + location slot.Such as (PcieCard 5).   | DisplayString | read-only |
| netCardHealthStatus          | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.5.x  | Net card health status define as:<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER       | read-only |
| netCardNICName               | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.6.x  | Net card nic name.                         | DisplayString | read-only |
| netCardNICManufacturer       | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.7.x  | Net card nic manufacturer name.            | DisplayString | read-only |
| netCardChipModel             | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.8.x  | Net card chip name.                        | DisplayString | read-only |
| netCardChipManufacturer      | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.9.x  | Net card chip manufacturer name.           | DisplayString | read-only |
| netCardMaxPortNumber         | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.10.x | Net card max port number.                  | INTEGER       | read-only |
| netCardPortsType             | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.11.x | Ports on net card type define as:<br/>1: copper(0) <br/>2: fiber(1) <br/>3: serdes(2) <br/>4: copperfiber(3) <br/>5: fiberserdes(4) <br/>6: unknown(255) | INTEGER       | read-only |
| netCardNICModel              | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.12.x | Net card nic model.Such as (2\*10GE+2\*25GE). | DisplayString | read-only |
| netCardTemperature           | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.13.x | Net card temperature. 255 means netcard is not support to get temperature.  | INTEGER       | read-only |
| netCardHistoryMaxTemperature | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.14.x | Net card history max temperature. 255 means netcard is not support to get temperature.  | INTEGER       | read-only |
| netCardFirmwareVersion       | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.15.x | Net card firmware version.                 | DisplayString | read-only |
| netCardSerialNumber          | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.16.x | Net card serial number.                    | DisplayString | read-only |
| netCardDriverName            | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.17.x | Net card driver name.                      | DisplayString | read-only |
| netCardRootBDF               | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.18.x | Net card root bdf.(same as first port bdf) | DisplayString | read-only |
| netCardPartNumber            | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.19.x | Net card part number.                      | DisplayString | read-only |
| netCardFpgaStatus            | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.20.x | smart card fpga health status as: <br/>1: normal(0) <br/>2: abnormal(1) <br/>3: unknown(255) | INTEGER | read-only |
| netCardFpgaTempStatus        | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.21.x | smart card fpga temp health status as: <br/>1: normal(0) <br/>2: abnormal(1) <br/>3: unknown(255) | INTEGER | read-only |
| netCardDeviceId              | 1.3.6.1.4.1.3902.2601.15.1.26.50.1.22.x | Net card device ID.                                          | INTEGER | read-only |

节点 netPortDescriptionEntry是描述表节点网卡的网口的详细信息表（netPortDescriptionTable）组成成分的。

其OID 为：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1). netCardProperty(26). netPortDescriptionTable(51). netPortDescriptionEntry(1) 

    提示：x表示网卡编号，y表示网口编号

| 节点名称              | 节点 OID 实例                             | 描述                                                         | 类型          | 权限      |
| --------------------- | ----------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| netPortNICIndex       | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.1.x.y  | Net port owner net card index.                               | INTEGER       | read-only |
| netPortLocation       | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.2.x.y  | Net card port location num, depends on silk.                 | INTEGER       | read-only |
| netPortType           | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.3.x.y  | Net port type define as:<br/>1: copper(0) <br/>2: fiber(1) <br/>3: serdes(2) <br/>4: unknown(255) | INTEGER       | read-only |
| netPortLinkStatus     | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.4.x.y  | Net port link status define as:<br/>1: linkdown(0) <br/>2: linkup(1) <br/>3: unknown(255) | INTEGER       | read-only |
| netPortCapableSpeed   | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.5.x.y  | Net port capable speed define as:<br/>1: speed10M(0) <br/>2: speed100M(1) <br/>3: speed1G(2) <br/>4: speed2500M(3) <br/>5: speed5G(4) <br/>6: speed10G(5) <br/>7: speed25G(6) <br/>8: speed40G(7) <br/>9: speed50G(8) <br/>10: speed56G(9) <br/>11: speed100G(10) <br/>12: speed200G(11) <br/>13: speed400G(12) <br/>14: speed800G(13) <br/>15: unknown(15) | INTEGER       | read-only |
| netPortCurrentSpeed   | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.6.x.y  | Net port current speed define as:<br/>1: speed10M(0) <br/>2: speed100M(1) <br/>3: speed1G(2) <br/>4: speed2500M(3) <br/>5: speed5G(4) <br/>6: speed10G(5) <br/>7: speed25G(6) <br/>8: speed40G(7) <br/>9: speed50G(8) <br/>10: speed56G(9) <br/>11: speed100G(10) <br/>12: speed200G(11) <br/>13: speed400G(12) <br/>14: speed800G(13) <br/>15: unknown(15) | INTEGER       | read-only |
| netPortMacAddr        | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.7.x.y  | Net port mac address.                                        | DisplayString | read-only |
| netPortNegotiatedMode | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.8.x.y  | Net port negotiated mode define as:<br/>1: auto(0) <br/>2: force(1) <br/>3: unknown(255) | INTEGER       | read-only |
| netPortDuplexMode     | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.9.x.y  | Net port duplex mode define as:<br/>1: halfduplex(0) <br/>2: fullduplex(1) <br/>3: notaccess(254) <br/>4: unknown(255) | INTEGER       | read-only |
| netPortLldpMode       | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.10.x.y | Net port lldp mode define as:<br/>1: lldpdisable(0) <br/>2: lldptxmode(1) <br/>3: lldprxmode(2) <br/>4: lldptxrxmode(3) <br/>4: unknown(255) | INTEGER       | read-only |
| netPortBDF            | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.11.x.y | Net port bdf.                                                | DisplayString | read-only |
| netPortNICDeviceName  | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.12.x.y | Net port owner net card device name.Same as owner card netCardDevicename. | DisplayString | read-only |
| netPortNICDeviceId    | 1.3.6.1.4.1.3902.2601.15.1.26.51.1.13.x.y | Net port owner net card device Id. | INTEGER | read-only |

节点 netCardMemoryInfoDescriptionEntry是描述表节点网卡的内存的详细信息表（netCardMemoryInfoDescriptionTable）组成成分的。

其OID 为：1.3.6.1.4.1.3902.2601.15.1.26.52.1  iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1). netCardProperty(26). netCardMemoryInfoDescriptionTable(52). netCardMemoryInfoDescriptionEntry(1) 

    提示：x表示网卡编号，z表示网卡内存信息编号

| 节点名称              | 节点 OID 实例                             | 描述                                                         | 类型          | 权限      |
| --------------------- | ----------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| netCardIndex          | 1.3.6.1.4.1.3902.2601.15.1.26.52.1.1.x.z  | Information about nic index.                                 | INTEGER       | read-only |
| netCardMemId          | 1.3.6.1.4.1.3902.2601.15.1.26.52.1.2.x.z  | Information about nic memory index.                          | INTEGER       | read-only |
| netCardMemType        | 1.3.6.1.4.1.3902.2601.15.1.26.52.1.3.x.z  | Information about nic memory type:<br/>1: qdr(1) <br/>2: ddr(2) <br/>3: unknown(255) | INTEGER       | read-only |
| netCardMemMode        | 1.3.6.1.4.1.3902.2601.15.1.26.52.1.4.x.z  | Information about nic memory mode:<br/>1: qdr4-2000mhz(1) <br/>2: ddr4-2400mhz(2) <br/>3: ddr4-2000mhz(3) <br/>4: unknown(255) | INTEGER       |read-only |
| netCardMemCapa        | 1.3.6.1.4.1.3902.2601.15.1.26.52.1.5.x.z  | Information about nic memory capacity.                       | INTEGER       | read-only |
| netCardMemStatus      | 1.3.6.1.4.1.3902.2601.15.1.26.52.1.6.x.z  | Information about nic memory status:<br/>1: normal(0) <br/>2: abnormal(1) <br/>3: unknown(255) | INTEGER       | read-only |

### 4.18.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.18.3 设置操作约束

​        不支持

### 4.18.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: netCardIndex.1 (integer) 1
    2: netCardLocationType.1 (integer) ocp(2)
    3: netCardLocationSlot.1 (integer) 1
    4: netCardDevicename.1 (octet string) OCP 1 [4F.43.50.20.31 (hex)]
    5: netCardHealthStatus.1 (integer) ok(0)
    6: netCardNICName.1 (octet string) E810-XXVDA2 [45.38.31.30.2D.58.58.56.44.41.32 (hex)]
    7: netCardNICManufacturer.1 (octet string) Intel [49.6E.74.65.6C (hex)]
    8: netCardChipModel.1 (octet string) E810 [45.38.31.30 (hex)]
    9: netCardChipManufacturer.1 (octet string) Intel [49.6E.74.65.6C (hex)]
    10: netCardMaxPortNumber.1 (integer) 2
    11: netCardPortsType.1 (integer) fiber(1)
    12: netCardNICModel.1 (octet string) 2*25GE [32.2A.32.35.47.45 (hex)]
    13: netCardTemperature.1 (integer) unknown(255)
    14: netCardHistoryMaxTemperature.1 (integer) unknown(255)
    15: netCardFirmwareVersion.1 (octet string) 2.3 [32.2E.33 (hex)]
    16: netCardSerialNumber.1 (octet string) N/A [4E.2F.41 (hex)]
    17: netCardDriverName.1 (octet string) ice [69.63.65 (hex)]
    18: netCardRootBDF.1 (octet string) N/A [4E.2F.41 (hex)]
    19: netCardPartNumber.1 (octet string) N/A [4E.2F.41 (hex)]
    20: netCardFpgaStatus.1 (integer) unknown(255)
    21: netCardFpgaTempStatus.1 (integer) unknown(255)
    22: netCardDeviceId.1 (integer) 1
    23: netPortNICIndex.1.1 (integer) 1
    24: netPortNICIndex.1.2 (integer) 1
    25: netPortLocation.1.1 (integer) 1
    26: netPortLocation.1.2 (integer) 2
    27: netPortType.1.1 (integer) fiber(1)
    28: netPortType.1.2 (integer) fiber(1)
    29: netPortLinkStatus.1.1 (integer) linkdown(0)
    30: netPortLinkStatus.1.2 (integer) linkdown(0)
    31: netPortCapableSpeed.1.1 (integer) speed25G(5)
    32: netPortCapableSpeed.1.2 (integer) speed25G(5)
    33: netPortCurrentSpeed.1.1 (integer) unknown(15)
    34: netPortCurrentSpeed.1.2 (integer) unknown(15)
    35: netPortMacAddr.1.1 (octet string) N/A [4E.2F.41 (hex)]
    36: netPortMacAddr.1.2 (octet string) N/A [4E.2F.41 (hex)]
    37: netPortNegotiatedMode.1.1 (integer) force(1)
    38: netPortNegotiatedMode.1.2 (integer) force(1)
    39: netPortDuplexMode.1.1 (integer) unknown(255)
    40: netPortDuplexMode.1.2 (integer) unknown(255)
    41: netPortLldpMode.1.1 (integer) lldpdisable(0)
    42: netPortLldpMode.1.2 (integer) lldpdisable(0)
    43: netPortBDF.1.1 (octet string) N/A [4E.2F.41 (hex)]
    44: netPortBDF.1.2 (octet string) N/A [4E.2F.41 (hex)]
    45: netPortNICDeviceName.1.1 (octet string) OCP 1 [4F.43.50.20.31 (hex)]
    46: netPortNICDeviceName.1.2 (octet string) OCP 1 [4F.43.50.20.31 (hex)]
    47: netPortNICDeviceId.1.1 (integer) 1
    48: netPortNICDeviceId.1.2 (integer) 1
    49: netCardIndex.1.1 (integer) 1
    50: netCardIndex.1.2 (integer) 1
    51: netCardIndex.1.3 (integer) 1
    52: netCardMemId.1.1 (integer) 1
    53: netCardMemId.1.2 (integer) 2
    54: netCardMemId.1.3 (integer) 3
    55: netCardMemType.1.1 (integer) ddr(2)
    56: netCardMemType.1.2 (integer) ddr(2)
    57: netCardMemType.1.3 (integer) ddr(2)
    58: netCardMemMode.1.1 (integer) ddr4-2400mhz(2)
    59: netCardMemMode.1.2 (integer) ddr4-2400mhz(2)
    60: netCardMemMode.1.3 (integer) ddr4-2400mhz(2)
    61: netCardMemCapa.1.1 (integer) 1
    62: netCardMemCapa.1.2 (integer) 0
    63: netCardMemCapa.1.3 (integer) 0
    64: netCardMemStatus.1.1 (integer) abnormal(1)
    65: netCardMemStatus.1.2 (integer) normal(0)
    66: netCardMemStatus.1.3 (integer) normal(0)
    ***** SNMP QUERY FINISHED *****



## 4.19 fcCardProperty详细规格

### 4.19.1 功能说明

#### 4.19.1.1 父节点介绍

FC卡的信息节点，包括2个表量：FC卡的详细信息表（包括 FC卡编号、槽位类型、槽位号、设备名称、健康状态、FC卡名称、厂商名称、芯片名称、芯片厂商名称、最大端口数量、FC卡model、固件版本、序列号、FC卡BDF信息、驱动名称、驱动版本等信息）；FC卡的网口详细信息表（ FC卡端口编号、FC端口丝印编号、链接状态、支持速率、当前速率、wwnn、wwpn、端口BDF、端口所属FC卡设备名称 ）。

 fcCardProperty表节点的OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).fcCardProperty (27)

#### 4.19.1.2 子节点介绍

**表量表**

节点 fcCardDescriptionEntry是描述表节点FC卡的详细信息表（fcCardDescriptionTable）组成成分的。

其OID 为：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).fcCardProperty(27).fcCardDescriptionTable(50).fcCardDescriptionEntry(1) 

    提示：x表示网卡编号

| 节点名称               | 节点 OID 实例                           | 描述                                                         | 类型          | 权限      |
| ---------------------- | --------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| fcCardIndex            | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.1.x  | Fc card index.                                               | INTEGER       | read-only |
| fcCardLocationType     | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.2.x  | Fc card location type define as:<br/>1: pcie(1) <br/>2: unknown(255) | INTEGER     | read-only |
| fcCardLocationSlot     | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.3.x  | Fc card location slot.                                       | INTEGER       | read-only |
| fcCardDevicename       | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.4.x  | Fc card slot info string: location type + location slot.Such as (Pcie Card 5). | DisplayString | read-only |
| fcCardHealthStatus     | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.5.x  | Fc card health status define as:<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER       | read-only |
| fcCardName             | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.6.x  | Fc card name.                                                | DisplayString | read-only |
| fcCardManufacturer     | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.7.x  | Fc card manufacturer name.                                   | DisplayString | read-only |
| fcCardChipModel        | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.8.x  | Fc card chip name.                                           | DisplayString | read-only |
| fcCardChipManufacturer | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.9.x  | Fc card chip manufacturer name.                              | DisplayString | read-only |
| fcCardMaxPortNumber    | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.10.x | Fc card max port number.                                     | INTEGER       | read-only |
| fcCardModel            | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.11.x | Fc card model.Such as (2\*16GE).                             | DisplayString | read-only |
| fcCardFirmwareVersion  | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.12.x | Fc card firmware version.                                    | DisplayString | read-only |
| fcCardSerialNumber     | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.13.x | Fc card serial number.                                       | DisplayString | read-only |
| fcCardRootBDF          | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.14.x | Fc card Root BDF.                                            | DisplayString | read-only |
| fcCardDriverName       | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.15.x | Fc card driver name.                                         | DisplayString | read-only |
| fcCardDriverVersion    | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.16.x | Fc card driver version.                                      | DisplayString | read-only |
| fcCardTemperature      | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.17.x | Fc card temperature(unit: Celsius).255 means fccard is not support to get temperature. | INTEGER | read-only |
| fcCardDeviceId         | 1.3.6.1.4.1.3902.2601.15.1.27.50.1.18.x | Fc card device Id.                                           | INTEGER       | read-only |

节点fcPortDescriptionTableEntry是描述表节点FC卡网口的详细信息表（fcPortDescriptionTable）组成成分的。

其OID 为：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).  fcCardProperty(27). fcPortDescriptionTable(51). fcPortDescriptionTableEntry(1) 

    提示：x表示网卡编号，y表示网口编号

| 节点名称             | 节点 OID 实例                            | 描述                                                         | 类型          | 权限      |
| -------------------- | ---------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| fcPortCardIndex      | 1.3.6.1.4.1.3902.2601.15.1.27.51.1.1.x.y | Fc port owner fc card index.                                 | INTEGER       | read-only |
| fcPortLocation       | 1.3.6.1.4.1.3902.2601.15.1.27.51.1.2.x.y | Fc card port location num, depends on silk.                  | INTEGER       | read-only |
| fcPortLinkStatus     | 1.3.6.1.4.1.3902.2601.15.1.27.51.1.3.x.y | Fc port link status define as:<br/>1: linkdown(0) <br/>2: linkup(1) <br/>3: unknown(255) | INTEGER       | read-only |
| fcPortSupportSpeed   | 1.3.6.1.4.1.3902.2601.15.1.27.51.1.4.x.y | Fc port capable speed define as:<br/>1: supportSpeed4-8-16G(28) <br/>2: supportSpeed8-16-32G(56)<br/>3: unknown(255) | INTEGER       | read-only |
| fcPortCurrentSpeed   | 1.3.6.1.4.1.3902.2601.15.1.27.51.1.5.x.y | Fc port current speed define as:<br/>1: speedauto(0) <br/>2: speed4G(4) <br/>3: speed8G(8) <br/>4: speed16G(16) <br/>5: speed32G(32) <br/>6: unknown(255) | INTEGER       | read-only |
| fcPortWwnn           | 1.3.6.1.4.1.3902.2601.15.1.27.51.1.6.x.y | Fc port wwnn.                                                | DisplayString | read-only |
| fcPortWwpn           | 1.3.6.1.4.1.3902.2601.15.1.27.51.1.7.x.y | Fc port wwwpn.                                               | DisplayString | read-only |
| fcPortBDF            | 1.3.6.1.4.1.3902.2601.15.1.27.51.1.8.x.y | Fc port BDF.                                                 | DisplayString | read-only |
| fcPortCardDeviceName | 1.3.6.1.4.1.3902.2601.15.1.27.51.1.9.x.y | Fc port owner fc card device name.Same as owner card fcCardDevicename | DisplayString | read-only |
| fcPortCardDeviceId   | 1.3.6.1.4.1.3902.2601.15.1.27.51.1.10.x.y | Fc port owner fc card device Id. | INTEGER | read-only |

### 4.19.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.19.3 设置操作约束

​        不支持

### 4.19.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: fcCardIndex.1 (integer) 1
    2: fcCardIndex.2 (integer) 2
    3: fcCardLocationType.1 (integer) pcie(1)
    4: fcCardLocationType.2 (integer) pcie(1)
    5: fcCardLocationSlot.1 (integer) 5
    6: fcCardLocationSlot.2 (integer) 6
    7: fcCardDevicename.1 (octet string) PCIE Card 5 [50.43.49.45.20.43.61.72.64.20.35 (hex)]
    8: fcCardDevicename.2 (octet string) PCIE Card 6 [50.43.49.45.20.43.61.72.64.20.36 (hex)]
    9: fcCardHealthStatus.1 (integer) ok(0)
    10: fcCardHealthStatus.2 (integer) ok(0)
    11: fcCardName.1 (octet string) QLE2690-ACE-SP [51.4C.45.32.36.39.30.2D.41.43.45.2D.53.50 (hex)]
    12: fcCardName.2 (octet string) QLE2740-ACE-SP [51.4C.45.32.37.34.30.2D.41.43.45.2D.53.50 (hex)]
    13: fcCardManufacturer.1 (octet string) Qlogic [51.6C.6F.67.69.63 (hex)]
    14: fcCardManufacturer.2 (octet string) Qlogic [51.6C.6F.67.69.63 (hex)]
    15: fcCardChipModel.1 (octet string) ISP2722 [49.53.50.32.37.32.32 (hex)]
    16: fcCardChipModel.2 (octet string) ISP2722 [49.53.50.32.37.32.32 (hex)]
    17: fcCardChipManufacturer.1 (octet string) Qlogic [51.6C.6F.67.69.63 (hex)]
    18: fcCardChipManufacturer.2 (octet string) Qlogic [51.6C.6F.67.69.63 (hex)]
    19: fcCardMaxPortNumber.1 (integer) 1
    20: fcCardMaxPortNumber.2 (integer) 1
    21: fcCardModel.1 (octet string) 1*16GE [31.2A.31.36.47.45 (hex)]
    22: fcCardModel.2 (octet string) 1*32GE [31.2A.33.32.47.45 (hex)]
    23: fcCardFirmwareVersion.1 (octet string) 01.07.06.00 [30.31.2E.30.37.2E.30.36.2E.30.30 (hex)]
    24: fcCardFirmwareVersion.2 (octet string) 02.50.05.00 [30.32.2E.35.30.2E.30.35.2E.30.30 (hex)]
    25: fcCardSerialNumber.1 (octet string) RFD2049P13324 [52.46.44.32.30.34.39.50.31.33.33.32.34 (hex)]
    26: fcCardSerialNumber.2 (octet string) RFD2124S86312 [52.46.44.32.31.32.34.53.38.36.33.31.32 (hex)]
    27: fcCardRootBDF.1 (octet string) 0000:16:00.0 [30.30.30.30.3A.31.36.3A.30.30.2E.30 (hex)]
    28: fcCardRootBDF.2 (octet string) 0000:a8:00.0 [30.30.30.30.3A.61.38.3A.30.30.2E.30 (hex)]
    29: fcCardDriverName.1 (octet string) qla2xxx [71.6C.61.32.78.78.78 (hex)]
    30: fcCardDriverName.2 (octet string) qla2xxx [71.6C.61.32.78.78.78 (hex)]
    31: fcCardDriverVersion.1 (octet string) N/A [4E.2F.41 (hex)]
    32: fcCardDriverVersion.2 (octet string) N/A [4E.2F.41 (hex)]
    33: fcCardTemperature.1 (integer) 62
    34: fcCardTemperature.2 (integer) 69
    35: fcCardDeviceId.1 (integer) 1
    36: fcCardDeviceId.2 (integer) 1
    37: fcPortCardIndex.1.1 (integer) 1
    38: fcPortCardIndex.2.1 (integer) 2
    39: fcPortLocation.1.1 (integer) 1
    40: fcPortLocation.2.1 (integer) 1
    41: fcPortLinkStatus.1.1 (integer) linkdown(0)
    42: fcPortLinkStatus.2.1 (integer) linkdown(0)
    43: fcPortSupportSpeed.1.1 (integer) supportSpeed4-8-16G(28)
    44: fcPortSupportSpeed.2.1 (integer) supportSpeed8-16-32G(56)
    45: fcPortCurrentSpeed.1.1 (integer) unknown(255)
    46: fcPortCurrentSpeed.2.1 (integer) unknown(255)
    47: fcPortWwnn.1.1 (octet string) 20:00:34:80:0d:3e:c9:a0 [32.30.3A.30.30.3A.33.34.3A.38.30.3A.30.64.3A.33.65.3A.63.39.3A.61.30 (hex)]
    48: fcPortWwnn.2.1 (octet string) 20:00:34:80:0d:3f:73:ee [32.30.3A.30.30.3A.33.34.3A.38.30.3A.30.64.3A.33.66.3A.37.33.3A.65.65 (hex)]
    49: fcPortWwpn.1.1 (octet string) 21:00:34:80:0d:3e:c9:a0 [32.31.3A.30.30.3A.33.34.3A.38.30.3A.30.64.3A.33.65.3A.63.39.3A.61.30 (hex)]
    50: fcPortWwpn.2.1 (octet string) 21:00:34:80:0d:3f:73:ee [32.31.3A.30.30.3A.33.34.3A.38.30.3A.30.64.3A.33.66.3A.37.33.3A.65.65 (hex)]
    51: fcPortBDF.1.1 (octet string) 0000:16:00.0 [30.30.30.30.3A.31.36.3A.30.30.2E.30 (hex)]
    52: fcPortBDF.2.1 (octet string) 0000:a8:00.0 [30.30.30.30.3A.61.38.3A.30.30.2E.30 (hex)]
    53: fcPortCardDeviceName.1.1 (octet string) PCIE Card 5 [50.43.49.45.20.43.61.72.64.20.35 (hex)]
    54: fcPortCardDeviceName.2.1 (octet string) PCIE Card 6 [50.43.49.45.20.43.61.72.64.20.36 (hex)]
    55: fcPortCardDeviceId1.1 (integer) 1
    56: fcPortCardDeviceId2.1 (integer) 1
    ***** SNMP QUERY FINISHED *****



## 4.20 gpuProperty详细规格

### 4.20.1 功能说明

#### 4.20.1.1 父节点介绍

    GPU的信息节点，包括2个表量：GPU的详细信息表（包括GPU编号、GPU核ID、槽位类型、槽位号、设备名称、健康状态、当前功率、当前温度、GPU名称、生产厂商名称、固件版本号、生产日期、部件号、序列号、最大核数、内存大小、额定功率等信息）；GPU性能的详细信息表（包括GPU索引、GPU类型、GPU槽位号、GPU总线号、GPU设备号、GPU功能号、GPU编码器使用率、GPU解码器使用率、GPU使用率、显存空闲量、显存空闲率、GPU温度、GPU功率）。

gpuProperty表节点的OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).gpuProperty (28)  

#### 4.20.1.2 子节点介绍

**表量表**

节点 gpuDescriptionEntry是描述表节点GPU的详细信息表（gpuDescriptionTable）组成成分的。

其OID 为：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).gpuProperty (28).gpuDescriptionTable(50).gpuDescriptionEntry(1) 

    提示：x表示 GPU编号，y表示核ID

| 节点名称              | 节点 OID 实例                             | 描述                                                         | 类型          | 权限      |
| --------------------- | ----------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| gpuIndex              | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.1.x.y  | GPU index.                                                   | INTEGER       | read-only |
| gpuId                 | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.2.x.y  | GPU core id.                                                 | INTEGER       | read-only |
| gpuLocationType       | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.3.x.y  | gpu location type define as:<br/>1: pcie(1) <br/>2: module(3) <br/>3: unknown(255)   | INTEGER       | read-only |
| gpuLocationSlot       | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.4.x.y  | GPU location slot.                                           | INTEGER       | read-only |
| gpuDevicename         | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.5.x.y  | GPU slot info string: location type + location slot.Such as (Pcie Card 5). | DisplayString | read-only |
| gpuHealthStatus       | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.6.x.y  | GPU health status define as:<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER       | read-only |
| gpuCurrentPower       | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.7.x.y  | GPU current power(unit: mW).<br /> -1 means unknown.         | INTEGER       | read-only |
| gpuCurrentTemperature | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.8.x.y  | GPU current temperature(unit: Celsius).<br /> 255 means unknown.  | INTEGER       | read-only |
| gpuName               | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.9.x.y  | GPU card name.                                               | DisplayString | read-only |
| gpuManufacturer       | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.10.x.y | GPU card manufacturer name.                                  | DisplayString | read-only |
| gpuFirmwareVersion    | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.11.x.y | GPU firmware version.                                        | DisplayString | read-only |
| gpuBuildDate          | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.12.x.y | GPU build date.                                              | DisplayString | read-only |
| gpuPartNumber         | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.13.x.y | GPU part number.                                             | DisplayString | read-only |
| gpuSerialNumber       | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.14.x.y | GPU serial number.                                           | DisplayString | read-only |
| gpuMaxCoreNumber      | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.15.x.y | GPU max core number.                                         | INTEGER       | read-only |
| gpuMemorySize         | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.16.x.y | GPU memory size(unit: GB).<br /> 65535 means unknown.        | INTEGER       | read-only |
| gpuRatedPower         | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.17.x.y | GPU rated power(unit: W).<br /> -1 means unknown.            | INTEGER       | read-only |
| gpuCurrentMemoryTemperature | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.18.x.y | GPU current memory temperature(unit: Celsius).<br /> 255 means unknown.    | INTEGER       | read-only |
| gpuMemoryBandWidth          | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.19.x.y | GPU Memory bandwidth(unit: GB/s).                      | INTEGER       | read-only |
| gpuDeviceId | 1.3.6.1.4.1.3902.2601.15.1.28.50.1.20.x.y | GPU device Id. | INTEGER | read-only |

节点 gpuPerfParamEntry是描述表节点GPU性能的详细信息表（gpuPerfParamTable）组成成分的。

其OID 为：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).gpuProperty (28).gpuPerfParamTable(51).gpuPerfParamEntry(1) 

    提示：x表示 GPU编号

| 节点名称              | 节点 OID 实例                             | 描述                                                         | 类型          | 权限      |
| --------------------- | ----------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| gpuDevIndex           | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.1.x    | GPU device index.                                            | INTEGER       | read-only |
| gpuType               | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.2.x    | GPU type define as: <br/>1: gpu(1) <br/>2: oam(2) <br/>3: sxm(3)  | INTEGER       | read-only |
| gpuSlot               | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.3.x    | GPU slot.                                                    | INTEGER       | read-only |
| gpuBus                | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.4.x    | GPU bus.                                                     | INTEGER       | read-only |
| gpuDevice             | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.5.x    | GPU device.                                                  | INTEGER       | read-only |
| gpuFunction           | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.6.x    | GPU function.                                                | INTEGER       | read-only |
| gpuEncodeUsage        | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.7.x    | GPU encode usage.                                            | INTEGER       | read-only |
| gpuDecodeUsage        | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.8.x    | GPU decode uasge.                                            | INTEGER       | read-only |
| gpuUsage              | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.9.x    | GPU usage.                                                   | INTEGER       | read-only |
| gpuReservedCapacityMiB | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.10.x  | GPU reserved capacity(unit: MiB).                            | INTEGER       | read-only |
| gpuReservedCapacityPercent | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.11.x | GPU reserved capacity(unit: percent).                     | INTEGER       | read-only |
| gpuTemperature        | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.12.x   | GPU temperature(unit: Celsius).                              | INTEGER       | read-only |
| gpuPower              | 1.3.6.1.4.1.3902.2601.15.1.28.51.1.13.x   | GPU power(unit: W).                                          | INTEGER       | read-only |


### 4.20.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.20.3 设置操作约束

​        不支持

### 4.20.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: gpuIndex.1.1 (integer) 1
    2: gpuIndex.2.1 (integer) 2
    3: gpuId.1.1 (integer) 1
    4: gpuId.2.1 (integer) 1
    5: gpuLocationType.1.1 (integer) pcie(1)
    6: gpuLocationType.2.1 (integer) pcie(1)
    7: gpuLocationSlot.1.1 (integer) 10
    8: gpuLocationSlot.2.1 (integer) 17
    9: gpuDevicename.1.1 (octet string) PCIE Card 10 [50.43.49.45.20.43.61.72.64.20.31.30 (hex)]
    10: gpuDevicename.2.1 (octet string) PCIE Card 17 [50.43.49.45.20.43.61.72.64.20.31.37 (hex)]
    11: gpuHealthStatus.1.1 (integer) ok(0)
    12: gpuHealthStatus.2.1 (integer) ok(0)
    13: gpuCurrentPower.1.1 (integer) unknown(-1)
    14: gpuCurrentPower.2.1 (integer) unknown(-1)
    15: gpuCurrentTemperature.1.1 (integer) 43
    16: gpuCurrentTemperature.2.1 (integer) unknown(255)
    17: gpuName.1.1 (octet string) NVIDIA A10 [4E.56.49.44.49.41.20.41.31.30 (hex)]
    18: gpuName.2.1 (octet string) NVIDIA A10 [4E.56.49.44.49.41.20.41.31.30 (hex)]
    19: gpuManufacturer.1.1 (octet string) Nvidia [4E.76.69.64.69.61 (hex)]
    20: gpuManufacturer.2.1 (octet string) Nvidia [4E.76.69.64.69.61 (hex)]
    21: gpuFirmwareVersion.1.1 (octet string) 94.02.5C.00.04 [39.34.2E.30.32.2E.35.43.2E.30.30.2E.30.34 (hex)]
    22: gpuFirmwareVersion.2.1 (octet string) N/A [4E.2F.41 (hex)]
    23: gpuBuildDate.1.1 (octet string) 2021/06/28 [32.30.32.31.2F.30.36.2F.32.38 (hex)]
    24: gpuBuildDate.2.1 (octet string) N/A [4E.2F.41 (hex)]
    25: gpuPartNumber.1.1 (octet string) N/A [4E.2F.41 (hex)]
    26: gpuPartNumber.2.1 (octet string) N/A [4E.2F.41 (hex)]
    27: gpuSerialNumber.1.1 (octet string) 1322621032509 [31.33.32.32.36.32.31.30.33.32.35.30.39 (hex)]
    28: gpuSerialNumber.2.1 (octet string) N/A [4E.2F.41 (hex)]
    29: gpuMaxCoreNumber.1.1 (integer) 1
    30: gpuMaxCoreNumber.2.1 (integer) 1
    31: gpuMemorySize.1.1 (integer) 24
    32: gpuMemorySize.2.1 (integer) 24
    33: gpuRatedPower.1.1 (integer) 150
    34: gpuRatedPower.2.1 (integer) 150
    35: gpuCurrentMemoryTemperature.1.1 (integer) unknown(255)
    36: gpuCurrentMemoryTemperature.2.1 (integer) unknown(255)
    37: gpuMemoryBandWidth.1.1 (octet string) 600GB/s [36.30.30.47.42.2F.73 (hex)]
    38: gpuMemoryBandWidth.2.1 (octet string) 600GB/s [36.30.30.47.42.2F.73 (hex)]
    39: gpuDeviceId.1.1 (integer) 1
    40: gpuDeviceId.2.1 (integer) 1
    41: gpuDevIndex.1 (integer) 1
    42: gpuDevIndex.2 (integer) 2
    43: gpuType.1 (integer) gpu(1)
    44: gpuType.2 (integer) gpu(1)
    45: gpuSlot.1 (integer) 8
    46: gpuSlot.2 (integer) 9
    47: gpuBus.1 (integer) 42
    48: gpuBus.2 (integer) 43
    49: gpuDevice.1 (integer) 0
    50: gpuDevice.2 (integer) 0
    51: gpuFunction.1 (integer) 0
    52: gpuFunction.2 (integer) 0
    53: gpuEncodeUsage.1 (integer) 0
    54: gpuEncodeUsage.2 (integer) 0
    55: gpuDecodeUsage.1 (integer) 0
    56: gpuDecodeUsage.2 (integer) 0
    57: gpuUsage.1 (integer) 0
    58: gpuUsage.2 (integer) 0
    59: gpuReservedCapacityMiB.1 (integer) 22685
    60: gpuReservedCapacityMiB.2 (integer) 22685
    61: gpuReservedCapacityPercent.1 (integer) 99
    62: gpuReservedCapacityPercent.2 (integer) 99
    63: gpuTemperature.1 (integer) 40
    64: gpuTemperature.2 (integer) 42
    65: gpuPower.1 (integer) 13426
    66: gpuPower.2 (integer) 12833
    ***** SNMP QUERY FINISHED *****


## 4.21 raidControllerProperty详细规格

### 4.21.1 功能说明

#### 4.21.1.1 父节点介绍

    RAID控制器的信息节点，包括1个表量：RAID控制器的详细信息表（包括控制器的名称、类型、健康状态、firmware版本、接口类型、BBU型号等信息）。

raidControllerProperty 表节点的OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).raidControllerProperty(29) 

#### 4.21.1.2 子节点介绍

**表量表**

节点 raidControllerDescriptionEntry是描述表节点RAID控制器的详细信息表（raidControllerDescriptionTable）组成成分的。

其OID为：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).raidControllerProperty(29).raidControllerDescriptionTable(50).raidControllerDescriptionEntry(1) 

    提示：x 表示RAID 控制器编号

| 节点名称                             | 节点 OID 实例                           | 描述                                                         | 类型          | 权限      |
| ------------------------------------ | --------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| raidControllerIndex                  | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.1.x  | Information about RAID controller index.                     | INTEGER       | read-only |
| raidControllerId                     | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.2.x  | Information about RAID controller Id.                        | INTEGER       | read-only |
| raidControllerName                   | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.3.x  | Information about RAID controller name.                      | DisplayString | read-only |
| raidControllerComponentName          | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.4.x  | Information about RAID controller component name.            | DisplayString | read-only |
| raidControllerMode                   | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.5.x  | Information about RAID controller mode.<br/>1: RAID(1)<br/>2: HBA(2)<br/>3: JBOD(3)<br/>4: unknown(255) | INTEGER       | read-only |
| raidControllerLocationType           | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.6.x  | Information about RAID controller location type.<br/> 1: embedded(1) <br/>2: PCIE(2) <br/> 3: unknown(255) | INTEGER    | read-only |
| raidControllerLocationSlot           | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.7.x  | Information about RAID controller location slot.             | INTEGER       | read-only |
| raidControllerVendor                 | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.8.x  | Information about RAID controller vendor.                    | DisplayString | read-only |
| raidControllerChipVendor             | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.9.x  | Information about RAID controller chip vendor.               | DisplayString | read-only |
| raidControllerChipModel              | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.10.x | Information about RAID controller chip model.                | DisplayString | read-only |
| raidControllerHealthStatus           | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.11.x | Information about RAID controller health status.<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER       | read-only |
| raidControllerSupportOOBManagement   | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.12.x | Information about RAID controller if support OOB management.<br/>1: no(1) <br/>2: yes(2) | INTEGER       | read-only |
| raidControllerFwVersion              | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.13.x | Information about RAID controller firmware version.          | DisplayString | read-only |
| raidControllerPackageVersion         | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.14.x | Information about RAID controller firmware package version.  | DisplayString | read-only |
| raidControllerNVDataVersion          | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.15.x | Information about RAID controller NVData version.            | DisplayString | read-only |
| raidControllerBiosVersion            | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.16.x | Information about RAID controller bios version.              | DisplayString | read-only |
| raidControllerDriverVersion          | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.17.x | Information about RAID controller driver version.            | DisplayString | read-only |
| raidControllerSerialNumber           | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.18.x | Information about RAID controller serial number.             | DisplayString | read-only |
| raidControllerSASAddress             | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.19.x | Information about RAID controller sas address.               | DisplayString | read-only |
| raidControllerPartNumber             | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.20.x | Information about RAID controller part number.               | DisplayString | read-only |
| raidControllerJBODEnable             | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.21.x | Information about the JBOD state of RAID controller.<br/>1: disable(1) <br/>2: enabled(2)<br/>3: unknown(255) | INTEGER       | read-only |
| raidControllerDeviceInterface        | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.22.x | Information about RAID controller device interface type.<br/>1: SPI(1) <br/>2: SAS-3G(2) <br/>3: SATA-1500M(3) <br/>4: SATA-3G(4)<br/>5: SAS-6G(5) <br/>6: SAS-12G(6) <br/>7: SATA-6G(7) <br/>8: SAS-24G(8) <br/>9: unknown(255)| INTEGER       | read-only |
| raidControllerMemorySizeInMiB        | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.23.x | Information about RAID controller memory size(unit: MB). <br/>65535 means unknown.     | INTEGER       | read-only |
| raidControllerTemperature            | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.24.x | Information about RAID controller temperature(unit: Celsius).<br/>255 means unknown.   | INTEGER       | read-only |
| raidControllerMinStripSupportInBytes | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.25.x | Information about the minimum strip size that RAID controller support. | INTEGER       | read-only |
| raidControllerMaxStripSupportInBytes | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.26.x | Information about the maximum strip size that RAID controller support. | INTEGER       | read-only |
| raidControllerSupportedRAIDLevels    | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.27.x | Information about RAID controller supported levels.          | DisplayString | read-only |
| raidControllerSpotProtocols          | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.28.x | Information about RAID controller supported protocols.       | DisplayString | read-only |
| raidControllerBBUPresence            | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.29.x | Information about RAID controller's BBU presence.<br/>1: absent(1) <br/>2: present(2)<br/>3: unknown(255) | INTEGER       | read-only |
| raidControllerBBUName                | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.30.x | Information about RAID controller's BBU name.                | DisplayString | read-only |
| raidControllerBBUHealthStatus        | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.31.x | Information about RAID controller's BBU health status.<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER       | read-only |
| raidControllerBBUAvailabilityStatus  | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.32.x | Information about RAID controller's BBU availability status.<br/>1: missing(0) <br/>2: ready(1) <br/>3: learnCycleActive(2) <br/>4: learnCycleFailed(3) <br/>5: replacePack(4) <br/>6: unknown(255) | INTEGER       | read-only |
| raidControllerBBUTemperature         | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.33.x | Information about RAID controller's BBU temperature(unit: Celsius).<br/>255 means unknown.    | INTEGER       | read-only |
| raidControllerBBUCurrent             | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.34.x | Information about RAID controller's BBU current(unit: mA).<br/>255 means unknown.        | INTEGER       | read-only |
| raidControllerBBUVoltage             | 1.3.6.1.4.1.3902.2601.15.1.29.50.1.35.x | Information about RAID controller's BBU voltage(unit: mV).<br/>255 means unknown.        | INTEGER       | read-only |

### 4.21.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.21.3 设置操作约束

​        不支持

### 4.21.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: raidControllerIndex.1 (integer) 1
    2: raidControllerId.1 (integer) 3
    3: raidControllerName.1 (octet string) AVAGO MegaRAID SAS 9361-8i [41.56.41.47.4F.20.4D.65.67.61.52.41.49.44.20.53.41.53.20.39.33.36.31.2D.38.69 (hex)]
    4: raidControllerComponentName.1 (octet string) RAID Card3 [52.41.49.44.20.43.61.72.64.33 (hex)]
    5: raidControllerMode.1 (integer) raid(1)
    6: raidControllerLocationType.1 (integer) pcie(2)
    7: raidControllerLocationSlot.1 (integer) 3
    8: raidControllerVendor.1 (octet string) Broadcom [42.72.6F.61.64.63.6F.6D (hex)]
    9: raidControllerChipVendor.1 (octet string) Broadcom [42.72.6F.61.64.63.6F.6D (hex)]
    10: raidControllerChipModel.1 (octet string) RAID_SAS3108 [52.41.49.44.5F.53.41.53.33.31.30.38 (hex)]
    11: raidControllerHealthStatus.1 (integer) ok(0)
    12: raidControllerSupportOOBManagement.1 (integer) yes(2)
    13: raidControllerFwVersion.1 (octet string) 4.680.00-8392 [34.2E.36.38.30.2E.30.30.2D.38.33.39.32 (hex)]
    14: raidControllerPackageVersion.1 (octet string) 24.21.0-0067 [32.34.2E.32.31.2E.30.2D.30.30.36.37 (hex)]
    15: raidControllerNVDataVersion.1 (octet string) 3.1705.00-0016 [33.2E.31.37.30.35.2E.30.30.2D.30.30.31.36 (hex)]
    16: raidControllerBiosVersion.1 (octet string) 6.36.00.3_4.19.08.00_0x06180203 [36.2E.33.36.2E.30.30.2E.33.5F.34.2E.31.39.2E.30.38.2E.30.30.5F.30.78.30.36.31.38.30.32.30.33 (hex)]
    17: raidControllerDriverVersion.1 (octet string) N/A [4E.2F.41 (hex)]
    18: raidControllerSerialNumber.1 (octet string) SKA2575807 [53.4B.41.32.35.37.35.38.30.37 (hex)]
    19: raidControllerSASAddress.1 (octet string) 500605b0127baf31 [35.30.30.36.30.35.62.30.31.32.37.62.61.66.33.31 (hex)]
    20: raidControllerPartNumber.1 (octet string) N/A [4E.2F.41 (hex)]
    21: raidControllerJBODEnable.1 (integer) disabled(1)
    22: raidControllerDeviceInterface.1 (integer) sas-12G(6)
    23: raidControllerMemorySizeInMiB.1 (integer) 2048
    24: raidControllerTemperature.1 (integer) 50
    25: raidControllerMinStripSupportInBytes.1 (integer) 65536
    26: raidControllerMaxStripSupportInBytes.1 (integer) 1048576
    27: raidControllerSupportedRAIDLevels.1 (octet string) RAID0, RAID1, RAID5, RAID6, RAID00, RAID10, RAID50, RAID60 [52.41.49.44.30.2C.20.52.41.49.44.31.2C.20.52.41.49.44.35.2C.20.52.41.49.44.36.2C.20.52.41.49.44.30.30.2C.20.52.41.49.44.31.30.2C.20.52.41.49.44.35.30.2C.20.52.41.49.44.36.30 (hex)]
    28: raidControllerSupportedProtocols.1 (octet string) SAS,SATA [53.41.53.2C.53.41.54.41 (hex)]
    29: raidControllerBBUPresence.1 (integer) absent(1)
    30: raidControllerBBUName.1 (octet string) N/A [4E.2F.41 (hex)]
    31: raidControllerBBUHealthStatus.1 (integer) unknown(255)
    32: raidControllerBBUAvailabilityStatus.1 (integer) unknown(255)
    33: raidControllerBBUTemperature.1 (integer) unknown(255)
    34: raidControllerBBUCurrent.1 (integer) unknown(255)
    35: raidControllerBBUVoltage.1 (integer) unknown(255)
    ***** SNMP QUERY FINISHED *****



## 4.22  hardDiskProperty详细规格

### 4.22.1 功能说明

#### 4.22.1.1 父节点介绍

    物理盘信息节点，包括3个标量：物理盘整体健康状态、服务器支持的最大硬盘数量、当前在位的硬盘数量，2个表量：物理盘的详细信息表（包括槽位号、厂商、序列号、型号、容量、状态等）、物理盘在位状态表（包括槽位号、在位状态）。

hardDiskProperty 表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).hardDiskProperty(30)

#### 4.22.1.2 子节点介绍

**标量表**

| 节点名称                | 节点 OID 实例                     | 描述                                                         | 类型    | 权限      |
| ----------------------- | --------------------------------- | ------------------------------------------------------------ | ------- | --------- |
| hardDiskEntireStatus    | 1.3.6.1.4.1.3902.2601.15.1.30.1   | Information about all hard disk health status.<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER | read-only |
| hardDiskMaxSupportNum   | 1.3.6.1.4.1.3902.2601.15.1.30.2   | Information about hard disk's max support num.<br />255 means unknown. | INTEGER | read-only |
| hardDiskTotalPresentNum | 1.3.6.1.4.1.3902.2601.15.1.30.3   | Information about hard disk's total present num.<br />255 means unknown. | INTEGER | read-only |



**表量表**

节点 hardDiskDescriptionEntry 是描述表节点物理盘的详细信息表（ hardDiskDescriptionTable ）组成成分的。

其OID 为：

iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).hardDiskProperty(30).hardDiskDescriptionTable(50).hardDiskDescriptionEntry(1)

    提示：x表示硬盘序号

| 节点名称                   | 节点 OID 实例                           | 描述                                                         | 类型          | 权限           |
| -------------------------- | --------------------------------------- | ------------------------------------------------------------ | ------------- | -------------- |
| hardDiskIndex              | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.1.x  | Hard disk index.                                             | INTEGER       | read-only      |
| hardDiskLocation           | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.2.x  | Hard disk location slot.<br /> 255 means unknown.            | INTEGER       | read-only      |
| hardDiskDevicename         | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.3.x  | Hard disk device name.                                       | DisplayString | read-only      |
| hardDiskHealthStatus       | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.4.x  | Hard disk health status.<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER       | read-only      |
| hardDiskAvailabilityStatus | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.5.x  | Hard disk availability status.<br />1: unconfigured-good(0) <br />2: unconfigured-bad(1) <br />3: global-hot-spare(2) <br />4: offline(4) <br />5: failed(5) <br />6: rebuild(6) <br />7: online(7) <br />8: copyback(8) <br />9: jbod(9) <br />10: unconfigured-shielded(10) <br />11: hot-spare-shielded(11) <br />12: configured-shielded(12) <br />13: dedicated-hot-spare(13) <br />14: foreign(14) <br />15: predictive-failure(15)  <br />16: unknown(255) | INTEGER       | read-only      |
| hardDiskManufacturer       | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.6.x  | Hard disk manufacturer.                                      | DisplayString | read-only      |
| hardDiskModelNumber        | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.7.x  | Hard disk model number.                                      | DisplayString | read-only      |
| hardDiskSerialNumber       | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.8.x  | Hard disk serial number.                                     | DisplayString | read-only      |
| hardDiskFwVersion          | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.9.x  | Hard disk firmware version.                                  | DisplayString | read-only      |
| hardDiskSASAddr            | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.10.x | Hard disk SAS address.                                       | DisplayString | read-only      |
| hardDiskMediaType          | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.11.x | Hard disk media type. <br />1: hdd(0) <br />2: ssd(1) <br />3: ssm(2) <br />4: unknown(255) | INTEGER       | read-only      |
| hardDiskInterfaceType      | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.12.x | Hard disk interface type. <br />1: undefined(0) <br />2: parallel-scsi(1) <br />3: sas(2) <br />4: sata(3) <br />5: fiber-channel(4) <br />6: pcie(5) <br />7: nvme(6) <br />8: unknown(255) | INTEGER       | read-only      |
| hardDiskCapacityInGB       | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.13.x | Hard disk capacity(unit: GB).                                | INTEGER       | read-only      |
| hardDiskCapacityInByte     | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.14.x | Hard disk capacity(unit: Byte).                              | INTEGER       | read-only      |
| hardDiskTemperature        | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.15.x | Hard disk temperature(unit: Celsius). <br />255 means unknown.  | INTEGER       | read-only      |
| hardDiskPowerState         | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.16.x | Hard disk power state.<br />1: spun-up(1) <br />2: spun-down(2) <br />3: transition(3) <br />4: unknown(255) | INTEGER       | read-only      |
| hardDiskCapableSpeed       | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.17.x | Hard disk maximum supported speed.<br />1: speed1p5Gbps(1) <br />2: speed3Gbps(2) <br />3: speed6Gbps(3) <br />4: speed12Gbps(4) <br />5: speed24Gbps(5) <br />6: speed5GTps(6) <br />7: speed8GTps(7) <br />8: speed16GTps(8) <br />9: speed32GTps(9) <br />10: unknown(255) | INTEGER       | read-only      |
| hardDiskNegotiatedSpeed    | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.18.x | Hard disk negotiated speed. <br />1: speed1p5Gbps(1) <br />2: speed3Gbps(2) <br />3: speed6Gbps(3) <br />4: speed12Gbps(4) <br />5: speed24Gbps(5) <br />6: speed5GTps(6) <br />7: speed8GTps(7) <br />8: speed16GTps(8) <br />9: speed32GTps(9) <br />10: unknown(255) | INTEGER       | read-only      |
| hardDiskRotateRate         | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.19.x | Hard disk rotate rate. <br />1: speed5400RPM(0) <br />2: speed7200RPM(1) <br />3: speed10000RPM(2) <br />4: speed10025RPM(3) <br />5: speed15000RPM(4) <br />6: na(5) <br />7: speed10500RPM(6) <br />8: speed10520RPM(7) <br />9: speed15030RPM(8) <br />10: speed15052RPM(9) <br />11: unknown(255) | INTEGER       | read-only      |
| hardDiskSize               | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.20.x | Hard disk size(in).<br />1: size2p5(0) <br />2: size3p5(1) <br />3: unknown(255) | INTEGER       | read-only      |
| hardDiskSmartState         | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.21.x | Hard disk smart state.<br />1: unknown(0) <br />2: detected(1) <br />3: not-detected(2) | INTEGER       | read-only      |
| hardDiskPrefailState       | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.22.x | Hard disk prefail state.<br />1: no(1) <br />2: yes(2) <br />3: unknown(255) | INTEGER       | read-only      |
| hardDiskPrefailErrCount    | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.23.x | Hard disk prefail error count.<br />1048575 means unknown.       | INTEGER       | read-only      |
| hardDiskMediaErrCount      | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.24.x | Hard disk media error count.<br />1048575 means unknown.         | INTEGER       | read-only      |
| hardDiskOtherErrCount      | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.25.x | Hard disk other error count.<br />1048575 means unknown.         | INTEGER       | read-only      |
| hardDiskLocationState      | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.26.x | Hard disk location led state. <br />1: led-on(1) <br />2: led-off(2) <br />3: unknown(255) | INTEGER       | read-only      |
| hardDiskHotSpareState      | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.27.x | Hard disk hot spare state.<br />1: none(0) <br />2: global(1) <br />3: dedicated(2) <br />4: unknown(255) | INTEGER       | read-only      |
| hardDiskRebuildProgress    | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.28.x | Hard disk rebuild progress (0 - 100%). <br />255 means unknown.  | INTEGER       | read-only      |
| hardDiskRemainLifetime     | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.29.x | Hard disk remaining lifetime rate(0-100%)<br />255 means unknown.| INTEGER       | read-only      |
| pchHardDiskCPUNum          | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.30.x | PCH disk CPU Number. <br />255 means unknown.      | INTEGER       | read-only      |
| pchHardDiskHBAPortNum      | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.31.x | PCH disk HBA Port Number. <br />255 means unknown. | INTEGER       | read-only      |
| pchHardDiskBDFNum          | 1.3.6.1.4.1.3902.2601.15.1.30.50.1.32.x | PCH disk BDF Number. | DisplayString        | read-only      |

节点 hardDiskPresenceEntry是描述表节点物理盘在位状态表（ hardDiskPresenceTable）组成成分的。其OID 为：

iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).hardDiskProperty(30).hardDiskPresenceTable(51).hardDiskPresenceEntry(1)

    提示：x表示硬盘序号

| 节点名称               | 节点 OID 实例                          | 描述                                                         | 类型    | 权限      |
| ---------------------- | -------------------------------------- | ------------------------------------------------------------ | ------- | --------- |
| hardDiskLocationSlot   | 1.3.6.1.4.1.3902.2601.15.1.30.51.1.1.x | Hard disk location slot.                                     | INTEGER | read-only |
| hardDiskPresenceStatus | 1.3.6.1.4.1.3902.2601.15.1.30.51.1.2.x | Hard disk presence. <br />1: absence(1) <br />2: presence(2) <br />3: unknown(255) | INTEGER | read-only |

### 4.22.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.22.3 设置操作约束

​        不支持

### 4.22.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: hardDiskEntireStatus.0 (integer) unknown(255)
    2: hardDiskMaxSupportNum.0 (integer) 25
    3: hardDiskTotalPresentNum.0 (integer) 0
    4: hardDiskLocationSlot.0 (integer) 0
    5: hardDiskLocationSlot.1 (integer) 1
    6: hardDiskLocationSlot.2 (integer) 2
    7: hardDiskLocationSlot.3 (integer) 3
    8: hardDiskLocationSlot.4 (integer) 4
    9: hardDiskLocationSlot.5 (integer) 5
    10: hardDiskLocationSlot.6 (integer) 6
    11: hardDiskLocationSlot.7 (integer) 7
    12: hardDiskLocationSlot.8 (integer) 8
    13: hardDiskLocationSlot.9 (integer) 9
    14: hardDiskLocationSlot.10 (integer) 10
    15: hardDiskLocationSlot.11 (integer) 11
    16: hardDiskLocationSlot.12 (integer) 12
    17: hardDiskLocationSlot.13 (integer) 13
    18: hardDiskLocationSlot.14 (integer) 14
    19: hardDiskLocationSlot.15 (integer) 15
    20: hardDiskLocationSlot.16 (integer) 16
    21: hardDiskLocationSlot.17 (integer) 17
    22: hardDiskLocationSlot.18 (integer) 18
    23: hardDiskLocationSlot.19 (integer) 19
    24: hardDiskLocationSlot.20 (integer) 20
    25: hardDiskLocationSlot.21 (integer) 21
    26: hardDiskLocationSlot.22 (integer) 22
    27: hardDiskLocationSlot.23 (integer) 23
    28: hardDiskLocationSlot.24 (integer) 24
    29: hardDiskPresenceStatus.0 (integer) absence(1)
    30: hardDiskPresenceStatus.1 (integer) absence(1)
    31: hardDiskPresenceStatus.2 (integer) absence(1)
    32: hardDiskPresenceStatus.3 (integer) absence(1)
    33: hardDiskPresenceStatus.4 (integer) absence(1)
    34: hardDiskPresenceStatus.5 (integer) absence(1)
    35: hardDiskPresenceStatus.6 (integer) absence(1)
    36: hardDiskPresenceStatus.7 (integer) absence(1)
    37: hardDiskPresenceStatus.8 (integer) absence(1)
    38: hardDiskPresenceStatus.9 (integer) absence(1)
    39: hardDiskPresenceStatus.10 (integer) absence(1)
    40: hardDiskPresenceStatus.11 (integer) absence(1)
    41: hardDiskPresenceStatus.12 (integer) absence(1)
    42: hardDiskPresenceStatus.13 (integer) absence(1)
    43: hardDiskPresenceStatus.14 (integer) absence(1)
    44: hardDiskPresenceStatus.15 (integer) absence(1)
    45: hardDiskPresenceStatus.16 (integer) absence(1)
    46: hardDiskPresenceStatus.17 (integer) absence(1)
    47: hardDiskPresenceStatus.18 (integer) absence(1)
    48: hardDiskPresenceStatus.19 (integer) absence(1)
    49: hardDiskPresenceStatus.20 (integer) absence(1)
    50: hardDiskPresenceStatus.21 (integer) absence(1)
    51: hardDiskPresenceStatus.22 (integer) absence(1)
    52: hardDiskPresenceStatus.23 (integer) absence(1)
    53: hardDiskPresenceStatus.24 (integer) absence(1)
    ***** SNMP QUERY FINISHED *****




## 4.23 nvmeDeviceProperty详细规格

### 4.23.1 功能说明

#### 4.23.1.1 父节点介绍

    NVMe设备信息节点，包括1个表量：NVMe设备的详细信息表（包括槽位信息、设备样式、设备名称、厂商、型号、序列号、容量、固件版本、媒介类型、接口类型、剩余寿命等。）

nvmeDeviceProperty表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).nvmeDeviceProperty(31)

#### 4.23.1.2 子节点介绍

**表量表**

节点 nvmeDeviceDescriptionEntry是描述表节点（nvmeDeviceDescriptionTable）组成成分的。

其OID 为： iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).nvmeDeviceProperty(31).nvmeDeviceDescriptionTable(50).nvmeDeviceDescriptionEntry(1) 

    提示：x表示NVMe设备编号（nvmeDeviceIndex）

| 节点名称                 | 节点 OID 实例                           | 描述                                                         | 类型          | 权限         |
| ------------------------ | --------------------------------------- | ------------------------------------------------------------ | ------------- |------------- |
| nvmeDeviceIndex          | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.1.x  | Information about nvme device index.                         | INTEGER       |read-only|
| nvmeDeviceLocation       | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.2.x  | Information about nvme device location slot.                 | INTEGER       |read-only|
| nvmeDeviceFormType       | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.3.x  | Information about nvme device form type. <br />1: u2(1)  <br />2: aic(2)  <br />3: m2(3)  <br />4: u3(4)  <br /> 5: unknown(255) | INTEGER       |read-only|
| nvmeDeviceName           | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.4.x  | Information about nvme device name.                          | DisplayString |read-only|
| nvmeDeviceStatus         | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.5.x  | Information about nvme device health status.<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER       |read-only|
| nvmeDeviceManufacturer   | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.6.x  | Information about nvme device manufacturer.                  | DisplayString |read-only|
| nvmeDeviceModelNumber    | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.7.x  | Information about nvme device model number.                  | DisplayString |read-only|
| nvmeDeviceSerialNumber   | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.8.x  | Information about nvme device serial number.                 | DisplayString |read-only|
| nvmeDevicePartNumber     | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.9.x  | Information about nvme device part number.                   | DisplayString |read-only|
| nvmeDeviceFwVersion      | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.10.x | Information about nvme device firmware version.              | DisplayString |read-only|
| nvmeDeviceMediaType      | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.11.x | Information about nvme device media type. <br />1: ssd(1) <br />2: unknown(255) | INTEGER       |read-only|
| nvmeDeviceInterfaceType  | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.12.x | Information about nvme device interface type. <br />1: pcie(5) <br />2: nvme(6) <br />3: unknown(255) | INTEGER       |read-only|
| nvmeDeviceCapacityInGB   | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.13.x | Information about nvme device capacity(unit: GB).            | INTEGER       |read-only|
| nvmeDeviceTemperature    | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.14.x | Information about nvme device temperature(unit: Celsius). <br />255 means unknown.     | INTEGER       |read-only|
| nvmeDeviceRemainLifetime | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.15.x | Information about nvme device remaining lifetime rate(0-100%). <br />255 means unknown. | INTEGER       |read-only|
| nvmeDeviceCapacityInByte | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.16.x | Information about nvme device capacity(unit: Byte).          | DisplayString |read-only|
| nvmeDeviceLocationState  | 1.3.6.1.4.1.3902.2601.15.1.31.50.1.17.x | NVME location led presence status. <br />1: on(1) <br />2: off(2) <br /> 3: unknown(255)  | INTEGER       |read-only|

### 4.23.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.23.3 设置操作约束

​        不支持

### 4.23.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: nvmeDeviceIndex.1 (integer) 1
    2: nvmeDeviceIndex.2 (integer) 2
    3: nvmeDeviceLocation.1 (integer) 0
    4: nvmeDeviceLocation.2 (integer) 6
    5: nvmeDeviceFormType.1 (integer) type-u2(1)
    6: nvmeDeviceFormType.2 (integer) type-u2(1)
    7: nvmeDeviceName.1 (octet string) Disk0 [44.69.73.6B.30 (hex)]
    8: nvmeDeviceName.2 (octet string) Disk6 [44.69.73.6B.36 (hex)]
    9: nvmeDeviceStatus.1 (integer) critical(4)
    10: nvmeDeviceStatus.2 (integer) critical(4)
    11: nvmeDeviceManufacturer.1 (octet string) Intel [49.6E.74.65.6C (hex)]
    12: nvmeDeviceManufacturer.2 (octet string) Intel [49.6E.74.65.6C (hex)]
    13: nvmeDeviceModelNumber.1 (octet string) INTEL SSDPE2KE016T8 [49.4E.54.45.4C.20.53.53.44.50.45.32.4B.45.30.31.36.54.38 (hex)]
    14: nvmeDeviceModelNumber.2 (octet string) INTEL SSDPE2KE016T8 [49.4E.54.45.4C.20.53.53.44.50.45.32.4B.45.30.31.36.54.38 (hex)]
    15: nvmeDeviceSerialNumber.1 (octet string) BTLN143106LR1P6AGN [42.54.4C.4E.31.34.33.31.30.36.4C.52.31.50.36.41.47.4E (hex)]
    16: nvmeDeviceSerialNumber.2 (octet string) BTLN143106071P6AGN [42.54.4C.4E.31.34.33.31.30.36.30.37.31.50.36.41.47.4E (hex)]
    17: nvmeDevicePartNumber.1 (octet string) N/A [4E.2F.41 (hex)]
    18: nvmeDevicePartNumber.2 (octet string) N/A [4E.2F.41 (hex)]
    19: nvmeDeviceFwVersion.1 (octet string) N/A [4E.2F.41 (hex)]
    20: nvmeDeviceFwVersion.2 (octet string) N/A [4E.2F.41 (hex)]
    21: nvmeDeviceMediaType.1 (integer) ssd(1)
    22: nvmeDeviceMediaType.2 (integer) ssd(1)
    23: nvmeDeviceInterfaceType.1 (integer) pcie(5)
    24: nvmeDeviceInterfaceType.2 (integer) pcie(5)
    25: nvmeDeviceCapacityInGB.1 (integer) 1600
    26: nvmeDeviceCapacityInGB.2 (integer) 1600
    27: nvmeDeviceTemperature.1 (integer) 255
    28: nvmeDeviceTemperature.2 (integer) 255
    29: nvmeDeviceRemainLifetime.1 (integer) unknown(255)
    30: nvmeDeviceRemainLifetime.2 (integer) unknown(255)
    31: nvmeDeviceDescriptionEntry.16.1 (octet string) 1600321314816
    32: nvmeDeviceDescriptionEntry.16.2 (octet string) 1600321314816
    ***** SNMP QUERY FINISHED *****



## 4.24 logicalDriveProperty详细规格

### 4.24.1 功能说明

#### 4.24.1.1 父节点介绍

    逻辑盘信息节点，包括1个表量：逻辑盘的详细信息表（包括逻辑盘的RAID级别，状态，读写策略，大小，条带大小，一致性，检查状态等信息）

logicalDriveProperty表节点的 OID：iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).logicalDriveProperty(32)

#### 4.24.1.2 子节点介绍

**表量表**

节点 logicalDriveDescriptionEntry是描述表节点（logicalDriveDescriptionTable）组成成分的。

其OID 为： iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).zte(3902).ssp(2601).zteServer(15).zteBMC(1).logicalDriveProperty(32).logicalDriveDescriptionTable(50).logicalDriveDescriptionEntry(1) 

    提示：x表示逻辑盘编号（logicalDriveIndex）

| 节点名称                           | 节点 OID 实例                           | 描述                                                         | 类型          | 权限      |
| ---------------------------------- | --------------------------------------- | ------------------------------------------------------------ | ------------- | --------- |
| logicalDriveRAIDControllerIndex    | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.1.x  | Information about RAID controller index to which this logical drive belongs. | INTEGER       | read-only |
| logicalDriveIndex                  | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.2.x  | Information about logical drive index in current RAID controller. | INTEGER       | read-only |
| logicalDriveName                   | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.3.x  | Information about logical drive name.                        | DisplayString | read-only |
| logicalDriveId                     | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.4.x  | Information about logical drive Id.                          | INTEGER       | read-only |
| logicalDriveRAIDLevel              | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.5.x  | Information about logical drive level.<br />1: raid0(0) <br />2: raid1(1) <br />3: raid5(2) <br />4: raid6(3) <br />5: raidIE(4) <br />6: raid00(5) <br />7: raid10(6) <br />8: raid50(7) <br />9: raid60(8) <br />10: unknown(255) | INTEGER       | read-only |
| logicalDriveHealthState            | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.6.x  | Information about logical drive health status.<br/>1: ok(0) <br/>2: minor(2) <br/>3: major(3) <br/>4: critical(4) <br/>5: unknown(255) | INTEGER       | read-only |
| logicalDriveAvailabilityState      | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.7.x  | Information about logical drive availability status.<br />1: offline(0) <br />2: part-degraded(1) <br />3: degraded(2) <br />4: optimal(3) <br />5: unknown(255) | INTEGER       | read-only |
| logicalDriveSizeInGB               | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.8.x  | Information about logical drive size(unit: GB).              | INTEGER       | read-only |
| logicalDriveDefaultReadPolicy      | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.9.x  | Information about logical drive default read policy.<br />1: no-read-ahead(0) <br />2: read-ahead(1) <br />3: unknown(255) | INTEGER       | read-only |
| logicalDriveDefaultWritePolicy     | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.10.x | Information about logical drive default write policy.<br />1: write-through(0) <br />2: always-write-back(1) <br />3: write-back(2) <br />4: unknown(255) | INTEGER       | read-only |
| logicalDriveDefaultIOPolicy        | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.11.x | Information about logical drive default IO policy.<br />1: cached-IO(0) <br />2: direct-IO(1) <br />3: unknown(255) | INTEGER       | read-only |
| logicalDriveCurrentReadPolicy      | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.12.x | Information about logical drive read policy.<br />1: no-read-ahead(0) <br />2: read-ahead(1) <br />3: unknown(255) | INTEGER       | read-only |
| logicalDriveCurrentWritePolicy     | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.13.x | Information about logical drive write policy.<br />1: write-through(0) <br />2: always-write-back(1) <br />3: write-back(2) <br />4: unknown(255) | INTEGER       | read-only |
| logicalDriveCurrentIOPolicy        | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.14.x | Information about logical drive IO policy.<br />1: cached-IO(0) <br />2: direct-IO(1) <br />3: unknown(255) | INTEGER       | read-only |
| logicalDriveSpanDepth              | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.15.x | Information about logical drive span depth.<br />255 means unknown.     | INTEGER       | read-only |
| logicalDriveNumDrivePerSpan        | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.16.x | Information about logical drive number of drives per span.<br />255 means unknown.  | INTEGER       | read-only |
| logicalDriveStripeSizeInBytes      | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.17.x | Information about logical drive stripe size in bytes.        | INTEGER       | read-only |
| logicalDriveDiskCachePolicy        | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.18.x | Information about logical drive disk cache policy. <br />1: unchanged(0) <br />2: enabled(1) <br />3: disabled(2) <br />4: unknown(255)<br /> | INTEGER       | read-only |
| logicalDriveAccessPolicy           | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.19.x | Information about logical drive access policy. <br />1: read-write(0) <br />2: read-only(1) <br />3: blocked(2) <br />4: hidden(3) <br />5: unknown(255) | INTEGER       | read-only |
| logicalDriveInitState              | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.20.x | Information about logical drive init state. <br />1: no-init(0) <br />2: quick-init(1) <br />3: full-init(2) <br />4: unknown(255) | INTEGER       | read-only |
| logicalDriveBGIEnable              | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.21.x | Information about logical drive BGI state.<br />1: disabled(1) <br />2: enabled(2) <br />3: unknown(255) | INTEGER       | read-only |
| logicalDriveConsistencyCheckStatus | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.22.x | Information about logical drive consistency check status.<br />1: stopped(0) <br />2: in-progress(1) <br />3: unknown(255) | INTEGER       | read-only |
| logicalDriveMembersNumber          | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.23.x | Information about logical drive members number.              | INTEGER       | read-only |
| logicalDriveMemberList             | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.24.x | Information about logical drive members list.The value such as (1,2,3,4). 255 means the hard disk is removed or abnormal.| DisplayString | read-only |
| logicalDriveControllerOwnership    | 1.3.6.1.4.1.3902.2601.15.1.32.50.1.25.x | Information about RAID controller name to which this logical drive belongs.The value such as 'AVAGO MegaRAID SAS 9361-8i(1)', 1 is raid card pcie slot. | DisplayString | read-only |

### 4.24.2 查询操作约束

​        支持 get,walk,getnext,getbulk 操作

### 4.24.3 设置操作约束

​        不支持

### 4.24.4 使用示例
    ***** SNMP QUERY STARTED *****
    1: logicalDriveRAIDControllerIndex.1.1 (integer) 1
    2: logicalDriveIndex.1.1 (integer) 1
    3: logicalDriveName.1.1 (octet string) (zero-length) 
    4: logicalDriveId.1.1 (integer) 0
    5: logicalDriveRAIDLevel.1.1 (integer) raid1(1)
    6: logicalDriveHealthState.1.1 (integer) ok(0)
    7: logicalDriveAvailabilityState.1.1 (integer) optimal(3)
    8: logicalDriveSizeInGB.1.1 (integer) 5588
    9: logicalDriveDefaultReadPolicy.1.1 (integer) read-ahead(1)
    10: logicalDriveDefaultWritePolicy.1.1 (integer) always-write-back(1)
    11: logicalDriveDefaultIOPolicy.1.1 (integer) direct-IO(1)
    12: logicalDriveCurrentReadPolicy.1.1 (integer) read-ahead(1)
    13: logicalDriveCurrentWritePolicy.1.1 (integer) write-through(0)
    14: logicalDriveCurrentIOPolicy.1.1 (integer) direct-IO(1)
    15: logicalDriveSpanDepth.1.1 (integer) 1
    16: logicalDriveNumDrivePerSpan.1.1 (integer) 2
    17: logicalDriveStripeSizeInBytes.1.1 (integer) 262144
    18: logicalDriveDiskCachePolicy.1.1 (integer) disk-default(0)
    19: logicalDriveAccessPolicy.1.1 (integer) read-write(0)
    20: logicalDriveInitState.1.1 (integer) no-init(0)
    21: logicalDriveBGIEnable.1.1 (integer) enabled(2)
    22: logicalDriveConsistencyCheckStatus.1.1 (integer) stopped(0)
    23: logicalDriveMembersNumber.1.1 (integer) 2
    24: logicalDriveMemberList.1.1 (octet string) 12,14 [31.32.2C.31.34 (hex)]
    25: logicalDriveControllerOwnership.1.1 (octet string) AVAGO MegaRAID SAS 9361-8i(PCIe3) [41.56.41.47.4F.20.4D.65.67.61.52.41.49.44.20.53.41.53.20.39.33.36.31.2D.38.69.28.50.43.49.65.33.29 (hex)]
    ***** SNMP QUERY FINISHED *****



# 5 SNMP TRAP信息OID模式查询

适用于中兴服务器OID模式的TRAP信息，如表5-1 TRAP信息特性树所示。

表5-1 TRAP信息特性树

	提示：x表示具体告警Trap OID

| 节点OID | 节点名称                               | 子节点名称                                        |
| ------- | -------------------------------------- | ------------------------------------------------- |
| 3       | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.x   | CPU告警trap（zteTrapCPUEvent）                    |
| 4       | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.x   | 硬盘托架告警trap（zteTrapDiskBayEvent）           |
| 7       | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.x   | 系统单板告警trap（zteTrapSystemBoardEvent）       |
| 10      | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.x  | PSU告警trap（zteTrapPSUEvent）                    |
| 11      | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.x  | PCIe卡告警trap（zteTrapPCIeCardEvent）            |
| 16      | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.x  | 交换板告警trap（zteTrapswitchEvent）              |
| 19      | 1.3.6.1.4.1.3902.2601.15.1.500.2.19.x  | PDB告警trap（zteTrapPDBEvent）                    |
| 26      | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.x  | 硬盘告警trap（zteTrapDiskEvent）                  |
| 29      | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.x  | 风扇告警trap（zteTrapFANEvent）                   |
| 30      | 1.3.6.1.4.1.3902.2601.15.1.500.2.30.x  | 冷却装置告警trap（zteTrapCoolingUnitEvent）       |
| 32      | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.x  | 内存告警trap（zteTrapMemoryEvent）                |
| 34      | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.x  | bios系统告警trap（zteTrapBiosSystemEvent）        |
| 35      | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.x  | 操作系统告警trap（zteTrapOperationSystemEvent）   |
| 42      | 1.3.6.1.4.1.3902.2601.15.1.500.2.42.x  | 网络连接告警trap（zteTrapNetworkConnectionEvent） |
| 46      | 1.3.6.1.4.1.3902.2601.15.1.500.2.46.x  | BMC事件告警trap（zteTrapBMCEvent）                |
| 48      | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.x  | PCI总线告警trap（zteTrapPCIBusEvent）             |
| 55      | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.x  | 通风告警trap（zteTrapAirInletEvent）              |
| 56      | 1.3.6.1.4.1.3902.2601.15.1.500.2.56.x  | 系统固件告警trap（zteTrapSystemFirmwareEvent）    |
| 144     | 1.3.6.1.4.1.3902.2601.15.1.500.2.144.x | 挂耳告警trap（zteTrapMountingEarEvent）           |
| 145     | 1.3.6.1.4.1.3902.2601.15.1.500.2.145.x | Raid卡告警trap（zteTrapRaidCardEvent）            |
| 146     | 1.3.6.1.4.1.3902.2601.15.1.500.2.146.x | PCIe网卡告警trap（zteTrapPCIeNetCardEvent）       |
| 150     | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.x | 板载网卡告警trap（zteTrapOnboardNetCardEvent）    |
| 151     | 1.3.6.1.4.1.3902.2601.15.1.500.2.151.x | OCP网卡告警trap（zteTrapOCPNetCardEvent）         |
| 152     | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.x | 环境湿度告警trap（zteTrapENVHUMIEvent）           |
| 160     | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.x | 主板告警trap（zteTrapMainBoardEvent）             |
| 224     | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.x | GPU基板告警trap（zteTrapGPUUBBEvent）             |
| 225     | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.x | 加速卡告警trap（zteTrapAccelerationCardEvent）    |
| 226     | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.x | GPU基板光模块告警trap（zteTrapGPUUBBOPTEvent）    |
| 228     | 1.3.6.1.4.1.3902.2601.15.1.500.2.228.x | CDU告警trap（zteTrapCDUEvent）                    |
| 254     | 1.3.6.1.4.1.3902.2601.15.1.500.2.254.x | Trap测试（zteTrapTrapTestEvent）                  |

每个TRAP OID上报的变量绑定信息，如表5-2 TRAP OID的变量绑定列表所示。

表5-2 TRAP OID变量绑定列表

| 变量绑定中文描述 | 变量绑定名称定义   | 变量绑定英文描述          | 变量绑定类型 | 取值                                                               |默认变量绑定OID |
| ---------------- | ------------------ | ------------------------- | ------------ | ------------------------------------------------------------------ | -------------------------------- |
| 事件序号         | zteTrapSeq         | Trap Seqence No.          | 整型         | 从1开始                                                            |1.3.6.1.4.1.3902.2601.15.1.500.1.1 |
| 产生时间         | zteTrapTime        | Trap Time                 | 字符串       | YYYY-MM-DDT hh:mm:ss                                               |1.3.6.1.4.1.3902.2601.15.1.500.1.2 |
| 事件主体         | zteTrapEntity      | Trap Entity               | 字符串       | 主体类型+主体实例号，如PSU1，FAN2                                  |1.3.6.1.4.1.3902.2601.15.1.500.1.3 |
| 事件传感器名称   | zteTrapSensorName  | Trap Sensor Name          | 字符串       | SEL类型的事件，需要由事件管理模块传递，非SEL类型的事件，可以填为空 |1.3.6.1.4.1.3902.2601.15.1.500.1.4 |
| 严重性级别       | zteTrapSeverity    | 0 -ok <br />1-inform<br />2-minor<br />3-major <br />4-critical | 整型        |1: ok(0)<br /> 2: inform(1)<br />3: minor(2)<br />4: major(3) <br />5: critical(4) |1.3.6.1.4.1.3902.2601.15.1.500.1.5 |
| 事件描述         | zteTrapDescription | Trap Description          | 字符串       | 业务模块上报的description字段                                      |1.3.6.1.4.1.3902.2601.15.1.500.1.6 |
| 事件主机标识     | zteTrapIdentifier  | Trap Identifier           | 字符串       | -                                                                  |1.3.6.1.4.1.3902.2601.15.1.500.1.7 |
| 事件状态         | zteTrapStatus      | Trap Status               | 整型         | 1: assert(0) <br />2: deassert(1)                                        |1.3.6.1.4.1.3902.2601.15.1.500.1.8 |
| 事件主体的SN     | zteTrapEntitySN    | Trap Entity Serial Number | 字符串       | -                                                                  |1.3.6.1.4.1.3902.2601.15.1.500.1.9 |
| 事件附加信息     | zteTrapAddInfo     | Trap Add Infomation       | 字符串       | -                                                                  |1.3.6.1.4.1.3902.2601.15.1.500.1.10 |

## 5.1 CPU告警trap

本小节介绍CPU告警trap如下表：

| 告警类型ID/告警码  | 告警Trap OID                              | 告警描述                                                     |
| ------------------ | ----------------------------------------- | ------------------------------------------------------------ |
| 18    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.18  | CPU温度高温关机 |
| 19    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.19  | CPU使用率超出阈值 |
| 65799    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.65799  | CPU温度高于轻微告警阈值 |
| 65801    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.65801  | CPU温度高于严重告警阈值 |
| 65803    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.65803  | CPU温度高于紧急告警阈值 |
| 66048    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.66048  | CPU电压低于轻微告警阈值 |
| 66050    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.66050  | CPU电压低于严重告警阈值 |
| 66052    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.66052  | CPU电压低于紧急告警阈值 |
| 66055    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.66055  | CPU电压高于轻微告警阈值 |
| 66057    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.66057  | CPU电压高于严重告警阈值 |
| 66059    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.66059  | CPU电压高于紧急告警阈值 |
| 66313 | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.66313 | CPU电流高于严重告警阈值 |
| 198401    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.198401  | CPU过热 |
| 7276288    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276288  | CPU系统错误 |
| 7276289    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276289  | CPU超温 |
| 7276290    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276290  | CPU内建自测试失败 |
| 7276291    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276291  | CPU POST失败挂死 |
| 7276292    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276292  | CPU初始化失败 |
| 7276293    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276293  | CPU配置错误 |
| 7276294 | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276294 | SM BIOS不可纠正CPU复合错误 |
| 7276295 | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276295 | CPU在位 |
| 7276296    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276296  | CPU禁用 |
| 7276298    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276298  | CPU自动节流 |
| 7276299    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276299  | CPU机器检查异常 |
| 7276300    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276300  | CPU纠错自检异常 |
| 7276301    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.7276301  | CPU内部错误 |
| 8388627    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8388627  | CPU使用率超出阈值恢复 |
| 8454407    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8454407  | CPU温度高于轻微告警阈值恢复 |
| 8454409    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8454409  | CPU温度高于严重告警阈值恢复 |
| 8454411    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8454411  | CPU温度高于紧急告警阈值恢复 |
| 8454656    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8454656  | CPU电压低于轻微告警阈值恢复 |
| 8454658    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8454658  | CPU电压低于严重告警阈值恢复 |
| 8454660    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8454660  | CPU电压低于紧急告警阈值恢复 |
| 8454663    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8454663  | CPU电压高于轻微告警阈值恢复 |
| 8454665    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8454665  | CPU电压高于严重告警阈值恢复 |
| 8454667    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8454667  | CPU电压高于紧急告警阈值恢复 |
| 8454921 | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8454921 | CPU电流高于严重告警阈值恢复 |
| 8587009    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.8587009  | CPU过热恢复 |
| 15664896    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664896  | CPU系统错误恢复 |
| 15664897    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664897  | CPU超温恢复 |
| 15664898    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664898  | CPU内建自测试失败恢复 |
| 15664899    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664899  | CPU POST失败挂死恢复 |
| 15664900    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664900  | CPU初始化失败恢复 |
| 15664901    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664901  | CPU配置错误恢复 |
| 15664902 | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664902 | SM BIOS不可纠正CPU复合错误恢复 |
| 15664903 | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664903 | CPU不在位 |
| 15664904    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664904  | CPU禁用恢复 |
| 15664906    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664906  | CPU自动节流恢复 |
| 15664907    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664907  | CPU机器检查异常恢复 |
| 15664908    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664908  | CPU纠错自检异常恢复 |
| 15664909    | 1.3.6.1.4.1.3902.2601.15.1.500.2.3.15664909  | CPU内部错误恢复 |

## 5.2 硬盘托架告警trap

本小节介绍硬盘托架告警trap如下表：

| 告警类型ID/告警码     | 告警Trap OID                              | 告警描述                                                     |
| --------------------- | ----------------------------------------- | ------------------------------------------------------------ |
| 65799    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.65799  | 硬盘温度高于高轻微告警阈值 |
| 65801    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.65801  | 硬盘温度高于高严重告警阈值 |
| 65803    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.65803  | 硬盘温度高于高紧急告警阈值 |
| 7277824    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.7277824  | 硬盘在线 |
| 7277825    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.7277825  | 硬盘驱动故障 |
| 7277826    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.7277826  | 硬盘故障预警 |
| 7277829    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.7277829  | 硬盘处于降级的逻辑阵列 |
| 7277830    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.7277830  | 硬盘处于离线的逻辑阵列 |
| 7277838    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.7277838  | 硬盘寿命预警 |
| 8454407    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.8454407  | 硬盘温度高于高轻微告警阈值恢复 |
| 8454409    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.8454409  | 硬盘温度高于高严重告警阈值恢复 |
| 8454411    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.8454411  | 硬盘温度高于高紧急告警阈值恢复 |
| 15666432    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.15666432  | 硬盘离线 |
| 15666433    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.15666433  | 硬盘驱动故障恢复 |
| 15666434    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.15666434  | 硬盘故障预警恢复 |
| 15666437    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.15666437  | 硬盘处于降级的逻辑阵列恢复 |
| 15666438    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.15666438  | 硬盘处于离线的逻辑阵列恢复 |
| 15666446    | 1.3.6.1.4.1.3902.2601.15.1.500.2.4.15666446  | 硬盘寿命预警恢复 |

## 5.3 系统单板告警trap

本小节介绍系统单板告警trap如下表：

| 告警类型ID/告警码     | 告警Trap OID                              | 告警描述                                                     |
| --------------------- | ----------------------------------------- | ------------------------------------------------------------ |
| 65799    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.65799  | 桥片温度高于轻微告警阈值 |
| 65801    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.65801  | 桥片温度高于严重告警阈值 |
| 65803    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.65803  | 桥片温度高于紧急告警阈值 |
| 66048    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.66048  | 节点54V输入电压低于低轻微告警阈值 |
| 66050    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.66050  | 节点54V输入电压低于低严重告警阈值 |
| 66055    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.66055  | 节点54V输入电压高于高轻微告警阈值 |
| 66057    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.66057  | 节点54V输入电压高于高严重告警阈值 |
| 464134    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.464134  | 系统处于不可恢复故障状态 |
| 465153    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.465153  | ME状态异常 |
| 7275776    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7275776  | 机箱盖打开 |
| 7276545 | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7276545 | 系统异常掉电 |
| 7278336    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7278336  | 系统固件错误 |
| 7278337    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7278337  | 系统固件挂起 |
| 7278594    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7278594  | 系统事件日志清除 |
| 7278595    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7278595  | 所有事件日志禁用 |
| 7278596    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7278596  | 系统事件日志已满 |
| 7278597    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7278597  | 系统事件日志几乎已满 |
| 7279106    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7279106  | 未知的系统硬件故障 |
| 7279616    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7279616  | 电源按键按下 |
| 7279618    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7279618  | 主机重启按键按下 |
| 7279632    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7279632  | 电源按键误触 |
| 7281920    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7281920  | 系统开机 |
| 7281921    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7281921  | 系统硬重启 |
| 7281922    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7281922  | 系统热重启 |
| 7281923    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7281923  | 用户要求从网卡启动 |
| 7281925    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7281925  | 操作系统/运行时软件硬重启 |
| 7281926    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7281926  | 操作系统/运行时软件热重启 |
| 7282691    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7282691  | 系统正常关机 |
| 7283200    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7283200  | 系统正常工作 |
| 7283205    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7283205  | 系统软关机 |
| 7283214    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7283214  | 系统状态未知 |
| 7283456    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7283456  | 系统看门狗超时 |
| 7283457    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7283457  | 系统看门狗超时重启 |
| 7283458    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7283458  | 系统看门狗超时关机 |
| 7283459    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7283459  | 系统看门狗超时关机再开机 |
| 7283464    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7283464  | 系统看门狗超时中断 |
| 7284993    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.7284993  | CMOS异常 |
| 8454407    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.8454407  | 桥片温度高于轻微告警阈值恢复 |
| 8454409    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.8454409  | 桥片温度高于严重告警阈值恢复 |
| 8454411    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.8454411  | 桥片温度高于紧急告警阈值恢复 |
| 8454656    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.8454656  | 节点54V输入电压低于低轻微告警阈值恢复 |
| 8454658    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.8454658  | 节点54V输入电压低于低严重告警阈值恢复 |
| 8454663    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.8454663  | 节点54V输入电压高于高轻微告警阈值恢复 |
| 8454665    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.8454665  | 节点54V输入电压高于高严重告警阈值恢复 |
| 8852742    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.8852742  | 系统处于不可恢复故障状态恢复 |
| 8853761    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.8853761  | ME状态异常恢复 |
| 15664384    | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.15664384  | 机箱盖打开恢复 |
| 15665153 | 1.3.6.1.4.1.3902.2601.15.1.500.2.7.15665153 | 系统异常掉电恢复 |

## 5.4 PSU告警trap

本小节介绍PSU告警trap如下表：

| 告警类型ID/告警码           | 告警Trap OID                    | 告警描述                                            |
| --------------------------- | ------------------------------- | --------------------------------------------------- |
| 17    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.17  | 电源输入欠压故障 |
| 18    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.18  | 电源输入欠压警告 |
| 19    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.19  | 电源输入过压故障 |
| 20    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.20  | 电源输入过压警告 |
| 21    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.21  | 电源输出欠压故障 |
| 22    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.22  | 电源输出欠压警告 |
| 23    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.23  | 电源输出过压故障 |
| 24    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.24  | 电源输出过压警告 |
| 25    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.25  | 电源输出欠流故障 |
| 26    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.26  | 电源输出过流故障 |
| 27    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.27  | 电源输出过流警告 |
| 28    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.28  | 电源过温故障 |
| 29    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.29  | 电源过温警告 |
| 30    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.30  | 电源风扇1故障 |
| 31    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.31 | 电源风扇1警告 |
| 32    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.32  | 电源风扇2故障 |
| 33    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.33  | 电源风扇2警告 |
| 34    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.34  | 系统功率超过告警阈值 |
| 65799    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.65799  | 电源温度高于高轻微告警阈值 |
| 65801    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.65801  | 电源温度高于高严重告警阈值 |
| 66050    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.66050  | 电源电压低于低严重告警阈值 |
| 66057    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.66057  | 电源电压高于高严重告警阈值 |
| 198913    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.198913  | 产生异常上下电 |
| 263169 | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.263169 | 电源风扇预测故障声明 |
| 722945    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.722945  | 电源冗余丢失 |
| 7276544    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.7276544  | 电源模块插入 |
| 7276545    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.7276545  | 检测到电源故障 |
| 7276546    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.7276546  | 电源故障预警 |
| 7276547    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.7276547  | 电源交流供电中断 |
| 7276548    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.7276548  | 电源输入丢失 |
| 7276550    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.7276550  | 电源配置错误 |
| 8388625    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388625  | 电源输入欠压故障恢复 |
| 8388626    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388626  | 电源输入欠压警告恢复 |
| 8388627    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388627  | 电源输入过压故障恢复 |
| 8388628    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388628  | 电源输入过压警告恢复 |
| 8388629    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388629  | 电源输出欠压故障恢复 |
| 8388630    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388630  | 电源输出欠压警告恢复 |
| 8388631    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388631  | 电源输出过压故障恢复 |
| 8388632    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388632  | 电源输出过压警告恢复 |
| 8388633    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388633  | 电源输出欠流故障恢复 |
| 8388634    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388634  | 电源输出过流故障恢复 |
| 8388635    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388635  | 电源输出过流警告恢复 |
| 8388636    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388636  | 电源过温故障恢复 |
| 8388637    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388637  | 电源过温警告恢复 |
| 8388638    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388638  | 电源风扇1故障恢复 |
| 8388639    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388639 | 电源风扇1警告恢复 |
| 8388640    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388640  | 电源风扇2故障恢复 |
| 8388641    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388641  | 电源风扇2警告恢复 |
| 8388642    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8388642  | 系统功率超过告警阈值恢复 |
| 8454407    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8454407  | 电源温度高于高轻微告警阈值恢复 |
| 8454409    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8454409  | 电源温度高于高严重告警阈值恢复 |
| 8454658    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8454658  | 电源电压低于低严重告警阈值恢复 |
| 8454665    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8454665  | 电源电压高于高严重告警阈值恢复 |
| 8587521    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.8587521  | 产生异常上下电恢复 |
| 8651777 | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.8651777 | 电源风扇预测故障声明恢复 |
| 9111553    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.9111553  | 电源冗余丢失恢复 |
| 15665152    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.15665152  | 电源模块拔出 |
| 15665153    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.15665153  | 检测到电源故障恢复 |
| 15665154    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.15665154  | 电源故障预警恢复 |
| 15665155    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.15665155  | 电源交流供电中断恢复 |
| 15665156    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.15665156  | 电源输入丢失恢复 |
| 15665158    | 1.3.6.1.4.1.3902.2601.15.1.500.2.10.15665158  | 电源配置错误恢复 |

## 5.5 PCIe卡告警trap

本小节介绍PCIe卡告警trap如下表：

| 告警类型ID/告警码           | 告警Trap OID                    | 告警描述                                            |
| --------------------------- | ------------------------------- | --------------------------------------------------- |
| 65792    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.65792  | 温度低于低轻微告警阈值 |
| 65794    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.65794  | 温度低于低严重告警阈值 |
| 65796    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.65796  | 温度低于低紧急告警阈值 |
| 65799    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.65799  | 温度高于高轻微告警阈值 |
| 65801    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.65801  | 温度高于高严重告警阈值 |
| 65803    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.65803  | 温度高于高紧急告警阈值 |
| 66048    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.66048  | 电压低于低轻微告警阈值 |
| 66055    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.66055  | 电压高于高轻微告警阈值 |
| 66313    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.66313  | 电流高于高严重告警阈值 |
| 7277569    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.7277569  | 内存不可纠正错误 |
| 7281409    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.7281409  | GPU线接错 |
| 8454400    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.8454400  | 温度低于低轻微告警阈值恢复 |
| 8454402    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.8454402  | 温度低于低严重告警阈值恢复 |
| 8454404    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.8454404  | 温度低于低紧急告警阈值恢复 |
| 8454407    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.8454407  | 温度高于高轻微告警阈值恢复 |
| 8454409    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.8454409  | 温度高于高严重告警阈值恢复 |
| 8454411    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.8454411  | 温度高于高紧急告警阈值恢复 |
| 8454656    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.8454656  | 电压低于低轻微告警阈值恢复 |
| 8454663    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.8454663  | 电压高于高轻微告警阈值恢复 |
| 8454921    | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.8454921  | 电流高于高严重告警阈值恢复 |
| 15666177   | 1.3.6.1.4.1.3902.2601.15.1.500.2.11.15666177  | 内存不可纠正错误恢复 |

## 5.6 PDB告警trap

本小节介绍PDB告警trap如下表：

| 告警类型ID/告警码 | 告警Trap OID                                | 告警描述                      |
| ----------------- | ------------------------------------------- | ----------------------------- |
| 65799             | 1.3.6.1.4.1.3902.2601.15.1.500.2.19.65799   | PDB温度高于高轻微告警阈值     |
| 65801             | 1.3.6.1.4.1.3902.2601.15.1.500.2.19.65801   | PDB温度高于高严重告警阈值     |
| 65803             | 1.3.6.1.4.1.3902.2601.15.1.500.2.19.65803   | PDB温度高于高紧急告警阈值     |
| 8454407           | 1.3.6.1.4.1.3902.2601.15.1.500.2.19.8454407 | PDB温度高于高轻微告警阈值恢复 |
| 8454409           | 1.3.6.1.4.1.3902.2601.15.1.500.2.19.8454409 | PDB温度高于高严重告警阈值恢复 |
| 8454411           | 1.3.6.1.4.1.3902.2601.15.1.500.2.19.8454411 | PDB温度高于高紧急告警阈值恢复 |

## 5.7 硬盘告警trap

本小节介绍硬盘告警trap如下表：

| 告警类型ID/告警码           | 告警Trap OID                    | 告警描述                                            |
| --------------------------- | ------------------------------- | --------------------------------------------------- |
| 19    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.19  | 硬盘SMART异常 |
| 20    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.20  | 硬盘温度高于严重告警阈值 |
| 21    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.21  | 硬盘寿命预警 |
| 22    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.22  | 硬盘丢失 |
| 23    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.23  | 硬盘有外部配置 |
| 24    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.24  | 硬盘故障 |
| 25    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.25  | 硬盘温度高于紧急告警阈值 |
| 26    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.26  | 硬盘使用率超出阈值 |
| 129    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.129  | 硬盘RAID阵列部分降级 |
| 130    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.130  | 硬盘RAID阵列降级 |
| 131    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.131  | 硬盘RAID阵列离线 |
| 8388627    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.8388627  | 硬盘SMART异常恢复 |
| 8388628    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.8388628  | 硬盘温度高于严重告警阈值恢复 |
| 8388629    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.8388629  | 硬盘寿命预警恢复 |
| 8388630    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.8388630  | 硬盘丢失恢复 |
| 8388631    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.8388631  | 硬盘有外部配置恢复 |
| 8388632    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.8388632  | 硬盘故障恢复 |
| 8388633    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.8388633  | 硬盘温度高于紧急告警阈值恢复 |
| 8388634    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.8388634  | 硬盘使用率超出阈值恢复 |
| 8388737    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.8388737  | 硬盘RAID阵列部分降级恢复 |
| 8388738    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.8388738  | 硬盘RAID阵列降级恢复 |
| 8388739    | 1.3.6.1.4.1.3902.2601.15.1.500.2.26.8388739  | 硬盘RAID阵列离线恢复 |

## 5.8 风扇告警trap

本小节介绍风扇告警trap如下表：

| 告警类型ID/告警码           | 告警Trap OID                    | 告警描述                                            |
| --------------------------- | ------------------------------- | --------------------------------------------------- |
| 19    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.19  | 风扇丢失关机 |
| 66050    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.66050  | 风扇电压低于严重告警阈值 |
| 66057    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.66057  | 风扇电压高于严重告警阈值 |
| 66560    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.66560  | 风扇转速低于轻微告警阈值 |
| 66562    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.66562  | 风扇转速低于严重告警阈值 |
| 66567    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.66567  | 风扇转速高于轻微告警阈值 |
| 66569    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.66569  | 风扇转速高于严重告警阈值 |
| 459777    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.459777  | 风扇状态异常 |
| 525312    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.525312  | 风扇设备离线 |
| 525313    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.525313  | 风扇设备在线 |
| 721921    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.721921  | 风扇冗余丢失 |
| 8454658    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.8454658  | 风扇电压低于严重告警阈值恢复 |
| 8454665    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.8454665  | 风扇电压高于严重告警阈值恢复 |
| 8455168    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.8455168  | 风扇转速低于轻微告警阈值恢复 |
| 8455170    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.8455170  | 风扇转速低于严重告警阈值恢复 |
| 8455175    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.8455175  | 风扇转速高于轻微告警阈值恢复 |
| 8455177    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.8455177  | 风扇转速高于严重告警阈值恢复 |
| 8848385    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.8848385  | 风扇状态异常恢复 |
| 8913920    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.8913920  | 风扇设备离线恢复 |
| 8913921    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.8913921  | 风扇设备离线 |
| 9110529    | 1.3.6.1.4.1.3902.2601.15.1.500.2.29.9110529  | 风扇冗余丢失恢复 |

## 5.9 冷却装置告警trap

本小节介绍冷却装置告警trap如下表：

| 告警类型ID/告警码                  | 告警Trap OID                       | 告警描述                                            |
| ---------------------------------- | ---------------------------------- | --------------------------------------------------- |
| 20    | 1.3.6.1.4.1.3902.2601.15.1.500.2.30.20  | 液冷系统漏液 |
| 21    | 1.3.6.1.4.1.3902.2601.15.1.500.2.30.21  | 液冷系统漏液检测线状态异常 |
| 22    | 1.3.6.1.4.1.3902.2601.15.1.500.2.30.22  | 液冷服务器漏液检测卡不在位 |
| 23    | 1.3.6.1.4.1.3902.2601.15.1.500.2.30.23  | 非液冷服务器但是漏液检测卡在位 |
| 24    | 1.3.6.1.4.1.3902.2601.15.1.500.2.30.24  | 液冷系统漏液检测线不在位 |
| 242945    | 1.3.6.1.4.1.3902.2601.15.1.500.2.30.242945  | 液冷系统漏液 |
| 465153    | 1.3.6.1.4.1.3902.2601.15.1.500.2.30.465153  | 液冷系统漏液 |
| 8388630    | 1.3.6.1.4.1.3902.2601.15.1.500.2.30.8388630  | 液冷服务器漏液检测卡不在位恢复 |
| 8388631    | 1.3.6.1.4.1.3902.2601.15.1.500.2.30.8388631  | 非液冷服务器但是漏液检测卡在位恢复 |

## 5.10 内存告警trap

本小节介绍内存告警trap如下表：

| 告警类型ID/告警码                  | 告警Trap OID                       | 告警描述                                            |
| ---------------------------------- | ---------------------------------- | --------------------------------------------------- |
| 17    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.17  | 内存使用率超出阈值 |
| 65799    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.65799  | 内存温度高于轻微告警阈值 |
| 65801    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.65801  | 内存温度高于严重告警阈值 |
| 65803    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.65803  | 内存温度高于紧急告警阈值 |
| 7277568    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277568  | 内存可纠正错误 |
| 7277569    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277569  | 内存不可纠正错误 |
| 7277570    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277570  | 内存奇偶校验错误 |
| 7277571    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277571  | 内存清理失败（标记位） |
| 7277572    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277572  | 内存设备禁用 |
| 7277573    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277573  | 内存可纠正错误日志记录达到限制 |
| 7277574 | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277574 | 内存在位 |
| 7277575    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277575  | 内存配置错误 |
| 7277577    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277577  | 内存自动节流 |
| 7277578    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277578  | 内存严重超温 |
| 7277579 | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277579 | 内存PMIC错误 |
| 7277581    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277581  | 内存故障预警 |
| 7277582    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.7277582  | 内存隔离 |
| 265217    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.265217    | 内存故障预警 |
| 8388625    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.8388625  | 内存使用率超出阈值恢复 |
| 8454407    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.8454407  | 内存温度高于轻微告警阈值恢复 |
| 8454409    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.8454409  | 内存温度高于严重告警阈值恢复 |
| 8454411    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.8454411  | 内存温度高于紧急告警阈值恢复 |
| 15666176    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666176  | 内存可纠正错误恢复 |
| 15666177    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666177  | 内存不可纠正错误恢复 |
| 15666178    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666178  | 内存奇偶校验错误恢复 |
| 15666179    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666179  | 内存清理失败（标记位）恢复 |
| 15666180    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666180  | 内存设备禁用恢复 |
| 15666181    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666181  | 内存可纠正错误日志记录达到限制恢复 |
| 15666182 | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666182 | 内存不在位 |
| 15666183    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666183  | 内存配置错误恢复 |
| 15666185    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666185  | 内存自动节流恢复 |
| 15666186    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666186  | 内存严重超温恢复 |
| 15666187 | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666187 | 内存PMIC错误恢复 |
| 15666189    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666189  | 内存故障预警恢复 |
| 15666190    | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.15666190  | 内存隔离恢复 |
| 8653825     | 1.3.6.1.4.1.3902.2601.15.1.500.2.32.8653825   | 内存故障预警恢复 |

## 5.11 Bios系统告警trap

本小节介绍Bios系统告警trap如下表：

| 告警类型ID/告警码                  | 告警Trap OID                       | 告警描述                                            |
| ---------------------------------- | ---------------------------------- | --------------------------------------------------- |
| 198401    | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.198401  | CPU微码加载失败 |
| 7276033    | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.7276033  | 输入多次错误密码 |
| 7278336    | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.7278336  | 系统固件错误 |
| 7278337    | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.7278337  | 系统固件挂起 |
| 7278338    | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.7278338  | POST错误（用户鉴权） |
| 7282176    | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.7282176  | 无可引导设备 |
| 7285505    | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.7285505  | 固件(BMC/BIOS)更新 |
| 7285511    | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.7285511  | 固件(BMC/BIOS)更新成功 |
| 7285767    | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.7285767  | FRU通信丢失 |
| 8587009    | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.8587009  | CPU微码加载失败恢复 |
| 15674119    | 1.3.6.1.4.1.3902.2601.15.1.500.2.34.15674119  | 固件(BMC/BIOS)更新失败 |

## 5.12 操作系统告警trap

本小节介绍操作系统告警trap如下表：

| 告警类型ID/告警码 | 告警Trap OID                                  | 告警描述              |
| ----------------- | --------------------------------------------- | --------------------- |
| 7282432           | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.7282432   | 软盘引导完成   |
| 7282433           | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.7282433   | 硬盘引导完成   |
| 7282434           | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.7282434   | 网络引导完成   |
| 7282435           | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.7282435   | 诊断引导完成   |
| 7282436           | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.7282436   | 光盘引导完成   |
| 7282437           | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.7282437   | ROM引导完成   |
| 7282438           | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.7282438   | 引导完成-未指定设备   |
| 7282439           | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.7282439   | 基础系统/虚机安装开始   |
| 7282440           | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.7282440   | 基础系统/虚机安装完成   |
| 7282441           | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.7282441   | 基础系统/虚机安装停止   |
| 7282442           | 1.3.6.1.4.1.3902.2601.15.1.500.2.35.7282442   | 基础系统/虚机安装失败   |


## 5.13 网络连接告警trap

本小节介绍网络连接告警trap如下表：

| 告警类型ID/告警码                  | 告警Trap OID                       | 告警描述                                            |
| ---------------------------------- | ---------------------------------- | --------------------------------------------------- |
| 7275780    | 1.3.6.1.4.1.3902.2601.15.1.500.2.42.7275780  | 局域网相关业务中断 |
| 15664388    | 1.3.6.1.4.1.3902.2601.15.1.500.2.42.15664388  | 局域网相关业务中断恢复 |

## 5.14 BMC事件告警trap

本小节介绍BMC事件告警trap如下表：

| 告警类型ID/告警码 | 告警Trap OID                                  | 告警描述      |
| ------------------|---------------------------------------------- | --------------|
| 17                | 1.3.6.1.4.1.3902.2601.15.1.500.2.46.17        | NTP同步失败   |
| 7281920           | 1.3.6.1.4.1.3902.2601.15.1.500.2.46.7281920   | BMC启动       |
| 7281921           | 1.3.6.1.4.1.3902.2601.15.1.500.2.46.7281921   | BMC重启       |
| 8388625                | 1.3.6.1.4.1.3902.2601.15.1.500.2.46.8388625        | NTP同步失败恢复   |

## 5.15 PCI总线告警trap

本小节介绍PCI总线告警trap如下表：

| 告警类型ID/告警码           | 告警Trap OID                       | 告警描述                                            |
| --------------------------- | ---------------------------------- | --------------------------------------------------- |
| 7279364    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.7279364  | PCI奇偶校验错误 |
| 7279365    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.7279365  | PCI系统错误 |
| 7279367    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.7279367  | PCI总线可纠正错误 |
| 7279368    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.7279368  | PCI总线不可纠正错误 |
| 7279370    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.7279370  | PCI总线致命错误 |
| 7279371    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.7279371  | PCI总线降频 |
| 7279387    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.7279387  | PCI总线降带宽 |
| 7279390    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.7279390  | PCIe模式改变 |
| 7279406    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.7279406  | PCIe模式错误 |
| 7279374    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.7279374  | PCIe发生EDPC事件 |
| 15667972    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.15667972  | PCI奇偶校验错误恢复 |
| 15667973    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.15667973  | PCI系统错误恢复 |
| 15667975    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.15667975  | PCI总线可纠正错误恢复 |
| 15667976    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.15667976  | PCI总线不可纠正错误恢复 |
| 15667978    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.15667978  | PCI总线致命错误恢复 |
| 15667979    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.15667979  | PCI总线降频恢复 |
| 15667995    | 1.3.6.1.4.1.3902.2601.15.1.500.2.48.15667995  | PCI总线降带宽恢复 |

## 5.16 通风告警trap

本小节介绍通风告警trap如下表：

| 告警类型ID/告警码 | 告警Trap OID                          | 告警描述              |
| ------------------|-------------------------------------- | --------------------- |
| 1                 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.1 | 入风口温度获取失败    |
| 65799 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.65799 | 入风口温度高于高轻微告警阈值 |
| 65801 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.65801 | 入风口温度高于高严重告警阈值 |
| 65803 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.65803 | 入风口温度高于高紧急告警阈值 |
| 65792 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.65792 | 入风口温度低于低轻微告警阈值 |
| 65794 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.65794 | 入风口温度低于低严重告警阈值 |
| 65796 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.65796 | 入风口温度低于低紧急告警阈值 |
| 8388609                 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.8388609 | 入风口温度获取失败恢复    |
| 8454407 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.8454407 | 入风口温度高于高轻微告警阈值恢复 |
| 8454409 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.8454409 | 入风口温度高于高严重告警阈值恢复 |
| 8454411 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.8454411 | 入风口温度高于高紧急告警阈值恢复 |
| 8454400 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.8454400 | 入风口温度低于低轻微告警阈值恢复 |
| 8454402 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.8454402 | 入风口温度低于低严重告警阈值恢复 |
| 8454404 | 1.3.6.1.4.1.3902.2601.15.1.500.2.55.8454404 | 入风口温度低于低紧急告警阈值恢复 |

## 5.17 系统告警trap

本小节介绍系统告警trap如下表：

| 告警类型ID/告警码           | 告警Trap OID                    | 告警描述                                            |
| --------------------------- | ------------------------------- | --------------------------------------------------- |
| 7278336    | 1.3.6.1.4.1.3902.2601.15.1.500.2.56.7278336  | DPU SOC POST超时 |
| 7278337    | 1.3.6.1.4.1.3902.2601.15.1.500.2.56.7278337  | DPU BIOS POST超时 |
| 7278338    | 1.3.6.1.4.1.3902.2601.15.1.500.2.56.7278338  | 开始等待DPU POST |
| 15666946    | 1.3.6.1.4.1.3902.2601.15.1.500.2.56.15666946  | 等待DPU POST成功 |

## 5.18 挂耳告警trap

本小节介绍挂耳告警trap如下表：

| 告警类型ID/告警码           | 告警Trap OID                    | 告警描述                                            |
| --------------------------- | ------------------------------- | --------------------------------------------------- |
| 17    | 1.3.6.1.4.1.3902.2601.15.1.500.2.144.17  | 机房环境温度高温关机 |
| 32    | 1.3.6.1.4.1.3902.2601.15.1.500.2.144.32  | 左挂耳功能失效 |

## 5.19 Raid卡告警trap

本小节介绍Raid卡告警trap如下表：

| 告警类型ID/告警码           | 告警Trap OID                    | 告警描述                                            |
| --------------------------- | ------------------------------- | --------------------------------------------------- |
| 18    | 1.3.6.1.4.1.3902.2601.15.1.500.2.145.18  | RAID卡BBU温度高 |
| 19    | 1.3.6.1.4.1.3902.2601.15.1.500.2.145.19  | RAID卡BBU电压低 |
| 8388626    | 1.3.6.1.4.1.3902.2601.15.1.500.2.145.8388626  | RAID卡BBU温度高恢复 |
| 8388627    | 1.3.6.1.4.1.3902.2601.15.1.500.2.145.8388627  | RAID卡BBU电压低恢复 |

## 5.20 PCIe网卡告警trap

本小节介绍PCIe网卡告警trap如下表：

| 告警类型ID/告警码                  | 告警Trap OID                       | 告警描述                                            |
| ---------------------------------- | ---------------------------------- | --------------------------------------------------- |
| 17    | 1.3.6.1.4.1.3902.2601.15.1.500.2.146.17  | PCIe网口链路断开 |
| 8388625    | 1.3.6.1.4.1.3902.2601.15.1.500.2.146.8388625  | PCIe网口链路连接 |

## 5.21 板载网卡告警trap

本小节介绍板载网卡告警trap如下表：

| 告警类型ID/告警码 | 告警Trap OID                                | 告警描述                          |
| ------------------| ------------------------------------------- | ----------------------------------|
| 65792             | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.65792  | 板载网卡温度低于低轻微告警阈值     |
| 65794             | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.65794  | 板载网卡温度低于低严重告警阈值     |
| 65796             | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.65796  | 板载网卡温度低于低紧急告警阈值     |
| 65799             | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.65799  | 板载网卡温度高于高轻微告警阈值     |
| 65801             | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.65801  | 板载网卡温度高于高严重告警阈值     |
| 65803             | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.65803  | 板载网卡温度高于高紧急告警阈值     |
| 8454400           | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.8454400| 板载网卡温度低于低轻微告警阈值恢复 |
| 8454402           | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.8454402| 板载网卡温度低于低严重告警阈值恢复 |
| 8454404           | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.8454404| 板载网卡温度低于低紧急告警阈值恢复 |
| 8454407           | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.8454407| 板载网卡温度高于高轻微告警阈值恢复 |
| 8454409           | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.8454409| 板载网卡温度高于高严重告警阈值恢复 |
| 8454411           | 1.3.6.1.4.1.3902.2601.15.1.500.2.150.8454411| 板载网卡温度高于高紧急告警阈值恢复 |

## 5.22 OCP网卡告警trap

本小节介绍OCP网卡告警trap如下表：

| 告警类型ID/告警码                  | 告警Trap OID                       | 告警描述                                            |
| ---------------------------------- | ---------------------------------- | --------------------------------------------------- |
| 17    | 1.3.6.1.4.1.3902.2601.15.1.500.2.151.17  | OCP网口链路断开 |
| 8388625    | 1.3.6.1.4.1.3902.2601.15.1.500.2.151.8388625  | OCP网口链路连接 |

## 5.23 主板告警trap

本小节介绍主板告警trap如下表：

| 告警类型ID/告警码                  | 告警Trap OID                       | 告警描述                                            |
| ---------------------------------- | ---------------------------------- | --------------------------------------------------- |
| 65799    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.65799  | 温度高于轻微告警阈值 |
| 65801    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.65801  | 温度高于严重告警阈值 |
| 65803    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.65803  | 温度高于紧急告警阈值 |
| 66048    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.66048  | 电压低于轻微告警阈值 |
| 66050    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.66050  | 电压低于严重告警阈值 |
| 66052    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.66052  | 电压低于紧急告警阈值 |
| 66055    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.66055  | 电压高于轻微告警阈值 |
| 66057    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.66057  | 电压高于严重告警阈值 |
| 66059    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.66059  | 电压高于紧急告警阈值 |
| 8454407    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.8454407  | 温度高于轻微告警阈值恢复 |
| 8454409    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.8454409  | 温度高于严重告警阈值恢复 |
| 8454411    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.8454411  | 温度高于紧急告警阈值恢复 |
| 8454656    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.8454656  | 电压低于轻微告警阈值恢复 |
| 8454658    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.8454658  | 电压低于严重告警阈值恢复 |
| 8454660    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.8454660  | 电压低于紧急告警阈值恢复 |
| 8454663    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.8454663  | 电压高于轻微告警阈值恢复 |
| 8454665    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.8454665  | 电压高于严重告警阈值恢复 |
| 8454667    | 1.3.6.1.4.1.3902.2601.15.1.500.2.160.8454667  | 电压高于紧急告警阈值恢复 |


## 5.24 GPU基板告警trap

本小节介绍GPU基板告警trap如下表：

| 告警类型ID/告警码 | 告警Trap OID                                | 告警描述                          |
| ------------------| ------------------------------------------- | ----------------------------------|
| 65792             | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.65792  | GPU基板温度低于低轻微告警阈值     |
| 65794             | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.65794  | GPU基板温度低于低严重告警阈值     |
| 65796             | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.65796  | GPU基板温度低于低紧急告警阈值     |
| 65799             | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.65799  | GPU基板温度高于高轻微告警阈值     |
| 65801             | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.65801  | GPU基板温度高于高严重告警阈值     |
| 65803             | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.65803  | GPU基板温度高于高紧急告警阈值     |
| 464129            | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.464129 | GPU基板轻微故障告警               |
| 464130            | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.464130 | GPU基板严重故障告警               |
| 8454400           | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.8454400| GPU基板温度低于低轻微告警阈值恢复 |
| 8454402           | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.8454402| GPU基板温度低于低严重告警阈值恢复 |
| 8454404           | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.8454404| GPU基板温度低于低紧急告警阈值恢复 |
| 8454407           | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.8454407| GPU基板温度高于高轻微告警阈值恢复 |
| 8454409           | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.8454409| GPU基板温度高于高严重告警阈值恢复 |
| 8454411           | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.8454411| GPU基板温度高于高紧急告警阈值恢复 |
| 8852737           | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.8852737| GPU基板轻微故障告警恢复           |
| 8852738           | 1.3.6.1.4.1.3902.2601.15.1.500.2.224.8852738| GPU基板严重故障告警恢复           |

## 5.25 加速卡告警trap

本小节介绍加速卡告警trap如下表：

| 告警类型ID/告警码 | 告警Trap OID                                | 告警描述                          |
| ------------------| ------------------------------------------- | ----------------------------------|
| 65792             | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.65792  | 加速卡温度低于低轻微告警阈值      |
| 65794             | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.65794  | 加速卡温度低于低严重告警阈值      |
| 65796             | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.65796  | 加速卡温度低于低紧急告警阈值      |
| 65799             | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.65799  | 加速卡温度高于高轻微告警阈值      |
| 65801             | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.65801  | 加速卡温度高于高严重告警阈值      |
| 65803             | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.65803  | 加速卡温度高于高紧急告警阈值      |
| 8454400           | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.8454400| 加速卡温度低于低轻微告警阈值恢复  |
| 8454402           | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.8454402| 加速卡温度低于低严重告警阈值恢复  |
| 8454404           | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.8454404| 加速卡温度低于低紧急告警阈值恢复  |
| 8454407           | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.8454407| 加速卡温度高于高轻微告警阈值恢复  |
| 8454409           | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.8454409| 加速卡温度高于高严重告警阈值恢复  |
| 8454411           | 1.3.6.1.4.1.3902.2601.15.1.500.2.225.8454411| 加速卡温度高于高紧急告警阈值恢复  |

## 5.26 GPU基板光模块告警trap

本小节介绍GPU基板光模块告警trap如下表：

| 告警类型ID/告警码 | 告警Trap OID                                | 告警描述                                 |
| ------------------| ------------------------------------------- | -----------------------------------------|
| 65792             | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.65792  | GPU基板光模块温度低于低轻微告警阈值      |
| 65794             | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.65794  | GPU基板光模块温度低于低严重告警阈值      |
| 65796             | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.65796  | GPU基板光模块温度低于低紧急告警阈值      |
| 65799             | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.65799  | GPU基板光模块温度高于高轻微告警阈值      |
| 65801             | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.65801  | GPU基板光模块温度高于高严重告警阈值      |
| 65803             | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.65803  | GPU基板光模块温度高于高紧急告警阈值      |
| 8454400           | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.8454400| GPU基板光模块温度低于低轻微告警阈值恢复  |
| 8454402           | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.8454402| GPU基板光模块温度低于低严重告警阈值恢复  |
| 8454404           | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.8454404| GPU基板光模块温度低于低紧急告警阈值恢复  |
| 8454407           | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.8454407| GPU基板光模块温度高于高轻微告警阈值恢复  |
| 8454409           | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.8454409| GPU基板光模块温度高于高严重告警阈值恢复  |
| 8454411           | 1.3.6.1.4.1.3902.2601.15.1.500.2.226.8454411| GPU基板光模块温度高于高紧急告警阈值恢复  |

## 5.27 环境湿度告警trap

本小节介绍环境湿度告警trap如下表：

| 告警类型ID/告警码 | 告警Trap OID                                 | 告警描述                       |
| ----------------- | -------------------------------------------- | ------------------------------ |
| 65792             | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.65792   | 环境湿度低于低轻微告警阈值     |
| 65794             | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.65794   | 环境湿度低于低严重告警阈值     |
| 65796             | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.65796   | 环境湿度低于低紧急告警阈值     |
| 65799             | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.65799   | 环境湿度高于高轻微告警阈值     |
| 65801             | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.65801   | 环境湿度高于高严重告警阈值     |
| 65803             | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.65803   | 环境湿度高于高紧急告警阈值     |
| 464898            | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.464898  | 环境过湿严重故障告警           |
| 464899            | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.464899  | 环境过湿紧急故障告警           |
| 8454400           | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.8454400 | 环境湿度低于低轻微告警阈值恢复 |
| 8454402           | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.8454402 | 环境湿度低于低严重告警阈值恢复 |
| 8454404           | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.8454404 | 环境湿度低于低紧急告警阈值恢复 |
| 8454407           | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.8454407 | 环境湿度高于高轻微告警阈值恢复 |
| 8454409           | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.8454409 | 环境湿度高于高严重告警阈值恢复 |
| 8454411           | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.8454411 | 环境湿度高于高紧急告警阈值恢复 |
| 8853506           | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.8853506 | 环境过湿严重故障告警恢复       |
| 8853507           | 1.3.6.1.4.1.3902.2601.15.1.500.2.152.8853507 | 环境过湿紧急故障告警恢复       |

## 5.28 交换板温度告警trap

本小节介绍交换板温度告警trap如下表：

| 告警类型ID/告警码 | 告警Trap OID                                 | 告警描述                       |
| ----------------- | -------------------------------------------- | ------------------------------ |
| 65792             | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.65792   | 交换板温度低于低轻微告警阈值     |
| 65794             | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.65794   | 交换板温度低于低严重告警阈值     |
| 65796             | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.65796   | 交换板温度低于低紧急告警阈值     |
| 65799             | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.65799   | 交换板温度高于高轻微告警阈值     |
| 65801             | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.65801   | 交换板温度高于高严重告警阈值     |
| 65803             | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.65803   | 交换板温度高于高紧急告警阈值     |
| 8454400           | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.8454400 | 交换板温度低于低轻微告警阈值恢复 |
| 8454402           | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.8454402 | 交换板温度低于低严重告警阈值恢复 |
| 8454404           | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.8454404 | 交换板温度低于低紧急告警阈值恢复 |
| 8454407           | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.8454407 | 交换板温度高于高轻微告警阈值恢复 |
| 8454409           | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.8454409 | 交换板温度高于高严重告警阈值恢复 |
| 8454411           | 1.3.6.1.4.1.3902.2601.15.1.500.2.16.8454411 | 交换板温度高于高紧急告警阈值恢复 |

## 5.29 CDU告警trap
本小节介绍CDU告警trap如下表：

| 告警类型ID/告警码 | 告警Trap OID                                | 告警描述                       |
| ----------------- | --------------------------------------------| ------------------------------ |
| 464129            | 1.3.6.1.4.1.3902.2601.15.1.500.2.228.464129 | CDU轻微故障告警                |
| 464130            | 1.3.6.1.4.1.3902.2601.15.1.500.2.228.464130 | CDU严重故障告警                |
| 199169            | 1.3.6.1.4.1.3902.2601.15.1.500.2.228.199169 | 液冷系统故障告警               |
| 8852737           | 1.3.6.1.4.1.3902.2601.15.1.500.2.228.8852737| CDU轻微故障告警恢复            |
| 8852738           | 1.3.6.1.4.1.3902.2601.15.1.500.2.228.8852738| CDU严重故障告警恢复            |
| 8587777           | 1.3.6.1.4.1.3902.2601.15.1.500.2.228.8587777| 液冷系统故障告警恢复           |

## 5.30 Trap测试

本小节介绍Trap测试如下表：

| 告警类型ID/告警码           | 告警Trap OID                    | 告警描述                                                |
| ---------------------------------- | ---------------------------------- | --------------------------------------------------- |
| 1    | 1.3.6.1.4.1.3902.2601.15.1.500.2.254.1  | trap测试 |



